;INIT ALL SWITCHES FOR CF TO 0.

.DEFINE FOOLIST[] [ XLIST ]

!-.INSERT-'SWINIT.SLO'-! = 0  ;ERROR MESSAGE FOR LOSERS

F2SW = 1	; SET F2SW = 1 FOR F2,  F2SW = 0 FOR F3

FAST = 1	;IF 0, ALL CYCLES ARE 500NS OR MORE.

SLOW1 = 1	;MAKES 350NS CYCLES LONGER BY 50*SLOW1 NS. DWP 2/10

SLOW2 = 0	;MAKES 400NS CYCLES LONGER BY 50*SLOW2 NS.

TYMNET = 0

DR11P = 0

TLXTAPE = 0

125TAPE = 0

SLOWTAPE = 0

KNYTAPE = 0

NTP = 0		;NEW TAPE CTRL (DMA TYPE)

TAPE = 0	;New tape ctrl with long records.

75IPS = 0	;Not 75IPS drive -- implies 125IPS

DLS = 0

IMP = 0
IMP1 = 0	;HIGH U-MEM VERSION OF IMP

WK = 0		;Walt's Kluge

VID = 0		;FooVision
VIC2 = 0	;Smart video controler (with sysnthsis)

LPT = 0		;Lineprinter (Printronix, etc.)

VC = 0		;Versatec/Varian plotter interface.

NEWMAP = 1	;SET FOR MACHINES F3-3 AND LATER.

CROCK = 1	;set to 1 to get some old crockish code back

DEBUGSW = 0	;Set to 1 to get some debugging crocks

TIMER = 0	;INTERVAL TIMER

STANSW = 0	;Special Stanford I/O devices

WAITS = 0	;BBN Pager was modified for WAITS

XUCODE = 0	;Set to 1 (exactly !) if 8k u-memory present.
