;Symbolics F2 with 8K micro-memory

;Initialize switch settings
.INSERT SWINIT.SLO

; F2 VERSION OF MICROCODE

; SET F2SW = 1 FOR F2,  F2SW = 0 FOR F3

F2SW = 1

XUCODE = 1	;8K u-mem present

NEWMAP = 1

TIMER = 1

DR11P = 1	;DR11 interface with packet-oriented microcode

;;;IMP = 1

DLSDEV = 20	; udevice code for TTY scanner

DLS = 1

DLSDEB = 1

DLS2 = 1

NTP = 1

TAPE = 1	; New tape code
75IPS = 1 ;75 IPS TAPE SPEED -- USED FOR READING OLD CCRMA TAPES.

VID = 0		; FooVision video turned off 3/31/81 Moon
VIC2 = 0	; No smart video control (with synthesis)
DPYDEV = 36
DPYDEV2 = 2

;;VC = 1		; Set to 1 for Versatec
VCDEV = 14	; udevice code for Versatec

;-----------------------------------------------------------------------
;Default DLS configuration.  Lines are reset to this on initialization.
;See DLS definition page for meaning of this bits.

;Caution:  Only lower 6 bits are permissible here.  This means you
;	   can't start out with looped, in break mode, or with character
;	   length other than 8.  You must use macro code to set those.
;
;-----------------------------------------------------------------------
;The following comments are bogus -- Moon
;
;Three groups of
;lines may be initialized, allowing for local terminal, 300 buad modems
;and split speed modems.
;Note:  Groups can be omitted by setting DLSGRPxN to zero.
;-----------------------------------------------------------------------
.DEFINE DLSINI [] [
DLSGRP[0 13 247 34]	;Lines 0-13 9600 baud
DLSGRP[14 DLSNLINES 247 33]	;Lines 14-LAST 1200
] ;DLSINI

.DEFINE DLIST [] [LIST]	;Define as LIST to enable FOOLIST
.DEFINE DXLIST [] [XLIST]	;Define as XLIST for FOOLIST stuff

XLIST

.INSERT CFDEF.SLO

LIST

.INSERT CFNEW

LIST-LABELS
LIST-CORMAP
