II. Load the absolute binary tape produced in Step 1 above
   using the Basic Binary Loader

III. COnfigure the program to the I/O and memory configuration
   of the system on which the program is to be run:

A. Load address 2B

B. Enter tape reader I/O slot number in Switch
   Register switches 0-5, and press "RUN".
C.  Enter tape punch I/O slot number in Switch
     Register switches 0-5; press "RUN"
D.  Enter last word available memory in Switch Registers;
    press "RUN".

    e.g.:

        7677B for 4K
       17677B for 8K
          Etc.

IV. Place tape to be copied or compared in tape reader and make reader ready.

V. Check for adaquate tape supply in punch IF a copy is desired
VI. Set Switch Register for desired operation:

A. SW0 "off" - read master tape into memory and
               punch a copy (if enables by SW14)

B.  SW14
