LOW MEM. ADDRESS TEST

PROGRAM OCCUPIES 0100-0143

1. S.A. = 100
2. SET LOWER LIMIT IN SW. REG (144)
3. PRESET, RUN  HALT 102001
4. SET UPPER LIMIT TO BE TESTED IN SW. REG
    (8K=017677  16K=037677)
5. RUN

TO CHANGE UPPER OR LOWER LIMITS FOLLOW
PROCEDURE USED FOR HIGH MEM ADDR TEST

