1                                                                   1
-
              INSTALLATION INSTRUCTIONS FOR NEW INSTALLATIONS
+             ____________ ____________ ___ ___ _____________
0                               April 1979
-    1.   DASDI a disk pack and restore the  tape(s)  provided  using
          TSS  DASDI  and  DUMPRESTORE.  The D4.2 general notes (item
          10047) contain instructions on the use of  these  programs.
          The  version  of  DASDI and DUMPRESTORE on the restore tape
          supports 3330s (and 7330s).  This pack  should  be  labeled
          xxxx01  where xxxx is any 4 characters (normally MTS0), and
+                       ____
          will be the "system residence pack" for MTS.
-    2.   The pack prepared in step 1 will have about 6,200 pages  of
          available  disk space if it is a 3330-1, about 30,000 pages
          if it is a 3330-11.  If you will  require  more  than  this
          initially,  you should DASDI any other packs desired.  Each
          should have a label of the form xxxxnn where  xxxx  is  the
+                                                       ____
          same  as  above and nn goes from 2 on up sequentially.  The
+                             __
          public volume number of each pack should also be nn.
+                                                          __
-    3.   Run DECKGEN to prepare a set of TABLES  for  your  machine.
          To  load  DECKGEN,  IPL  from  the pack prepared in step 1.
          This will probably put the machine in  wait  state  (unless
          you have a 3066, 3270, or 1052-compatable device at address
          740).   To get IPLREADER to talk to you, press "request" on
          a 1052 or "enter"  on  a  3066  or  3270  (i.e.,  cause  an
          attention  interrupt).  When it asks if you want to run the
          current system, reply "NO" and enter the commands:
0              LOAD NAME=*IPL.DECKGEN
               START
0         See the DECKGEN writeup (item 10055) for information on how
          to proceed from here.  Since  DECKGEN  was  loaded  by  the
          IPLREADER  (instead  of  from  tape)  and therefore is told
          where the console is,  it  is  not  necessary  to  give  an
          attention interrupt on the console to wake it up.
-    4.   You  are  now  ready to load MTS itself.  IPL from the pack
          prepared in step 1, and again reply NO when  asked  if  you
          want the current system.  This time enter the commands:
0              LOAD NAME=*IPL.D4.2
               REPLACE TABLES FROM xxx
               (Reply to the prompt for a printer address for a map)
               START
0         where  xxx  is  the address of the tape written by DECKGEN.
+                ___
          D4.2 MTS should now be running.
1                                                                   2
-
     5.   Proceed with the start-up procedures described in  the  MTS
          operators' manual (item 10057).  Some additional points not
          mentioned in the operators' manual are:
0         A.   The  prompt for the time and date will only occur only
               if the TOD clock is not set.  Entering  the  time  and
               date as
0                      2 41 pm 5 23 78 EDT
0              would  set the time and date to 14:41 Eastern Daylight
               Time on 23 May 1978.
0         B.   MTS keeps GMT in the TOD clock.  Although this  agrees
               with  the  standard  set by IBM for the use of the TOD
               clock, very few IBM systems do this.  This means  that
               even if the clock is set, it probably will be off by a
               few hours if an IBM system was the last system used on
               the machine.
-    6.   Prepare a correct IPL system containing the TABLES for your
          machine by signing on from some terminal and entering:
0              SIG MTS
               password (see below)
               RUN RAMROD
               CREATE xxxxx FROM D4.2SYS
               enter comments if desired
               REPLACE TABLES.DUMMY FROM >Tyyy
               enter comments if desired
               enter null line or date when prompted for version
               reply "OK" to confirmation request
               DELETE SEG0.NCA.TABLES
               reply "OK" to confirmation request
               DELETE SEG1.NCA.TABLES
               reply "OK" to confirmation request
               RENAME TABLES.DUMMY TABLES
               reply "OK" to confirmation request
               CURRENT
               reply "OK" to confirmation request
0         The  passwords  for  most of the userids on the distributed
          test pack are the same as the userids, e.g.,  the  password
          for  MTS  is MTS.  The only userids for which the passwords
          are different are the terminal benchmark ids  (BMnn)  since
          the  passwords  for these are irrelevant.  The xxxxx on the
+                                                        _____
          CREATE command is a name for the new system, which normally
          would be the MTS "model number" for the date,  e.g.,  UG157
          for  August  15,  1977.  Tyyy is the name of the tape drive
+               __     __      _   ____
          containing the tape written by DECKGEN.  The next time  you
          IPL  you  can reply "YES" (or enter a null line) when asked
          if you want to run the  current  system.   See  the  RAMROD
          (item  10038)  and IPLREADER (item 10037) writeups for more
          information.
1                                                                   3
-
     7.   You now have a working version of  MTS  (presumably).   You
          can  start  to  run user programs after you've created some
          user  ids.   To  do  this,  see  the  description  of   the
          accounting  maintenance  procedures  (104/110),  which  you
          should obtain from the *FS tapes.
0         There are several things that you will probably want to  do
          to  clean  up  a  few loose ends before going much further.
          Some of these are:
0         A.   Fix HASP for whatever local options you  desire.   See
               the  description  of  these options (item 10059).  You
               may also want  to  change  some  of  the  commands  in
               STRT:HSP, the command file for *HSP, which can be used
               by the operators to start up HASP after an IPL.
0         B.   You will want to also change the contents of STRT:LAS,
               the  command  file  for *LAS, which can be used by the
               operators to start up the terminal lines.
0         C.   Fix TSFO to agree with whatever hardware is available.
               There are several assembly parameters described in the
               source.
0         D.   Fix  up  the   command   statistics   directory   file
               SYS:CMDDIR for the appropriate tapes.  If you don't do
               this,  the  system will occasionally mount a tape with
               rack number CMDTP (which must be  labeled  CMD001)  to
               dump  the  command  statistics  data.  Eventually this
               tape will fill up with command statistics data and the
               system  will  get  mad  unless  you  have   fixed   up
               SYS:CMDDIR  to  give  it more tapes to use.  A writeup
               describing the structure of  this  file  is  available
               (531/31) on the *FS tapes.
-    8.   General things new installations should know.
0         A.   How to sign on using the operators console:
0              1. Enter "MTS OPER" on the operators' console
               2. It will come back immediately for input.
               3. Enter the signon command.
               4. You  are  now  signed  on  if  the  ID  exists.  No
                  password is  required  for  signon  from  OPER  and
                  SIGFILEs are not active for signon from OPER.  Also
                  the  "last  signon"  message and the "signed on at"
                  message are not printed if MSOURCE is OPER.
0         B.   A 2301 drum must have device name DRM1.  If you have a
               second 2301, it must be named DRM2.  Similarly,  2305s
               must  be named FHF0 to FHF7 for the first one, FHF8 to
               FHFF for the second one, FHFG to FHFN for  the  third,
               etc.
0         C.   A  "privileged"  ID is one with X'80' on in the second
1                                                                   4
-
               byte  (byte  1)  of  the  accounting  record  (set  by
               accounting maintenance program on request).  If the ID
               is  privileged  then  no  checking  for maximum money,
               etc., is made.  The expiration date and  maximum  file
               space, however, are checked.  Also this bit allows the
+                              ___
               user  to  declare  a  program to be run with PROT=OFF,
               allows "public file privilege" (see next), and  allows
               privileged SYSTEMSTATUS commands to be given.
0         D.   A  "public file privileged" ID is one with X'08' on in
               the second byte of the accounting record.  This allows
               the user to create a public file.
0         E.   A user with the  ACCPUSE  bit  on  in  his  accounting
               record  can  also  declare  a  program  to be run with
               PROT=OFF  and  can   issue   privileged   SYSTEMSTATUS
               commands.
0         F.   A  user  with  either  ACCTLB  or  ACCPLB  on  in  his
               accounting record can set LSS (Limited-Service  State)
               off even if the load is too high.
