1                                                                   1
-
              INSTALLATION INSTRUCTIONS FOR NEW INSTALLATIONS
+             ____________ ____________ ___ ___ _____________
0                          MTS Distribution 5.1
0                               August 1983
-    1.   Run DECKGEN to prepare a set of TABLES  for  your  machine.
          To load DECKGEN, IPL from the Dump/Restore tape.  This will
          probably put the machine into wait state (unless you have a
          3066,  3270, or 1052-compatable device at address 3A8).  To
          get the IPLREADER to talk to you, press "request" on a 1052
          or "enter" on a 3066 or  3270  (i.e.,  cause  an  attention
          interrupt).   When  it  asks if you want to run the current
          system, reply "NO" and enter the commands:
0              LOAD NAME=*IPL.DECKGEN ADDR=xxx
               START
0         where xxx is the device address of a tape  drive  on  which
+               ___
          the MTS Utility tape is mounted.  See component 1021/12 for
          more information about the IPLREADER.
0         See  the  DECKGEN  writeup (comp. 004/8) for information on
          how to proceed from here.  Since DECKGEN was loaded by  the
          IPLREADER and therefore is told where the console is, it is
          not necessary to give an attention interrupt on the console
          to  wake  it  up.   It is a good idea to run DECKGEN from a
          hardcopy terminal if this is possible.  If not, you  should
          take  notes  as  you go along because you may need to rerun
          DECKGEN if you make a mistake and you can save some time if
          you keep a record of what you've done.  You should  include
          at  least  one public volume, MTS001, in these tables.  The
          tables you produce should be written to  tape  for  use  in
          steps  2  and  15  below.  There is no need to include your
          entire configuration in these tables if you intend  to  use
          the  tables  macros  to produce tables for your system (see
          section 17F below).
-    2.   You  are  now  ready  to  load  MTS  itself.   Rewind   the
          Dump/Restore  tape  and  IPL  from it again.  Reply NO when
          asked if you want the current system.  This time enter  the
          commands:
0              LOAD  NAME=*IPL.NDSKSYS  ADDR=xxx
               REPLACE  TABLES  FROM  yyy
               (Reply to the prompt for a printer address for a map
               or press the cancel key (on a 3066, 3215 or 1052) or
               PA2 (on a 3270) if you don't want a map).
               START
0         where xxx is the address of the MTS Utility tape and yyy is
+               ___                                            ___
          the  address of the tape written by DECKGEN in step 1.  The
          no disk version of MTS should now be running.
1                                                                   2
-
     3.   Proceed with the start-up procedures described in  the  MTS
          operators'  manual (comp. 592).  Some additional points not
          mentioned in the operators' manual are:
0         A.   The prompt for the time and date will  occur  only  if
               the  TOD  clock is not set.  For example, entering the
               time and date as
0                      2 41 pm 5 23 81 EDT
0              will set the time and date to 14:41  Eastern  Daylight
               Time  on  23 May 1981.  The timezone need not be given
               if you gave the correct timezone when you ran DECKGEN,
               i.e., MTS will use that one by default.
0         B.   MTS keeps GMT in the TOD clock.  Although this  agrees
               with  the  standard  set by IBM for the use of the TOD
               clock, some IBM systems do not do  this.   This  means
               that even if the clock has been set by another system,
               it  may  be  off by several hours and you will want to
               reply "NO" when asked if the time is correct.  You can
               then enter the correct local time, which MTS will  use
+                                     _____
               to load the TOD clock with GMT.
-    4.   At  this  point  you  will be told that MTS001 (or whatever
          name(s) you told DECKGEN to use) couldn't be  found  (which
          is  reasonable  since  we  haven't restored it yet) and you
          should respond by entering CANCEL.  This will result  in  a
          fairly  serious  looking  message about an error in catalog
          initilization which can be ignored.  If you are using a set
          of assembled  TABLES  rather  than  TABLES  produced  using
          DECKGEN,  the  message  you  see  at  this  point  will  be
          different, but the effect is the same.
-    5.   Start the job status master job by typing
0              JOBS  MAS
0         at the operator's console.
-    6.   The following steps can be done from the operator's console
          or from a 1052, 3066, 3036, 3277, 3278  or  3279  terminal.
          If you are going to work from the operator's console you'll
          need to start an MTS job by typing
0              MTS  NDSK  OPER
0         at  the  console.  If you are going to work from a terminal
          you'll need to start an MTS job on that terminal by typing
0              MTS  NDSK  xxxx
0         at the operator's console, where xxxx  is  the  MTS  device
+                                          ____
1                                                                   3
-
          name  of the terminal to be used.  The NDSK parameter tells
          MTS to avoid using the file system.
-    7.   Next, signon by entering
0              SIGNON  ccid
               ccid     (the password)
0         where ccid is  any  four  character  string.   If  you  are
+               ____
          working  at  the  operator's  console you won't be asked to
          enter a password.  If you are working from a  terminal  you
          will need to enter a password and because you are using the
          no  disk  system  the password will be the same as the ccid
          used on the signon command (remember that MTS ccids shorter
          than four characters are  padded  on  the  right  with  the
          string  ".$."   and  that  the  pad  characters  need to be
          included in the PW).
-    8.   Next attach the MTS Utility tape to your job by entering
0              $SET  PROT=OFF
               $GET  >Txxx
               $CONTROL  *AFD*  VOLUME=MTSUTL
0         where Txxx is the MTS device name of the tape  drive  where
+               ____
          the MTS Utility tape is mounted.
-    9.   If  you  have  2305s  or  4305s to use for paging, you must
          format them by entering
0              $CONTROL  *AFD*  POSN=FMT2305
               $RUN  *AFD*
               FFnn
               FFnn
                .
                .
                .
               $ENDFILE
-    10.  If you are going to  use  an  obsolete  2301s  for  paging,
          format them by entering
0              $CONTROL  *AFD*  POSN=DRUMINIT
               $RUN  *AFD*
-    11.  If  you have 2305s, 3805s, 3825s, 4305s or 2301s to use for
          paging, start the paging device processor by typing
0              PDP
0         at the operator's console.
1                                                                   4
-
     12.  Next DASDI a paging disk and at least one public volume  by
          entering
0              $CONTROL  *AFD*  POSN=DASDI
               $RUN  *AFD*
               Dxxx PAG001 VX PAGING
               Dyyy MTS001 VX 1 IPL
               .  .  .
               $ENDFILE
0         where  Dxxx  is the name of the device where the new paging
+                ____
          pack is mounted and Dyyy is the name of  the  device  where
+                             ____
          the  new file system volume(s) is mounted.  See the General
          Notes (comp. 461/19) for instructions on using FILE:DASDI.
-    13.  If you started the PDP in step 11, add the paging  disk  by
          typing
0              PGET  Dxxx
0         at  the  operator's  console.   If you didn't start the PDP
          before, start it now by typing
0              PDP
0         at the console.
-    14.  Use  DISKCOPY  to  restore  the  D5.1   system   from   the
          distributed  dump/restore  tape(s).  You should specify the
          IPL option, but SLOW and SWAP aren't  necessary.   See  the
          General Notes for information on running DISKCOPY.
0              $CONTROL  *AFD*  POSN=DISKCOPY
               $RUN *AFD*
               TAPE
               >Tnnn
               DISK
               Dyyy MTS001
               IPL
               $ENDFILE
0         where >Tnnn is the name of the MTS device on which the D5.1
+                ____
          dump/restore  tape  is  mounted  and Dyyy is the MTS device
+                                              ____
          name of the disk drive to which the data will be restored.
-    15.  Stop your machine, and IPL from the new disk.  Again  reply
          NO  when  asked  if  you want to run the current system and
          enter the commands:
1                                                                   5
-
               LOAD NAME=*IPL.D5.1SYS
               REPLACE TABLES FROM xxx
               (Reply to the prompt for a printer address for a map)
               START
0         where xxx is the address of the tape written by DECKGEN  in
+               ___
          step 1.  The D5.1 version of MTS should now be running.
-    16.  Proceed  with  the start-up procedures described in the MTS
          Operators' Manual (comp. 592).  This time you shouldn't  be
          told that MTS001 couldn't be found.
0         After initilization is complete you should do the following
          from the operator's console or a terminal
0              SIGNON  MTS
               password     (see below)
               $RUN  RAMROD
               CREATE  xxxxx  FROM  D5.1SYS
               enter comments if desired
               REPLACE  TABLES.DUMMY  FROM  >Tyyy
               enter comments if desired
               enter null line or date when prompted for version
               reply "OK" to confirmation request
               DELETE  SEG0.NCA.TABLES
               reply "OK" to confirmation request
               DELETE  SEG1.NCA.TABLES
               reply "OK" to confirmation request
               RENAME  TABLES.DUMMY TABLES
               reply "OK" to confirmation request
               CURRENT
               reply "OK" to confirmation request
0         The  passwords  for  most of the userids on the distributed
          test pack are the same as the userids, e.g.,  the  password
          for  MTS  is MTS (unlike the NDSKSYS passwords the ccid pad
          characters are not part of the password,  so  the  password
          for  MTS  is  just  MTS).   The  only userids for which the
          passwords are different  are  the  terminal  benchmark  IDs
          (Bnnn) since the passwords for these are irrelevant.  (Note
          that  a  password  is  not  required  if  you are using the
          operator's console as your  terminal.)  The  xxxxx  on  the
+                                                      _____
          CREATE command is a name for the new system, which normally
          would  be  the MTS "model number" for the date, e.g., UG153
          for August 15, 1983.  Tyyy is the MTS device  name  of  the
+              __    __     _   ____
          tape drive containing the tape written by DECKGEN.
0         This  procedure  will  cause  the  "current" system on your
          MTS001 pack to correspond to your machine configuration  so
          that  the next time you IPL you can reply "YES" (or enter a
          null line) when asked  if  you  want  to  run  the  current
          system.   See  the  RAMROD  (comp. 1019/16)  and  IPLREADER
          (comp. 1021/12) writeups for more information.
1                                                                   6
-
     17.  You now have a working D5.1 version  of  MTS  (presumably).
          You  can  start  to  run user programs after you've created
          some user IDs.  To do this,  see  the  description  of  the
          accounting  maintenance procedures (104/137) and (104/138),
          which you should obtain from the *FS tapes.
0         There are several things that you will probably want to  do
          to  clean  up  a  few loose ends before going much further.
          Some of these are:
0         A.   Fix HASP for whatever local options you  desire.   See
               the description of these options (comp.  387/26).  You
               may  also  want  to  change  some  of  the commands in
               STRT:HSP, the command file for *HSP, which can be used
               by the operators to issue the appropriate HASP  $START
               commands after starting HASP.
0         B.   You will also want to change the contents of STRT:LAS,
               the  command  file  for *LAS, which can be used by the
               operators to start up the terminal lines.
0         C.   Fix TSFO (the 2703/1270 MTS Device Support Routine) to
               agree with whatever hardware is available.  There  are
               several assembly parameters described in the source.
0         D.   Fix   up   the   command   statistics  directory  file
               SYS:CMDDIR for the appropriate tapes.  If you don't do
               this, the system will occasionally mount a  tape  with
               rack  number  CMDTP  (which must be labeled CMD001) to
               dump the command  statistics  data.   Eventually  this
               tape will fill up with command statistics data and the
               system   will   get  mad  unless  you  have  fixed  up
               SYS:CMDDIR  to  give  it  more  tapes   to   use.    A
               description of the structure of this file is available
               in the Operators' Manual on the *FS tapes (comp. 592).
0         E.   Write  new  versions  of  the  IPLBOOT  and  IPLREADER
               programs to the system pack with  the  correct  device
               address  for  your  system  console (see the IPLREADER
               description, comp. 1021/12).
0         F.   In the tables produced by DECKGEN  none  of  the  file
               system  disks  are flagged as being under disk manager
               control.   You  can  place  them  under  disk  manager
               control  using  the DMGRSTAT job program or the *-file
               job *DSK.  This will need to be done  after  each  IPL
               until  you  code  and assemble a version of tables for
               your configuration use the tables macros.
0              G.  Install ASMH.  Once you have  a  signed  and  paid
     license  agreement  with  IBM  for ASMH contact UM for a starter
     version of ASMH (ASMH is an IBM program product and as a  result
     cannot be included on the standard MTS distribution tapes).
1                                                                   7
-
          18.  General things new installations should know.
-              A.
               How to sign on using the operator's console:
0              1. Enter "MTS OPER" on the operator's console
               2. It will come back immediately for input.
               3. Enter the signon command.
               4. You  are  now  signed  on  if  the  ID  exists.  No
               password is required for signon from OPER for  "staff"
               IDs  and  SIGFILEs  are not processed.  Also the "last
               signon" message and the "signed on at" message are not
               printed.
0         B.   An obsolete 2301 drum must have device name DRM1.   If
               you  have  a  second  2301,  it  must  be  named DRM2.
               Similarly, 2305s must be named FF00 to  FF07  for  the
               first  one,  FF08  to FF0F for the second one, FF10 to
               FF17 for the third, etc.  3805s and  3825s  should  be
               named FB00, FB08, FB10, ....
0         C.   A  "privileged"  ID is one with X'80' on in the second
               byte  (byte  1)  of  the  accounting  record  (set  by
               accounting maintenance program on request).  If the ID
               is  privileged  then  no  checking  for maximum money,
               etc., is made.  The expiration date and  maximum  file
               space, however, are checked.  Also this bit allows the
+                              ___
               user   to  run  programs  with  PROT=OFF,  and  allows
               privileged SYSTEMSTATUS commands to be given.
0         D.   A "public file privileged" ID is one with X'08' on  in
               the second byte of the accounting record.  This allows
               the user to create a public file.
0         E.   A  user  with  the  ACCPUSE  bit  on in his accounting
               record can also declare  a  program  to  be  run  with
               PROT=OFF   and   can   issue  privileged  SYSTEMSTATUS
               commands.
0         F.   A  user  with  either  ACCTLB  or  ACCPLB  on  in  his
               accounting  record can set LSS (Limited-Service State)
               off even if the load is too high.
0         G.   Certain IDs are used automatically during the start-up
               sequence (INIT, SEG2, SYS., STRT).  These IDs must  be
               part  of  project WOPN on the test pack system so that
               they can signon even  if  the  "in  use"  bit  in  the
               accounting record is set.  The project number used for
               this  test in your production system may be changed by
               using a different project or project substring (or set
               of   them)   on   the   &IPLPROJ   SETC   symbol    in
               COPY:GLOBALSETS and reassembling MTS.
0         H.   MTS makes certain checks to be sure that only IDs that
               belong  to  individuals  that  work  for the computing
1                                                                   8
-
               installation   can   perform   certain    "privileged"
               operations.   This  check  is  made  by  checking  the
               project number associated with the  ID.   At  UM  only
               projects  that start with "W" are assumed to belong to
               installation staff.  This may be changed  by  altering
               the   setting   of   the   SETC   symbol  &SYSPROJ  in
               COPY:GLOBALSETS and assembling and  installing  a  new
               version of MTS.
0              I.  The distributed system contains a dummy version of
     the  rate  number subroutine (RNBR) which gives zero rates.  You
     will almost certainly  want  to  replace  this  routine  with  a
     version  that  calculates rate numbers according to the rules of
     your installation and also update the file *RATEFILE to  include
     your MTS rates.
