# PDP-8 Simulator Configuration

DEC's PDP-8, introduced in 1965, was the first mass produced minicomputer, as well as the first computer costing less than $20,000. It remained in active production until 1988; more than 50,000 units were produced. All the models in the family were based on one of the seven CPU designs (photographs courtesy of Digital Equipment Corporation):

- 1965: PDP-8
- 1966: PDP-8/S - serial logic design
- 1968: PDP-8/I - first design with integrated circuits (also PDP-8/L)
- 1970: PDP-8/E - first Omnibus design (also PDP-8/F, PDP-8/M)
- 1975: PDP-8/A
- 1979: Intersil 6100 - first LSI design (VT78)
- 1981: Harris 6120 - last design (DECmate I, DECmate II, DECmate III)

Option | Description | Capacity
CPU and memory | PDP-8/E | 4KW - 32KW
CPU options | KM8E memory extension and timeshare control |
| KE8E EAE (extended arithmetic element) |
| TSC8-75 timesharing controller for ETOS |
| FPP-8A floating point processor |
Console | KL8E and KSR-33 Teletype |
Extra terminals | KL8JA and KSR-33 Teletype | 4 terminals
Paper tape | PC8E paper tape reader and punch |
Real time clock | KW8E real time clock |
Line printer | LP8E line printer |
DECtape | TC08/TU56 DECtape | 190KW
| TD8E/TU56 DECtape | 190KW
Disk | RX8E/RX01 single density floppy disk | 256KB
| RX28/RX02 double density floppy disk | 512KB
| DF32/DS32 fixed head disk | 128KW
| RF08/RS08 fixed head disk | 1MW
| RK8E/RK05 cartridge disk | 1.6MW
| RL8A/RL01-RL02 cartridge disk | 5-10MB
Cassette tape | TA8E/TU60 cassette tape | 93KB
Magnetic tape | TM8E/TU10, 800bpi 9 track magnetic tape |

Updated 03-May-2012 by Bob Supnik (simh AT trailing-edge DOT com - anti-spam encoded)