# 8080, Z80, and 8086 Microcomputers Simulator Configuration

The Altair 8080 was quickly followed by an explosion of microcomputers and single-board computers from a variety of small companies. This simulator supports:

- MITS Altair 8800
- Vector Graphics MZ
- Imsai 8080
- North Star Horizon
- Compupro 8-16
- ADC Super-Six Single Board Computer
- N8VEM Single Board Computer

The original simulator for the Altair 8800 was developed by Charles Owen. This expanded version was developed by Peter Schorn, Howard Harte, and Ernie Price.

Photographs:

- MITS Altair 8800 (courtesy of Data General Corporation)

Option | Description | Capacity
CPU and memory | Intel 8080 or 8086 or Z80 8b microprocessor | 4KB - 1024KB
| Compupro Selector Channel |
Console | MITS 88-2SIO serial interface card, port 1 |
Paper tape reader/punch | MITS 88-2SIO serial interface card, port 2 |
Floppy disk | MITS 88-DISK, 1-8 drives | 338KB
| ADC Super-Six, 1-4 drives | 630KB
| Compupro Floppy Controller, 1-4 drives | 630KB
| Cromeco Floppy Controller, 1-4 drives | 256KB
| Imsai FIF controller, 1-8 drives | 1.11MB
| Micropolis Floppy Controller, 1-4 drives | 338KB
| North Star Floppy Controller, 1-4 drives | 358KB
| Intel i8272 Floppy Controller, 1-4 drives | 630KB
| Western Digital 179X Floppy Controller, 1-4 drives | 630KB
Hard disk | Hard disk, 1-8 units | 8.4MB
| Compupro Hard Disk Controller, 1-4 drives | 21MB
| Compupro ST-506 Disk Controller, 1-4 drives | 18MB

Updated 15-Dec-2008 by Bob Supnik (simh AT trailing-edge DOT com- anti-spam encoded)