# Honeywell H316 Simulator Configuration

The Honeywell Series 16 was initially developed by Computer Controls Corporation in the mid-60's. 3C's systems were named DDP-x16. When Honeywell bought 3C, it renamed the models to Hx16. Among the models in this series were

- DDP-516 (H516) - the original Arpanet IMP
- DDP-116
- DDP-416
- H316
- H716

Photographs:

- H316 (courtesy of Mike Umbricht)

Option | Description | Capacity
CPU and memory | H316 CPU | 8KB - 32KB
CPU options | double precision integer arithmetic |
Console | 316/516-33 KSR-33 Teletype |
Paper tape | 316/516-50 paper tape reader |
| 316/516-52 paper tape punch |
Clock | 316/516-12 real-time clock |
Line printer | Analex unbuffered shuttle line printer |
Fixed head disk | 4400 fixed head disk | 98KW - 1532KW
Moving head disk | 4623/4653/4720 disk pack controller | 831KW - 8314KW
Magnetic tape | 4100 7-track magtape controller |

Updated 30-Jan-2007 by Bob Supnik (simh AT trailing-edge DOT com - anti-spam encoded)