« Установка RSX-11M Часть II Сравнение MCR и DCL »
Установка RSX-11M Часть I
Устанавливать RSX-11M 4.6 будем с образа ленты, который можно взять здесь - rsx11m46.zip
Если в процессе установки какой то пункт не понятен, то можно найти его описание в мануале по установке - System Generation and Installation Guide (RSX-11M Version 4.2)
Итак запускаем simh, вставляем ленту:
sim> attach rsx11m46.tpc
sim> boot ts0
и приступаем к установке!
(то что нужно вводить, выделено жирным)
RSX-11M/RSX-11M-PLUS Standalone Copy System V04
RSX-11M/RSX-11M-PLUS Standalone Configuration and Disk Sizing Program
Valid switches are:
/CSR=nnnnnn to change the default device CSR
/VEC=nnn to change the default device vector
/FOR=n to change the default magtape formatter number
/DEV to list all default device CSR and vectors
Enter first device: MS0:
Enter second device: DB0:
Hit RETURN and enter date and time as 'TIM HH:MM MM/DD/YY'
>TIM 08:14 02/25/92
>RUN BAD
BAD>DB0:
BAD -- DB0: Total bad blocks= 0.
BAD>^Z
>RUN BRU
BRU>/REW/INIT/BAC:DBSYS MS0: DB0:
BRU - Starting Tape 1 on MS0:
BRU - End of Tape 1 on MS0:
BRU - Completed
BRU>
ctrl+e
Simulation stopped, PC: 001344 (CLRB (R1)+)
sim> boot rp
RSX-11M V4.6 BL56 124.K MAPPED (BASELINE)
>RED DB:=SY:
>RED DB:=LB:
>MOU DB:RSXM56
>@DB:[1,2]STARTUP
>* PLEASE ENTER TIME AND DATE (HR:MN DD-MMM-YY) [S]: 08:20 24-FEB-92
>* ENTER LINE WIDTH OF THIS TERMINAL [D D:132.]:
>SET /BUF=TI:132.
>ACS SY:/BLKS=1024.
>@
>@TAPEKIT
>;
>; RSX-11M V4.6 BL56 tape distribution kit extraction procedure.
>; Started on 12-JUL-92 at 10:26:12
>;
>INS LB:$BRU
>;
>* Enter drive and unit with tape distribution kit [ddn:] [S]: MS0:
>LOA MS:/PAR=GEN
>;
>; Copying rest of RSXM56 to DB0: ...
>;
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:RSXBAS MS0: DB0:
BRU - Starting Tape 1 on MS0:
BRU - End of Tape 1 on MS0:
BRU - Completed
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:EXCPRV MS0: DB0:
BRU - Starting Tape 1
BRU - End of Tape 1
BRU - Completed
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:PRVBLD MS0: DB0:
BRU - Starting Tape 1
BRU - End of Tape 1
BRU - Completed
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:RLUTIL MS0: DB0:
BRU - Starting Tape 1
BRU - End of Tape 1
BRU - Completed
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:MCRSRC MS0: DB0:
BRU - Starting Tape 1
BRU - End of Tape 1
BRU - Completed
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:HLPDCL MS0: DB0:
BRU - Starting Tape 1
BRU - End of Tape 1
BRU - Completed
>BRU/DENS:1600/NOINI/SUP/UFD/BAC:RMSV20 MS0: DB0:
BRU - Starting Tape 1
BRU - End of Tape 1
BRU - Completed
>;
>; Completed on 12-JUL-92 at 10:26:32
>;
>@
>
ctrl+e
Simulation stopped, PC: 002770 (CLRB (R1)+)
sim>
На данном этапе были установлены файлы с ленты на диск RP06, в следующих частях сконфигурируем(SYSGEN) и настроим систему.
комментарии # 21-02-2014 06:12, Unik

### Оставить комментарий к «Установка RSX-11M Часть I»

Имя
Текст комментария *

# ~Digital PDP-11~

## Навигация

## Страницы

О сайте

## Поиск

## Ссылки

- jaqblog
- Soft&Manual
- BASIC PDP-11
- PDP-11 Nostalgia
- PDP-11
- Ancient Bits adventure
- pdp-11.org.ru
- RetroCMP
- Soft
- Soft and other
- PDP2011
- Raspberry Pi PDP-11
- RSX11M.com
- Paper Tape
- TU-58 XXDP
***
- RSTS/E
- ELVIRA
- Wofford WITCH
- RSTS.org
- RSTS/E walkthru

gopher://pdp11.tk/

## Комментарии

Korchagin в Turtles Ninja
Гость в Доступный PDP-11. Часть 2.
Vladimir в PDP-11/45 online