« DECnet over IP Установка DATATRIEVE-11. VCP »
Установка FMS-11 v2.1
FMS-11/RSX V2.1 это система управления Ввода/Вывода основанная на использовании форм и применяющаяся в разработке приложений ввода данных. Само приложение можно разрабатывать на многих популярных языках для которых как видно ниже есть библиотеки и примеры.
Скачиваем отсюда fmsrsx_v2_1.zip и устанавливаем:
>UFD [30,10]
>SET /UIC=[30,10]
>INS $FLX
>MOU/FOR MS0:
>FLX SY:/RS=MS0:[30,10]FMSINS.CMD/DO
>@FMSINS
>;
>; FMSINS.CMD
>;
>; Copyright (C) 1985 by
>; Digital Equipment Corporation, Maynard, Mass.
>;
>; Install FMS-11/RSX
>;
>SET /MCR=TI:
>;
>;
>* Enter distribution device and unit number [S R:2-3]: MS0
>;
>;
>;
>* Is the distribution tape 1600 BPI? [Y/N]: Y
>;
>FLX SY:/RS=MS0:[30,10]*.*/DO/DNS:1600.
>FLX SY:/RS=MS0:[30,20]*.*/DO/IM/DNS:1600.
>;
>DMO MS0:
17:03:50 *** MS0: -- Dismount complete
DMO -- TT0: dismounted from MS0: *** Final dismount initiated ***
>;
>;
>PIP TI:=README.TXT
FMS-11/RSX V 2.1 07-NOV-86
Introduction
This kit contains the necessary files to install FMS-11/RSX
Version 2.1 .
Installation
DIGITAL recommends that this kit be installed in the [30,10]
directory with /NONAMED_DIRECTORY set as the default. If you
wish to install this kit in other than [30,10] and/or in
/NAMED_DIRECTORY mode, set your default to the chosen
directory, copy [30,10]FMSINS.CMD from the kit to the default
directory, and start the installation procedure (@FMSINS).
The installation is directory and device independant, however,
future updates to FMS-11/RSX 2.1 will assume a [30,10] installation.
New functionality
Two FDV keypad definitions are now available. The first is the
same keypad used for FMS-11 1.0. The second duplicates similar
functionality with the VAX FMS keypad. The standard libraries
on this kit are built with the V 1.0 keypad layout.
The differences between the two are as follows:
FMS-11 1.0 FMS-11/RSX 2.1
---------------------- --------------------------
(PF1) Insert/Overstrike (PF3) switch to overstrike
toggle switch mode
(PF1)(PF3) switch to insert
mode
(PF3) Exit Scrolled (PF1)(Uparrow) Exit scrolled
area backwards backwards
(PF4) Exit Scrolled (PF1)(Dowmarrow) Exit scrolled
area forward forwards
To build your Form Driver with the new keyboard layout use the FDVBLD.CMD
procedure.
>;
>; Build FMS Utilities and Demo Programs
>;
>;
>; FMSBLD.CMD
>;
>; Copyright (C) 1985 by
>; Digital Equipment Corporation, Maynard, MA
>;
>SET /MCR=TI:
>;
>;
>* Build FORTRAN IV UETP and demo programs ? [Y/N]: Y
INS -- File not found
>;
>; FORTRAN IV compiler (...FOR) not available.
>; FORTRAN IV demo and UETP won't be built
>;
>;
>* Build FORTRAN-77 UETP and demo programs ? [Y/N]: Y
>;
>; FORTRAN-77 OTS FILE LB:[1,1]F77FCSOTS.OLB not available.
>; FORTRAN-77 FCS versions of demo and UETP won't be built
>;
>; FORTRAN-77 OTS FILE LB:[1,1]F77RMSOTS.OLB not available.
>; FORTRAN-77 RMS versions of demo won't be built
>;
>; FORTRAN-77 demo's and UETP won't be built
>;
>;
>* Build COBOL-11 demo programs ? [Y/N]: Y
>;
>; COBOL-11 OTS FILE LB:[1,1]CBLLIB.OLB not available.
>; COBOL-11 demo's won't be built
>;
>;
>* Build COBOL-81 demo programs ? [Y/N]: Y
INS -- File not found
>;
>; COBOL-81 compiler (...C81) not available.
>; COBOL-81 demo's won't be built
>;
>;
>* Build BASIC-PLUS-II demo programs ? [Y/N]: Y
>;
>* Build DIBOL-83 demo programs ? [Y/N]: Y
>;
>* Build RMS demo's with RMSRES resident library? [Y/N]: Y
>;
>; Build the FMS utilities (FED and FUT)
>;
>TKB @FEDTKB
>TKB @FUTTKB
>;
>;
>; Build the FMS demonstration programs in FORTRAN IV, FORTRAN-77
>; COBOL-11, COBOL-81, BASIC-PLUS-II, DIBOL-83, and MACRO.
>;
>;
>; DEMBLD.CMD
>;
>; Copyright (C) 1985 Digital Equipment Corporation, Maynard, MA
>;
>; Build the demonstration programs
>;
>;
>;
>;
>;
>;
>;
>;
>; Task build BASIC-PLUS-II demo
>;
>BP2 @BASDEM
PDP-11 BASIC-PLUS-2 V2.7-00
@BASDEM
@BASDEM
OLD BASDEM.B2S
COMPILE/LIST/OBJECT
BASDEM 05:04 PM 06-Feb-;6
EXIT
>TKB @BASRMSRES
>;
>; Task name is BASRMSRES.TSK
>;
>;
>; Build DIBOL-83 demo
>;
>DIB DBLDEM,DBLDEM=DBLDEM
No errors detected
>TKB @DBLRMSRES
>;
>; Task name is DBLRMSRES.TSK
>;
>;
>; Build MACRO demo
>;
>MAC @MACDEM
MCR -- Task not in system
>TKB @MACFCSTKB
TKB -- *FATAL*-Lookup failure on file MACDEM.OBJ
>;
>; Task name is MACFCSDEM.TSK
>;
>;
>;
>; Build the UETP
>;
>;
>; UTPBLD.CMD
>;
>; Copyright (C) 1985 Digital Equipment Corporation, Maynard, MA
>;
>; Build the FMS UETP
>;
>SET /MCR=TI:
>;
>;
>;
>; Assemble MACRO version of the file initialization program
>;
>MAC INITF,INITF/CR/-SP=INITF
MCR -- Task not in system
>;
>; Task build file initialization program
>;
>TKB @INITKB
TKB -- *FATAL*-Lookup failure on file INITF.OBJ
>;
>; Assemble script modules
>;
>; Assemble FDV terminal I/O module with script hook
>; included by SCRSYM.MAC
>;
>MAC UTPTIO,UTPTIO/CR/-SP=FMSMAC/ML,SCRSYM,FDVTIO
MCR -- Task not in system
>MAC UTPFDV,UTPFDV/CR/-SP=FMSMAC/ML,SCRSYM,FDV,FDVXIO
MCR -- Task not in system
>;
>; Assemble UETP Script Processor
>;
>MAC SCRIPT,SCRIPT/CR/-SP=FMSMAC/ML,SCRIPT
MCR -- Task not in system
>;
>; Assemble MACRO version of UETP
>;
>MAC SIS,SIS/CR/-SP=FMSMAC/ML,SIS
MCR -- Task not in system
>;
>; Task build MACRO version of UETP
>;
>TKB @UTPMACTKB
TKB -- *FATAL*-Lookup failure on file SIS.OBJ
>;
>;
>;
>;
>;
>;
>; Build any desired Forms Driver resident library
>;
>;
>; FDV RESIDENT LIBRARY GERNERATOR
>;
>; The options are :
>;
>; 1) Build FDV resident library with RMS-11 support
>; 2) Build FDV resident library with FCS CODE
>; 3) Build FDV resident library with FCS support
>; 4) None (exit)
>;
>;
>* Which resident library would you like to build [O]: 1
>;
>; Build the FDVRMS resident library. Library will
>; have RMS support.
>;
>MAC @FDVRMSRES.CMD
MCR -- Task not in system
>TKB @FDVRMSTKB.CMD
TKB -- *FATAL*-Lookup failure on file FDVDRL.OBJ
>SET /UIC=[1,1]
>ASN LB:=SY:
>PIP *.*/UF/NV=DB0:[30,10]FDVRMS.TSK,.STB
PIP -- No such file(s)
DB0:[30,10]FDVRMS.TSK
PIP -- No such file(s)
DB0:[30,10].STB
>SET /UIC=[30,10]
>ASN DB0:=SY:
>REMOVE FDVRMS/REG
REM -- Common not in system
>INSTALL LB:[1,1]FDVRMS/PAR=GEN
INS -- File not found
>PIP FDVDRL.OBJ;*/DE
PIP -- No such file(s)
SY0:[30,10]FDVDRL.OBJ;*
>;
>; Applications built against the FDVRMS library should include
>; the module FDVDRT.OBJ at taskbuild time.
>;
>;
>;
>* Would you like the RMS demos built clustered with RMS? [Y/N]: Y
>;
>; Build BASIC+II demo with RMSRES and FDVRMS clustered
>;
>TKB @BASRMSCLS
TKB -- *FATAL*-Lookup failure on file FDVDRT.OBJ
>;
>; Task name is BASRMSCLS
>;
>;
>; Build Dibol-83 demo with RMSRES and FDVRMS and DBLRSX clustered
>;
>TKB @DBLRMSCLS
TKB -- *FATAL*-Lookup failure on file FDVDRT.OBJ
>;
>; Task name is DBLRMSCLS.TSK
>;
>;
>; FDV RESIDENT LIBRARY GERNERATOR
>;
>; The options are :
>;
>; 1) Build FDV resident library with RMS-11 support
>; 2) Build FDV resident library with FCS CODE
>; 3) Build FDV resident library with FCS support
>; 4) None (exit)
>;
>;
>* Which resident library would you like to build [O]: 4
>;
>;
>;
>; Installation complete
>;
>@
>
Документации по FMS-11 в интернете почти нет, поэтому не понятно как его использовать. Но можно прочитать его обзор от HP - SP1227PF.PDF.
комментарии # 06-02-2016 14:13, Unik

### Оставить комментарий к «Установка FMS-11 v2.1»

Имя
Текст комментария *

# ~Digital PDP-11~

## Навигация

## Страницы

О сайте

## Поиск

## Ссылки

- jaqblog
- Soft&Manual
- BASIC PDP-11
- PDP-11 Nostalgia
- PDP-11
- Ancient Bits adventure
- pdp-11.org.ru
- RetroCMP
- Soft
- Soft and other
- PDP2011
- Raspberry Pi PDP-11
- RSX11M.com
- Paper Tape
- TU-58 XXDP
***
- RSTS/E
- ELVIRA
- Wofford WITCH
- RSTS.org
- RSTS/E walkthru

gopher://pdp11.tk/

## Комментарии

Korchagin в Turtles Ninja
Гость в Доступный PDP-11. Часть 2.
Vladimir в PDP-11/45 online