« Настройка DECnet-11M-PLUS V4.6 Сеть в SIMH »
Установка DECnet-11M-PLUS V4.6
Устанавливать DECnet-11M-PLUS V4.6 будем с ленты, для чего понадобится диск под NETGEN. Создадим его, смонтировав пустой RL02 диск в rl0
ATTACH RL0 decnet.dsk
Дальше смотрим лог установки, где сначала подготавливаем наш чистый RL0 диск, копируем на него PREGEN.CMD и запускаем его.
sim> boot rp0
RSX-11M-PLUS V4.6 BL87 512.KW System:"PISTON"
>RED DB:=SY:
>RED DB:=LB:
>RED DB:=SP:
>MOU DB0:"RSX11MPBL87"
>@DB:[1,2]STARTUP
>; PLEASE NOTE
>;
>; If you have not yet read the system release notes, please do so
>; now before attempting to perform a SYSGEN or to utilize the new
>; features of this system.
>;
>;
Z[c
SET -- Inquire cannot determine terminal type
>;
>; Please ignore any random characters that may have printed on your
>; terminal just now. They came from a SET /INQUIRE=TI: command.
>; Evidently your terminal does not recognize escape sequences.
>; This will not affect the running of this command file.
>;
>* Please enter time and date (HH:MM DD-MMM-YYYY) [S]: 19:46 21-JAN-2016
>TIME 19:46 21-JAN-2016
>ACS SY:/BLKS=1024.
>CON ONLINE ALL
>ELI /LOG/LIM
>CLI /INIT=DCL/CTRLC/DPR="<15><12>/$ /"
>INS LB:[1,1]RMSRESAB.TSK/RON=YES/PAR=GEN
>INS LB:[1,1]RMSLBL.TSK/RON=YES/PAR=GEN
>INS LB:[1,1]RMSLBM.TSK/RON=YES/PAR=GEN
>INS $QMGCLI
>INS $QMGCLI/TASK=...PRI
>INS $QMGCLI/TASK=...SUB
>QUE /START:QMG
>INS $QMGPRT/TASK=PRT.../SLV=NO
>QUE LP0:/CR/NM
>START/ACCOUNTING
>CON ESTAT LP0:
>QUE LP0:/SP/FL:2/LOWER/FO:0
>QUE BAP0:/BATCH
>QUE LP0:/AS:PRINT
>QUE BAP0:/AS:BATCH
>INS LB:[1,1]dblrsx/par=gen
>INS $dibol83
>INS $dblmsgmgr
>INS $dblsort1
>INS $dblsort2
>INS $dblmnugen/task=mnu
>dcl run msgmgr /delay=1s
>INS $F77
>INS $PDP11C
>INS $PDPPAS
>INS LB:[1,54]B2RESQ.TSK/RON=YES/PAR=GEN
>INS $BP2IC2
>INS LB:[6,3]cobol.tsk
>INS LB:[6,3]cblmrg.tsk
>INS LB:[6,3]refrmt.tsk
>INS $K11IDM
>INS $EDT
>INS $TKB
>DFL LB:[GAMES]=SYS$GAMES/GBL/FIN
>INS SYS$GAMES:COOKIE/TASK=...COO
>@
>INS $BAD
>SET /UIC=[1,1]
>ALL DL0:
>MOU/FOR DL0:
>BAD DL0:
BAD -- DL0: Total bad blocks= 0.
>INIT DL0: NETGEN
>DMO DL0:
19:48:01 *** DL0: -- Dismount complete
DMO -- TT0: dismounted from DL0: *** Final dismount initiated ***
>DEA DL0:
>MOU DL0: NETGEN
>ALL MS0:
>MOU/FOR MS0:
>UFD DL0:[137,10]
>SET /UIC=[137,10]
>INS $BRU
>BRU /REW/NOI/UFD MS0: DL0:
BRU - Starting Tape 1 on MS0:
BRU - End of Tape 1 on MS0:
BRU - Completed
>@DL0:[137,10]PREGEN
>;
>; ======================================================================
>; PREGEN - RSX-11M/S/M-PLUS CEX System Pre-Generation Procedure
>; Started at 19:51:42 on 21-JAN-16
>; ======================================================================
>;
>; Copyright (c) 1996,1997,1998 by Mentec, Inc., U.S.A.
>; All rights reserved
>;
>* 01.00 Do you wish to see the PREGEN notes? [Y/N]: N
>;
>; Installing the following tasks:
>; FLX
>;
>* 04.00 Where is the Network distribution kit loaded [S]: MS0:
>* 04.01 Is the tape already loaded in MS0:? [Y/N]: Y
>* 04.02 Is the tape 1600 BPI? [Y/N]: Y
>DMO MS0:/LOCK=V
19:58:01 *** MS0: -- Dismount complete
DMO -- TT0: dismounted from MS0: *** Final dismount initiated ***
>* 05.00 Where is the NETGEN disk loaded [S]: DL0:
>* 05.01 Is the disk already loaded in DL0:? [Y/N]: Y
BRU - Starting Tape 1 on MS0:
BRU - End of Tape 1 on MS0:
BRU - Completed
19:58:18 *** MS0: -- Dismount complete
DMO -- TT0: dismounted from MS0: *** Final dismount initiated ***
>;
>* 03.00 Copy the DECnet distribution kit? [Y/N]: Y
>* 04.00 Where is the DECnet distribution kit loaded [S]: MS0:
>* 04.01 Is the tape already loaded in MS0:? [Y/N]: Y
>* 04.02 Is the tape 1600 BPI? [Y/N]: Y
BRU - Starting Tape 1 on MS0:
BRU - End of Tape 1 on MS0:
BRU - Completed
19:59:12 *** MS0: -- Dismount complete
DMO -- TT0: dismounted from MS0: *** Final dismount initiated ***
>;
>* 03.00 Copy the PSI distribution kit? [Y/N]: Y
>* 04.00 Where is the PSI distribution kit loaded [S]: MS0:
>* 04.01 Is the tape already loaded in MS0:? [Y/N]: Y
>* 04.02 Is the tape 1600 BPI? [Y/N]: Y
FLX -- File not found
MS0:[137,10]PSIMOV.DAT
FLX -- File not found
MS0:[137,10]PSIMOV.DAT
>;
>; Error - The file MS0:[137,10]PSIMOV.DAT could not be copied.
>;
19:59:53 *** MS0: -- Dismount complete
DMO -- TT0: dismounted from MS0: *** Final dismount initiated ***
>;
>* 03.00 Copy the PSI distribution kit? [Y/N]: N
>;
DMO -- TT0: dismounted from DL0: *** Final dismount initiated ***
>;
>; ======================================================================
>; PREGEN - Stopped at 20:00:23 on 21-JAN-16
>; ======================================================================
>;
20:00:23 *** DL0: -- Dismount complete
>@
>MOU DL0: NETGEN
>@DL0:[137,10]NETGEN
>;
>; =====================================================================
>; NET - RSX-11M-PLUS CEX System Generation Procedure
>; Started at 20:02:56 on 21-JAN-16
>; =====================================================================
>;
>; Copyright (c) 1996,1997,1998 by Mentec, Inc., U.S.A.
>; All rights reserved
>;
>; Generate a CEX System, Version 04.06, for your RSX-11M-PLUS target system.
>;
>; The following CEX Products may be generated
>; DECnet
>;
>; The distribution kits must be up to the current patch level. If
>; necessary, you should stop the generation and apply the necessary
>; patches.
>;
>; The logical device name LB: should already be assigned to the device
>; which contains the library files for the system you are generating.
>; These files are EXELIB.OLB, EXEMC.MLB, RSXMAC.SML, SYSLIB.OLB and
>; NOANSLIB.OLB for RSX-11M-PLUS and 11SLIB.OLB for RSX-11S.
>;
>; The logical device names IN:, OU:, LS: and MP: should not be assigned
>; to any devices before starting the generation. These logical device
>; names are used by NETGEN to refer to various disks used during the
>; generation.
>;
>;
>; Do you want to:
>* -Continue, E-Exit [S]:
>;
>;
>; ====================================================================
>; NETGEN Disk contains NO DECNET AUTOPATCH corrections
>; ====================================================================
>;
>; =====================================================================
>; NET - Section 1 - General Initialization
>; =====================================================================
>;
>* 01.00 Do you want to see the NETGEN notes/cautions [D=N]? [Y/N]:
>* 02.00 Target system device [dduu, D=SY:] [S]:
>* 03.00 Listing/map device [dduu, D=None] [S]:
>* 04.00 UIC Group Code for NETGEN output [O R:1-377 D:5]:
>;
>; Checking for required tasks and UICs.
>;
>;
>; Creating UFD for SY:[005,001]
>; Creating UFD for SY:[005,010]
>;
>; 07.00 User ID to be used to identify your new responses
>* [D=None] [S R:0.-30.]:
>* 08.00 Is this generation to be a dry run [D=N]? [Y/N]:
>* 09.00 Do you want a standard function network [D=N]? [Y/N]: Y
>* 11.00 Should old files be deleted [D=N]? [Y/N]: Y
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; NET - Section 2 - Define the target system
>; =====================================================================
>;
>* 02.00 RSXMC.MAC location (ddu:[g,m], D=SY:[011,010]) [S]:
>;
>; SY00:[011,010]RSXMC.MAC is being copied to SY:[005,010]RSXMC.MAC
>;
>; SY:[005,010]RSXMC.MAC is being scanned to define your target system.
>; This may take up to several minutes.
>;
>; The target is an RSX-11M-PLUS system, with...
>; A 20K-Executive
>; Kernel data space enabled
>; Extended memory support (more than 124K words of memory)
>; Multi-user protection
>; Extended instruction set (EIS)
>; Powerfail recovery support
>; Dynamic task checkpoint allocation
>; PLAS support
>; Queue Manager (QMG) support
>;
>; Creating UFD for SY:[005,024]
>; Creating UFD for SY:[005,054]
>;
>* 04.00 RSX11M.STB location (ddu:[g,m], D=SY00:[001,054]) [S]:
>;
>; SY00:[001,054]RSX11M.STB is being copied to SY:[005,054]RSX11M.STB
>;
>;
>; Checking for required library files and tasks.
>;
>* 05.00 Should tasks link to the Supervisor Mode FCS library [D=N]? [Y/N]:
>* 06.00 Should tasks link to the Memory Resident FCS library [D=N]? [Y/N]: Y
>;
>; The DECnet CEX Product will be generated.
>;
>; Routing or non-routing nodes can be generated from your distribution kit.
>;
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; NET - Section 3 - Define the system lines
>; =====================================================================
>;
>* 01.00 Device Driver Process name [=Done] [S R:0-3]: UNA
>* 02.00 How many UNA controllers are there [D R:1.-16. D:1.]:
>;
>* 03.01 CSR address for UNA-0 [O R:160000-177777 D:174510]:
>* 03.02 Vector address for UNA-0 [O R:0-774 D:120]:
>* 03.03 Device priority for UNA-0 [O R:4-6 D:5]:
>;
>* 04.07 Set the state for UNA-0 ON when loading the network [D=N]? [Y/N]: Y
>;
>* 01.00 Device Driver Process name [=Done] [S R:0-3]:
>;
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; NET - Section 4 - Define the CEX System
>; =====================================================================
>;
>; Creating build files for AUX, the CEX Auxillary routine.
>;
>; Creating build files for CETAB, the CEX configuration tables.
>;
>; Creating build files for the DDMs, the device driver modules.
>;
>; UNA
>;
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; NET - Section 5 - Define the Comm Exec Support Components
>; =====================================================================
>;
>; Creating build files for NTINIT, the network initializer.
>;
>; Creating build files for NTL, the network loader.
>;
>; Creating build files for MLD, the general microcode loader.
>;
>; Creating build files for EVL/EVC, the event logger and collector.
>;
>; EVL will use 6. event buffers.
>;
>; =====================================================================
>; NET - Section 6 - Define the System Management Utilities
>; =====================================================================
>;
>; Creating build files for NCP, the network control program.
>;
>; Creating build files for NMVACP and NMDRV, the Network Management
>; Volatile ACP and driver.
>;
>; Creating build files for CFE, the configuration file editor.
>;
>; Creating build files for NDA, the network dump analyzer.
>;
>; Creating build files for VNP, the virtual network control program.
>;
>; Creating build files for LOO, the loop test sender task.
>;
>; Creating build files for EVF, the event file interpreter program.
>;
>;
>; =====================================================================
>; NET - Section 7 - Define the CEX Products
>; =====================================================================
>;
>; Questions concerning the following CEX Products will now be asked.
>;
>; DECnet
>;
>;
>; =====================================================================
>; DEC - DECnet CEX Product Generation Procedure
>; Starting questions at 20:07:38 on 21-JAN-16
>; =====================================================================
>;
>; Copyright (c) 1996,1997,1998 by Mentec, Inc., U.S.A.
>; All rights reserved
>;
>; Generate the DECnet CEX Product for your RSX-11M-PLUS target
>; System.
>;
>; =====================================================================
>; DEC - Section 1 - Define the target and remote nodes
>; =====================================================================
>;
>* 01.00 What is the target node name [S R:0-6]: PISTON
>* 02.00 What is the target node address [S R:0.-8.]: 1.77
>* 03.00 Target node ID [D=None] [S R:0.-32.]: Simh/RSX11M+ System
>* 04.00 Do you want to generate a routing node [D=N]? [Y/N]:
>;
>; Extended network support for network command terminals and products
>; layered on DECnet, will be included.
>;
>* 07.00 Remote node name [=Done] [S R:0-6]:
>;
>; The DECnet MACRO user library and FORTRAN/COBOL/BASIC+2 library will
>; be included.
>;
>; The DECnet MACRO user library will be placed on your target disk
>; as "SY:[1,1]NETLIB.MLB".
>;
>; The DECnet FORTRAN/COBOL/BASIC+2 object library will be placed on your
>; target disk as "SY:[1,1]NETFOR.OLB".
>;
>; If necessary, please move them to the library disk (LB:) on your
>; target system, if this is different from your target disk (SY:).
>;
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; DEC - Section 2 - Define the DECnet Communications Components
>; =====================================================================
>;
>; Creating build files for XPT, the routing process.
>;
>; Creating build files for ECL, the network services process and driver.
>;
>; Creating build files for NETACP, the network services ACP.
>;
>; NETACP will be checkpointable.
>;
>; Creating build files for EPM, the Ethernet protocol manager process.
>;
>; =====================================================================
>; DEC - Section 3 - Define the DECnet Network Management Components
>; =====================================================================
>;
>; Creating build files for NICE, the network information and control
>; server task.
>;
>; Creating build files for EVR, the network event receiver task.
>;
>; Creating build files for NTD, the node state display task.
>;
>; Creating build files for NTDEMO, the node state display server task.
>;
>; Creating build files for LIN, the link watcher task.
>;
>; Creating build files for MIR, the loop test mirror task.
>;
>; Creating build files for NVP, the network connect verification task.
>;
>; Creating build files for SCP, the node name server control task.
>;
>; Creating build files for NNC, the node name collector task.
>;
>; Creating build files for NNS, the node name server.
>;
>;
>; =====================================================================
>; DEC - Section 4 - Define the DECnet Satellite Support Components
>; =====================================================================
>;
>* 02.00 Do you want the Satellite Support Components [D=N]? [Y/N]:
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; DEC - Section 5 - Define the DECnet File Utilities
>; =====================================================================
>;
>; Creating build files for NFT, the network file access user task.
>;
>; Creating build files for FTS, the network file access spooler
>; user task.
>;
>; Creating build files for FAL, the network file access server.
>;
>; FAL will support RMS file access.
>; FAL will be a multi-copy object.
>; FAL will not be overlaid.
>; FAL will use the memory resident RMS library.
>; FAL user data buffer size will be 2048 bytes.
>;
>; Creating build files for MCM, the network command or batch file
>; submission server.
>;
>; MCM requests will be queued to BATCH.
>;
>; =====================================================================
>; DEC - Section 6 - Define the DECnet Terminal and Control Utilities
>; =====================================================================
>;
>; Creating build files for RMT and RMTACP, the remote network terminal
>; task and ACP.
>;
>; The maximum number of simultaneous RMT users is 4.
>;
>; Creating build files for HT: and RMHACP, the remote network terminal
>; driver and ACP.
>;
>; RMHACP will support 4 simultaneous incoming connections.
>; HTDRV will support 4 HT: units.
>;
>; Creating build files for NCT, the network command terminal server
>;
>; Creating build files for RTH, the network command terminal host
>; support.
>;
>; Creating build files for TLK, the remote talk user task.
>;
>; Creating build files for LSN, the remote talk server task.
>;
>; Creating build files for PHO, the inter-terminal conversation utility.
>;
>; Creating build files for LAT/LCP, the Local Area Transport terminal
>; service process and LAT Control Program
>;
>; Creating build files for TCL, the remote task control server task.
>;
>;
>; =====================================================================
>; DEC - DECnet CEX Product Generation Procedure
>; DECnet question/answer section completed at 20:13:15 on 21-JAN-16
>; =====================================================================
>;
>;
>; =====================================================================
>; NET - Section 8 - Complete the CEX System Definitions
>; =====================================================================
>;
>; Creating build files for DLX, the Direct Line Access process.
>;
>* 02.00 What is the Large Data Buffer (LDB) size [D R:576.-1484. D:576.]:
>;
>; Do you want to:
>* -Continue, R-Repeat section, P-Pause, E-Exit [S]:
>;
>;
>; =====================================================================
>; NET - Section 9 - Build the CEX System at 20:13:29 on 21-JAN-16
>; =====================================================================
>;
>; All questions have now been asked and the selected components will now
>; be built. This may take from one to three hours, depending on the
>; selection of components and the system you are running on.
>;
>PIP SY:[005,054]CETAB.MAC/PU/NM
>PIP SY:[005,054]AUX.DAT/PU/NM
>;
>SET /UIC=[1,2]
>PIP OU:[1,2]NETHLP.ULB=IN:[1,2]NETHLPD.HLP
>PIP OU:[1,2]NETHLP.ULB/PU/NM
>SET /UIC=[005,024]
>;
>PIP OU:[5,54]/NV=IN:[3,54]RSXVEC.STB
>PIP OU:[5,54]/NV/CO=IN:[131,54]AUX.TSK
>PIP OU:[5,54]/NV=IN:[131,54]AUX.STB
>PIP OU:[5,54]AUX.TSK/PU/NM,AUX.STB
>MAC @OU:[5,24]CETABASM.CMD
>PIP OU:[5,24]CETAB.OBJ/PU/NM
>TKB @OU:[5,24]CETABBLD.CMD
>PIP OU:[5,54]CETAB.TSK/PU/NM,CETAB.STB
>PIP OU:[5,54]/NV/CO=IN:[132,54]NTINIT.TSK
>PIP OU:[5,54]NTINIT.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[132,54]NTL.TSK
>PIP OU:[5,54]NTL.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[132,54]MLD.TSK
>PIP OU:[5,54]/NV=IN:[132,54]MLD.STB
>PIP OU:[5,54]MLD.TSK/PU/NM,MLD.STB
>MAC @OU:[5,24]EVLASM.CMD
>PIP OU:[5,24]EVLDAT.OBJ/PU/NM
>TKB @OU:[5,24]EVLBLD.CMD
>PIP OU:[5,54]/NV=IN:[131,24]EVL.DAT
>PIP OU:[5,54]EVL.TSK/PU/NM,EVL.STB,EVL.DAT
>TKB @OU:[5,24]EVCBLD.CMD
>PIP OU:[5,54]EVC.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]NCPRES.TSK
>PIP OU:[5,54]NCPRES.TSK/PU/NM
>MAC @OU:[5,24]NMVACPASM.CMD
>PIP OU:[5,24]NMDRV.OBJ/PU/NM,NMTAB.OBJ
>TKB @OU:[5,24]NMVACPBLD.CMD
>PIP OU:[5,54]/NV/CO=IN:[135,54]NMVACP.TSK
>PIP OU:[5,54]/NV=IN:[135,54]NMVACP.STB
>PIP OU:[5,54]NMVACP.TSK/PU/NM,NMDRV.TSK,NMDRV.STB
>PIP OU:[5,54]/NV/CO=IN:[132,54]CFERES.TSK
>PIP OU:[5,54]CFERES.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[141,54]NDA.TSK
>PIP OU:[5,54]NDA.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[132,54]VNP.TSK
>PIP OU:[5,54]VNP.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]LOO.TSK
>PIP OU:[5,54]/NV=IN:[135,54]LOO.STB
>PIP OU:[5,54]LOO.TSK/PU/NM,LOO.STB
>PIP OU:[5,54]/NV/CO=IN:[135,54]EVFRES.TSK
>PIP OU:[5,54]EVFRES.TSK/PU/NM
>MAC @OU:[5,24]DLXASM.CMD
>PIP OU:[5,24]DLXTAB.OBJ/PU/NM
>TKB @OU:[5,24]DLXBLD.CMD
>PIP OU:[5,54]DLX.DAT/NV=IN:[131,24]DLX.DAT
>PIP OU:[5,54]DLX.TSK/PU/NM,DLX.STB,DLX.DAT
>PIP OU:[5,54]DLXTAB.TSK/PU/NM,DLXTAB.STB
>;
>TKB @OU:[5,24]UNABLD.CMD
>PIP OU:[5,54]UNA.TSK/PU/NM,UNA.STB
>PIP OU:[5,54]/NV=IN:[131,24]UNA.DAT
>PIP OU:[5,54]UNA.DAT/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[131,54]UNAMC.TSK
>PIP OU:[5,54]UNAMC.TSK/PU/NM
>SET /UIC=[1,1]
>PIP OU:[1,1]NETLIB.MLB/NV=IN:[1,10]NETLIBU.MLB
>PIP OU:[1,1]NETLIB.MLB/PU
>LBR OU:[1,1]NETFOR.OBS=IN:[133,24]DAPFOR/EX
>LBR OU:[1,1]NETTMP.OBS=IN:[133,24]DAPTRC/EX
>LBR OU:[1,1]NETFOR/CO:1:320.:192.=IN:[134,24]NETFOR.OLB
>LBR OU:[1,1]NETFOR/IN=OU:[1,1]NETFOR.OBS
>LBR OU:[1,1]NETFOR/IN/-EP=OU:[1,1]NETTMP.OBS
>LBR OU:[1,1]NETFOR/DG:$MBLUN:$ASTBL:$ASTLU
Entry points deleted:
$MBLUN
$ASTBL
$ASTLU
>PIP OU:[1,1]NETFOR.OBS;*/DE,NETTMP.OBS;*
>PIP OU:[1,1]NETFOR.OLB/PU
>SET /UIC=[005,024]
>PIP OU:[005,024]/NV=IN:[137,24]NTEST.CMD
>PIP OU:[005,024]NTEST.CMD/PU/NM
>SET /UIC=[005,054]
>PIP OU:[005,054]/NV/CO=IN:[133,54]DTS.TSK,DTR.TSK
>PIP OU:[005,054]DTS.TSK/PU/NM,DTR.TSK
>SET /UIC=[005,024]
>TKB @OU:[5,24]XPTBLD.CMD
>PIP OU:[5,54]XPT.DAT/NV=IN:[131,24]XPT.DAT
>PIP OU:[5,54]XPT.TSK/PU/NM,XPT.STB,XPT.DAT
>MAC @OU:[5,24]ECLASM.CMD
>PIP OU:[5,24]ECLTAB.OBJ/PU/NM
>TKB @OU:[5,24]ECLBLD.CMD
>PIP OU:[5,54]ECL.DAT/NV=IN:[131,24]ECL.DAT
>PIP OU:[5,54]ECL.TSK/PU/NM,ECL.STB,ECLTAB.TSK,ECLTAB.STB,ECL.DAT
>PIP OU:[5,54]/NV/CO=IN:[135,54]PROXY.TSK
>TKB @OU:[5,24]NETACPBLD.CMD
>PIP OU:[5,54]NETACP.TSK/PU/NM,NETACP.STB
>TKB @OU:[5,24]EPMBLD.CMD
>PIP OU:[5,54]/NV=IN:[131,24]EPM.DAT,EPMST.DAT
>PIP OU:[5,54]EPM.TSK/PU/NM,EPM.STB,EPM.DAT,EPMST.DAT
>PIP OU:[5,54]/NV/CO=IN:[135,54]NICE.TSK
>PIP OU:[5,54]NICE.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]EVR.TSK
>PIP OU:[5,54]EVR.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]NTD.TSK
>PIP OU:[5,54]NTD.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]NTDEMO.TSK
>PIP OU:[5,54]NTDEMO.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]LIN.TSK
>PIP OU:[5,54]LIN.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[135,54]MIR.TSK
>PIP OU:[5,54]/NV=IN:[135,54]MIR.STB
>PIP OU:[5,54]MIR.TSK/PU/NM,MIR.STB
>PIP OU:[5,54]/NV/CO=IN:[132,54]NVP.TSK
>PIP OU:[5,54]NVP.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[165,54]SCPRES.TSK
>PIP OU:[5,54]SCPRES.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[161,54]NNCRES.TSK
>PIP OU:[5,54]NNCRES.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[162,54]NNDRV.TSK,NNDRV.STB,NNS.TSK,IN:[162,24]NNS.DAT
>PIP OU:[5,54]NNDRV.TSK,NNDRV.STB,NNS.TSK,NNS.DAT/PU/NM
>TKB @OU:[5,24]NFTBLD.CMD
>PIP OU:[5,54]NFTRES.TSK/PU/NM
>SET /UIC=[5,24]
>MAC @OU:[5,24]FTSASM.CMD
>TKB @OU:[5,24]FTSBLD.CMD
>PIP OU:[5,54]FTSRES.TSK/PU/NM,FTSDEQRES.TSK
>SET /UIC=[5,24]
>MAC @OU:[5,24]FALASM.CMD
>PIP OU:[5,24]FALPRM.OBJ/PU/NM
>TKB @OU:[5,24]FALBLD.CMD
>PIP OU:[5,54]FAL.TSK/PU/NM,FALRES.TSK,FALFSL.TSK
>TKB @OU:[5,24]MCMBLD.CMD
>PIP OU:[5,54]MCM.TSK/PU/NM
>MAC @OU:[5,24]RMTASM.CMD
>PIP OU:[5,24]RMTACP.OBJ/PU/NM
>TKB @OU:[5,24]RMTBLD.CMD
>PIP OU:[5,54]RMT.TSK/PU/NM,RMTACP.TSK
>MAC @OU:[5,24]RMHACPASM.CMD
>PIP OU:[5,24]RMHACP.OBJ/PU/NM,HTTAB.OBJ
>TKB @OU:[5,24]RMHACPBLD.CMD
>PIP OU:[5,54]RMHACP.TSK/PU/NM,HTDRV.TSK,HTDRV.STB
>PIP OU:[5,54]/NV/CO=IN:[140,54]TRXCTL.TSK
>PIP OU:[5,54]/NV/CO=IN:[140,54]TRXCOL.TSK
>PIP OU:[5,54]TRXCTL.TSK/PU/NM
>PIP OU:[5,54]TRXCOL.TSK/PU/NM
>TKB @OU:[5,24]NCTBLD.CMD
>PIP OU:[5,54]NCT.DAT/NV=IN:[140,24]NCT.DAT
>PIP OU:[5,54]NCT.TSK/PU/NM,NCT.STB,NCT.DAT
>PIP OU:[5,54]NCT1.TSK/PU/NM,NCT1.STB
>PIP OU:[5,54]NCTCTL.TSK/PU/NM
>MAC @OU:[5,24]RTHASM.CMD
>TKB @OU:[5,24]RTHBLD.CMD
>PIP OU:[5,24]RTHTAB.OBJ/PU/NM
>PIP OU:[5,54]RTH.DAT/NV=IN:[140,24]RTH.DAT
>PIP OU:[5,54]RTH.TSK/PU/NM,RTH.STB,RTH.DAT
>PIP OU:[5,54]RTHTAB.TSK/PU/NM,RTHTAB.STB
>TKB @OU:[5,24]TLKBLD.CMD
>PIP OU:[5,54]TLKRES.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[133,54]LSN.TSK
>PIP OU:[5,54]LSN.TSK/PU/NM
>PIP OU:[5,54]/NV/CO=IN:[133,54]PHONE.TSK
>PIP OU:[5,54]PHONE.TSK/PU/NM
>SET /UIC=[1,2]
>PIP OU:[1,2]/NV=IN:[133,10]PHONEHELP.HLP
>PIP OU:[1,2]PHONEHELP.HLP/PU
>SET /UIC=[5,24]
>PIP OU:[5,54]/NV/CO=IN:[135,54]LCP.TSK
>PIP OU:[5,54]/NV/CO=IN:[131,54]LAT.TSK,LAT.STB
>PIP OU:[5,54]/NV/CO=IN:[131,54]LAT1.TSK,LAT1.STB
>PIP OU:[5,54]/NV/CO=IN:[131,54]LTD.TSK,LTD.STB
>PIP OU:[5,54]/NV/CO=IN:[131,54]LTD1.TSK,LTD1.STB
>PIP OU:[5,54]LAT.DAT/NV=IN:[131,24]LAT.DAT
>PIP OU:[5,54]LTD.DAT/NV=IN:[131,24]LTD.DAT
>PIP OU:[5,54]LAT.TSK/PU/NM,LAT.STB,LAT.DAT
>PIP OU:[5,54]LAT1.TSK/PU/NM,LAT1.STB
>PIP OU:[5,54]LTD.TSK/PU/NM,LTD.STB
>PIP OU:[5,54]LTD1.TSK/PU/NM,LTD1.STB
>PIP OU:[5,54]LTD.DAT/PU/NM
>PIP OU:[5,54]LCP.TSK/PU/NM
>MAC @OU:[5,24]TCLASM.CMD
>PIP OU:[5,24]TCLPWD.OBJ/PU/NM
>TKB @OU:[5,24]TCLBLD.CMD
>PIP OU:[5,54]TCL.TSK/PU/NM
>;
>; =====================================================================
>; NET - Section 10 - Generation Clean Up
>; =====================================================================
>;
>; Creating NETCFG.TXT, the network configuration description file.
>; Creating NETCFE.CMD, the network configuration command file.
>; Creating NETINS.CMD, the network installation command file.
>; Creating NETREM.CMD, the network removal command file.
>;
>;
>; The network HELP file library has been placed on your target disk, as:
>;
>; SY:[1,2]NETHLP.ULB
>;
>; This file should be moved to your target systems library device (LB:).
>;
>;
>; =====================================================================
>; NET - RSX-11M-PLUS CEX System Generation Procedure
>; Stopped at 20:13:49 on 21-JAN-16
>; =====================================================================
>;
>@
>RUN $SHUTUP
RSX-11M-PLUS Shut down program
Enter minutes to wait before shutdown:
Reason for shutdown ( for none):
OK to shutdown? [Y/N]: Y
All further logins are disabled
21-JAN-16 20:14 System is now shutting down -- PISTON
QUE /STO:QMG
>
STOP/ACCOUNTING SHUTUP
20:14:24 SYSLOG -- 47. Exiting
>
@LB:[1,2]SHUTUP
>VCP DISCONNECT /ALL
>@
>
ELI /NOLOG
>
ACS DB0:/BLKS=0.
ACS -- Checkpoint file now inactive
>
DMO DB0:/DEV/LOCK=V
DMO -- System disk being dismounted
DMO -- SYSTEM dismounted from DB0: *** Final dismount initiated ***
20:14:25 *** DB0: -- Dismount complete
>
DMO DL0:/DEV/LOCK=V
DMO -- TT0: dismounted from DL0: *** Final dismount initiated ***
20:14:30 *** DL0: -- Dismount complete
>
SHUTUP operation complete
комментарии # 21-01-2016 17:31, Unik

### Оставить комментарий к «Установка DECnet-11M-PLUS V4.6»

Имя
Текст комментария *

# ~Digital PDP-11~

## Навигация

## Страницы

О сайте

## Поиск

## Ссылки

- jaqblog
- Soft&Manual
- BASIC PDP-11
- PDP-11 Nostalgia
- PDP-11
- Ancient Bits adventure
- pdp-11.org.ru
- RetroCMP
- Soft
- Soft and other
- PDP2011
- Raspberry Pi PDP-11
- RSX11M.com
- Paper Tape
- TU-58 XXDP
***
- RSTS/E
- ELVIRA
- Wofford WITCH
- RSTS.org
- RSTS/E walkthru

gopher://pdp11.tk/

## Комментарии

Korchagin в Turtles Ninja
Гость в Доступный PDP-11. Часть 2.
Vladimir в PDP-11/45 online