« DECnet. Настройка LAT. Установка времени в RSX11M+ »
Коды ошибок RSX11M+
Мне часто бывает нужно посмотреть код возникнувшей ошибки в RSX11M+ и каждый раз искать в документации их не охота, поэтому выкладываю коды здесь чтобы иногда загядывать сюда :) Также эти коды используются и в RSX11M но их там меньше.

    Коды ошибок директив

    	Error Number

    Abbr	(Dec) 	(Oct) 	Meaning

    .UPN 	-1 	377 	Insufficient dynamic storage

    .INS 	-2 	376 	Specified task not installed

    .PTS 	-3 	375 	Partition too small for task

    .UNS 	-4 	374 	Insufficient dynamic storage for send

    .ULN 	-5 	373 	Unassigned logical unit number (LUN)

    .HWR 	-6 	372 	Device handler not resident

    .ACT 	-7 	371 	Task not active

    .ITS 	-8 	370 	Directive inconsistent with task state

    .FIX 	-9 	367 	Task already fixed/unfixed

    .CKP 	-10 	366 	Issuing task not checkpointable

    .TCH 	-11 	365 	Task is checkpointable

    .RBS 	-15 	361 	Receive buffer too small

    .PRI 	-16 	360 	Privilege violation

    .RSU 	-17 	357 	Resource in use

    .NSW 	-18 	356 	No swap space available

    .ILV 	-19 	355 	Illegal vector specified

    .ITN 	-20 	354 	Illegal table number

    .LNF 	-21 	353 	Logical name not found

    .AST 	-80 	260 	Directive issued/not issued from asynchronous system trap (AST)

    .MAP 	-81 	257 	Illegal mapping specified

    .lOP 	-83 	255 	Window has I/O in progress

    .ALG 	-84 	254 	Alignment error

    .WOV 	-85 	253 	Address window allocation overflow

    .NVR 	-86 	252 	Invalid region 10

    .NVW 	-87 	251 	Invalid address window 10

    .ITP 	-88 	250 	Invalid TI: parameter

    .IBS 	-89 	247 	Invalid send buffer size (greater than 25510)

    .LNL 	-90 	246 	LUN locked in use

    .lUI 	-91 	245 	Invalid User Identification Code (UIC)

    .IOU 	-92 	244 	Invalid device or unit

    .ITI 	-93 	243 	Invalid time parameters

    .PNS 	-94 	242 	Partition/region not in system

    .IPR 	-95 	241 	Invalid priority (greater than 25010)

    .ILU 	-96 	240 	Invalid logical unit number (LUN)

    .IEF 	-97 	237 	Invalid event flag (number)

    .ADP 	-98 	236 	Part of Directive Parameter Block(DPB) out of user's space

    .SDP 	-99 	235 	Directive Identification Code(DIC) or DPB size invalid

    Коды ошибок I/O

    	Error Number

    Abbr	(Dec) 	(Oct) 	Meaning

    .BAD 	-1 	377 	Bad parameters

    .IFC	-2 	376 	Invalid function code

    .DNR	-3 	375 	Device not ready

    .VER	-4 	374 	Parity error on device

    .ONP	-5 	373 	Hardware option not present

    .SPC	-6 	372 	Illegal user buffer

    .DNA	-7 	371 	Device not attached

    .DAA	-8 	370 	Device already attached

    .DUN	-9 	367 	Device not attachable

    .EOF	-10 	366 	End-of-file (EOF) detected

    .EOV	-11 	365 	End-of-volume (EOV) detected

    .WLK	-12 	364 	Write attempted to locked unit

    .DAO	-13 	363 	Data overrun

    .SRE	-14 	362 	Send/receive failure

    .ABO	-15 	361 	Request terminated

    .PRI	-16 	360 	Privilege violation

    .RSU	-17 	357 	Shareable resource in use

    .OVR	-18 	356 	Illegal overlay request

    .BYT	-19 	355 	Odd byte count (or virtual address)

    .BLK	-20 	354 	Logical block number (LBN) too large

    ,MOD	-21 	353 	Invalid Universal Digital Controller (UDC) module number

    .CON	-22 	352 	UDC connect error

    .NOD	-23 	351 	Caller's nodes exhausted

    .DFU	-24 	350 	Device full

    .IFU	-25 	347 	Index file full

    .NSF	-26 	346 	No such file

    .LCK	-27 	345 	Locked from read/write access

    .HFU	-28 	344 	File header full

    .WAC	-29 	343 	Accessed for write

    .CKS	-30 	342 	File header checksum failure

    . WAr	-31 	341 	Attribute control list format error

    .RER	-32 	340 	File processor device read error

    .WER	-33 	337 	File processor device write error

    .ALN	-34 	336 	File already accessed on logical unit number (LUN)

    .SNC	-35 	335 	File 10, file number check

    .SQC	-36 	334 	File 10, sequence number check

    .NLN	-37 	333 	No file accessed on LUN

    .CLO	-38 	332 	File was not properly closed

    .NBF	-39 	331 	Open-No buffer space available for file

    .RBG	-40 	330 	Illegal record size

    .NBK	-41 	327 	File exceeds space allocated, no blocks

    .ILL	-42 	326 	Illegal operation on File Descriptor Block (FOB)

    .BTP	-43 	325 	Bad record type

    .RAC	-44 	324 	Illegal record access bits set

    . RAT	-45 	323 	Illegal record attribute bits set

    .RCN	-46 	322 	Illegal record number-too large

    .ICE	-47 	321 	Internal consistency error

    .2DV	-48 	320 	Rename-two different devices

    .FEX·	-49 	317 	Rename-a new file name already in use

    .BDR	-50 	316 	Bad directory file

    .RNM	-51 	315 	Cannot rename old file system

    .BDI	-52 	314 	Bad directory syntax

    .FOP	-53 	313 	File already open

    .BNM	-54 	312 	Bad file name

    .BDV	-55 	311 	Bad device name

    .BBE	-56 	310 	Bad block on device

    .DUP	-57 	307 	Enter-duplicate entry in directory

    .STK	-58 	306 	Not enough stack space (File Control Services (FCS) or file control processor (FCP)

    .FHE	-59 	305 	Fatal hardware error on device

    .NFI	-60 	304 	File ID was not specified

    .ISQ	-61 	303 	Illegal sequential operation

    .EOT	-62 	302 	End-of-tape (EOT) detected

    .BVR	-63 	301 	Bad version number

    .BHD	-64 	300 	Bad file header

    .OFL	-65 	277 	Device off line

    .BCC	-66 	276 	Block check, cyclic redundancy check (CRC), or framing error

    .ONL	-67 	275 	Device on line

    .NNN	-68 	274 	No such node

    .NFW	-69 	273 	Path lost to partner

    .DIS	-69 	273 	Path lost to partner

    .8LB	-70 	272 	Bad logical buffer

    .TMM	-71 	271 	Too many outstanding messages

    .NDR	-72 	270 	No dynamic space available

    .UR}	-73 	267 	Connection rejected by user

    .NR}	-74 	266 	Connection rejected by network

    .EXP	-75 	265 	File expiration date not reached

    .BTF	-76 	264 	Bad tape format

    .NNC	-77 	263 	Not ANSI "Dn format byte count

    .NDA	-78 	262 	No data available

    .NLK	-79 	261 	Task not linked to specified ICSjICR interrupts

    .NST	-80 	260 	Specified task not installed

    .AST	-80 	260 	No asynchronous system trap(AST) specified in connect

    .FLN	-81 	257 	Device off line when offline request was issued

    .IES	-82 	256 	Invalid escape sequence

    .PES	-83 	255 	Partial escape sequence

    .ALC	-84 	254 	Allocation failure

    .ULK	-85 	253 	Unlock error

    .WCK	-86 	252 	Write-check failure

    .NTR	-87 	251 	Task not triggered

    .REJ	-88 	250 	Transfer rejected by receiving central processing unit (CPU)

    .FLG	-89 	247 	Event flag already specified

    .DSQ	-90 	246 	Disk quota exceeded

    .IQU	-91 	245 	Inconsistent qualifier usage

    .RES	-92 	244 	Circuit reset during operation

    .TML	-93 	243 	Too many links to task

    .NNT	-94 	242 	Not a network task

    .TMO	-95 	241 	Timeout on request

    .CNR	-96 	240 	Connection rejected

    .UKN	-97 	237 	Unknown name

    .SZE	-98 	236 	Unable to size device

    . MIl	-99 	235 	Media inserted incorrectly

    .SPI	-100 	234 	Spindown ignored

    .FER	-101 	233 	Forced error mark encountered

    .IRR	-102 	232 	Insufficient resources at remote node

    .sUI	-103 	231 	Service in use

    .PIO	-104 	230 	Deaccess failed due to pending I/O

    .CBE	-105 	227 	Compare buffer error

Если после не корректного выключения стали появляться такие ошибки:
10:15:42 SYSLOG -- 70. *ERROR* On scan file open
10:15:42 SYSLOG -- 4. FCS I/O error code = 334
file: DU0:[???,???]SYSSCAN.TMP;1
То исправить это можно так:
SET /DEF=[1,6]
PIP LB:[1,6]SYSSCAN.TMP;*/RM
комментарии # 15-02-2016 17:17, Unik

### Оставить комментарий к «Коды ошибок RSX11M+»

Имя
Текст комментария *

# ~Digital PDP-11~

## Навигация

## Страницы

О сайте

## Поиск

## Ссылки

- jaqblog
- Soft&Manual
- BASIC PDP-11
- PDP-11 Nostalgia
- PDP-11
- Ancient Bits adventure
- pdp-11.org.ru
- RetroCMP
- Soft
- Soft and other
- PDP2011
- Raspberry Pi PDP-11
- RSX11M.com
- Paper Tape
- TU-58 XXDP
***
- RSTS/E
- ELVIRA
- Wofford WITCH
- RSTS.org
- RSTS/E walkthru

gopher://pdp11.tk/

## Комментарии

Korchagin в Turtles Ninja
Гость в Доступный PDP-11. Часть 2.
Vladimir в PDP-11/45 online