; 2-Aug-85 PIR MIB<12> flipped ; 24-Apr-85 PIR Updated to match new style I-box ; 26-Mar-85 RLS First try for CVAX 2 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx x xxxxx 11111111111 ; label field ; * NEW FIELD PATTERNS FOR PROCESSING .MCR, .ADR, AND .ACR FILes 50 xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx111111111111111111111111111111x ; .ACR date and time 51 xx111111111111111111xxxxxxx ; location of date and time in .ADR file 52 1x ; memory in .mcr 53 1x ; memory in .acr 54 xx1111111111111111111111111111xx ; uAddress and 64 bit uWord in .mcr file 55 xx111xxxxxxxxxxxxxxxxxxxxxxxxxxx ; uAddress in .acr file 56 xxxxxxx1111111111111xxxxxxxxxxxx ; uWord in .acr file 57 xxxxxxxxxxxxxxxxxxxxxx1111xxxxxx ; first hex address printing field in .acr 58 xxxxxxxxxxxxxxxxxxxxxxxxxxx1111x ; second hex address printing field in .acr 59 xxxxxxxxxxxxxxxxxxxxx11111xxxxxx ; first page number 'p1234' in .acr 60 xxxxxxxxxxxxxxxxxxxxxxxxxx11111x ; second page number 'p2345' in .acr 61 1111xxxxxxxxxxxxxxxxxxxxxxxxxxxx ; length = number of digits between commas 62 11111 111111xxxxxxxxxxxxxxxxxxxx ; length = number of digits in microwords 101 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 00100 xxxxxxxxxxx ; ret 102 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01000 xxxxxxxxxxx ; decnext 103 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01010 xxxxxxxxxxx ; dl.bwl.at.rvm_decnext 104 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01011 xxxxxxxxxxx ; at.rvm_decnext 105 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01100 xxxxxxxxxxx ; dl.bwl.at.r_decnext 106 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01101 xxxxxxxxxxx ; at.r_decnext 107 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01110 xxxxxxxxxxx ; at.av_decnext 108 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 01111 xxxxxxxxxxx ; dl.bwl_decnext 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10000 xxxxxxxxxxx ; alu.nzv case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10001 xxxxxxxxxxx ; alu.nzc case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10010 xxxxxxxxxxx ; sc<2:0> case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10011 xxxxxxxxxxx ; sc<5:3> case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10101 xxxxxxxxxxx ; psl<26:24> case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10110 xxxxxxxxxxx ; state<2:0> case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 10111 xxxxxxxxxxx ; state<5:3> case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11000 xxxxxxxxxxx ; mem mgt1 status case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11001 xxxxxxxxxxx ; mem mgt2 status case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11010 xxxxxxxxxxx ; mem mgt3 status case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11011 xxxxxxxxxxx ; fpa'dl case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11100 xxxxxxxxxxx ; I box status case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11101 xxxxxxxxxxx ; Opcode<2:0> case 109 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 1 11110 xxxxxxxxxxx ; Load ID<2:0> case 110 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 0 0 xxxx xxxxxxxxxxx ; jump 111 xxx xxx xxxxxxxxxxxxxx xxxxx xxxxxx 0 1 xxxx xxxxxxxxxxx ; call