From: Digest <deadmail>
To: "OS/2GenAu Digest"<deadmail>
Date: Tue, 27 Jun 2006 00:00:23 EST-10EDT,10,-1,0,7200,3,-1,0,7200,3600
Subject: [os2genau_digest] No. 1317
Reply-To: <deadmail>
X-List-Unsubscribe: www.os2site.com/list/

**************************************************
Monday 26 June 2006
 Number  1317
**************************************************

Subjects for today
 
1  Re:  Printer installation : Chuck McKinnis <mckinnis at sandia dot net>

**= Email   1 ==========================**

Date:  Sun, 25 Jun 2006 13:54:22 -0600
From:  Chuck McKinnis <mckinnis at sandia dot net>
Subject:  Re:  Printer installation



Leigh Bunting wrote:
> Chuck McKinnis wrote:
> 
>> As the author of the eCS Install Local Printer routine, I can verify 
>> that it is a disaster.  It used some old IBM code that was almost 
>> impossible to make work correctly with current printers, ports, and 
>> drivers.
>>
>> The updated eCS Printer Install routine (inst_prt.zip) can be 
>> downloaded from www.ecomstation dot com.
> 
> Thanks Chuck, that worked. More in a minute.
> 
> It seems that the original attempt at installation worked but did not 
> create any printer icon, as using Chuck's suggestion said that the files 
> had already been installed.
> 
> However the instructions in the file were a bit puzzling to this old fart.
> 
> I assumed the 'EC' in instruction 3 were not supposed to be there.  
> Instruction 5 left me scratching my head, as the 'ecsins3.sgs' file did 
> not exist, so I ignored it. There was one called 'ecslns3.sgs', though. 
> Perhaps Chuck could explain what I was supposed to do with this 
> instruction.

#3 looks strange.  #3 from the web page says:

Create <boot_drive>:\ecs\system\sguide if it does not exist.

#5 does say "(if it exists)".  If it does not exist, you probably can't 
update it :).

> 
> Not that it really matters, I suppose, as the printer now is 
> operational. It is a HP Deskjet 610C that I was given, sans power 
> supply. This item, I conveniently found at a computer flea market last 
> weekend, after parting with $A5. When fired up, it refused to load paper 
> and the print heads made some funny clunking noises as they traversed. 
> Some percussive maintenance of the paper drive mechanism seems to have 
> resolved that issue.
> ----------------------------------------------
> Manual installation:
> 
> 1. Unzip the inst_prt.zip file to a work directory.
> 2. Create <boot_drive>:\ecs\system\sguide if it does not exist.
> 3. Copy the ecsprint.exe to 
> <boot_drive>:\ecs\system\*EC*sguide\ecsprint.exe.
> 4. Update the Install Local Printer object in the Printers folder to 
> execute <boot_drive>:\ecs\system\sguide\ecsprint.exe and remove any 
> parameters or working directory.
> 5. Update <boot_drive>:\ecs\system\sguide\nls\<lang>\ecsins3.sgs (if it 
> exists) by replacing "start sguide.exe 
> <boot_drive>:\ecs\system\sguide\nls\de\printer.sgs" with "start 
> ecsprint.exe"
> ------------------------------------------------
> So after many years, the originally 2nd-hand Canon BJ4200 might have to 
> be retired.
> 
> Thanks for everyone's help.
> 


-- 
Chuck McKinnis
Covenant Solutions
http://www.7cities dot net/~mckinnis/os2/
505-286-3191

Wrinkled Was Not One of the Things I Wanted to Be When I Grew Up

----------------------------------------------------------------------------------
 

