From: Digest <deadmail>
To: "OS/2GenAu Digest"<deadmail>
Date: Thu, 12 Jan 2006 00:02:10 EST-10EDT,10,-1,0,7200,3,-1,0,7200,3600
Subject: [os2genau_digest] No. 1237
Reply-To: <deadmail>
X-List-Unsubscribe: www.os2site.com/list/

**************************************************
Wednesday 11 January 2006
 Number  1237
**************************************************

Subjects for today
 
1  Re:  IBM ServeRAID 3L : Chris Graham [WarpSpeed]" <chrisg at warpspeed dot com dot au>

**= Email   1 ==========================**

Date:  Wed, 11 Jan 2006 16:01:29 +1100 (EDT)
From:  "Chris Graham [WarpSpeed]" <chrisg at warpspeed dot com dot au>
Subject:  Re:  IBM ServeRAID 3L

On Tue, 10 Jan 2006 21:06:05 +1100, Ed Durrant wrote:

>Ed Durrant wrote:
>> Chris Graham [WarpSpeed] wrote:
>>> Does anyone have one of these?
>>>
>>> Do they get LED activity when a real LED is attached to J4 - ACT_LED?
>>>
>>> I only ever get the led glowing when the machine is rebooting but never
>>> when the actual disks are in use. (Yes I'd tried both orientations).
>>>
>>> Does anyone else who has one have this issue?
>> 
>
>Here's a useful diagram - which indicates that an LED can be added - is 
>this the connector you are using ?
>
>http://www-307.ibm dot com/pc/support/site.wss/document.do?sitestyle=ibm&lndocid=MCGN-44LQ66

Yes, that labels it the Hard Drive Activity LED Connector, or ACT_LED as
silk screened on the card itself.

-Chris

WarpSpeed Computers - The Graham Utilities for OS/2.
Voice:  +61-3-9395-1504   Internet:   chrisg at warpspeed dot com dot au
FAX:    +61-3-9395-7633   Web Page:   http://www.warpspeed dot com dot au
Postal: WarpSpeed Computers, PO Box 4293, Hoppers Crossing DC, VIC 3029, AUSTRALIA


----------------------------------------------------------------------------------
 

