    DC(IV)                       5/27/74                       DC(IV)

    NAME
         dc - DC-11 communications interface

    DESCRIPTION
         The  discussion  of typewriter I/O given in tty(IV) applies
         to these devices.

         The DC-11 typewriter  interface  operates  at  any  of  four
         speeds,  independently  settable  for input and output.  The
         speed is selected by the same encoding used by the  DH  (IV)
         device  (enumerated  in stty(II)); impossible speed changes
         are ignored.

    FILES
         /dev/tty[01234567abcd]   113B Dataphones (not currently con-
         nected- see dh(IV))

    SEE ALSO
         tty(IV), stty(II), dh(IV)

    BUGS

                                  - 1 -