    DH(IV)                       5/27/74                       DH(IV)

    NAME
         dh - DH-11 communications multiplexer

    DESCRIPTION
         Each  line  attached to the DH-11 communications multiplexer
         behaves as described in tty(IV).  Input and output for each
         line  may  independently  be set to run at any of 16 speeds;
         see stty(II) for the encoding.

    FILES
         /dev/tty[f-u]

    SEE ALSO
         tty(IV), stty(II)

    BUGS

                                  - 1 -