    STTY(I)                      6/12/72                      STTY(I)

    NAME
         stty - set typewriter options

    SYNOPSIS
         stty [ option ... ]

    DESCRIPTION
         Stty  sets  certain  I/O options on the current output type-
         writer.  With no argument, it reports the  current  settings
         of  the  options.   The option strings are selected from the
         following set:

         even      allow even parity
         -even     disallow even parity
         odd       allow odd parity
         -odd      disallow odd parity
         raw       raw mode input (no erase, kill,  interrupt,  quit,
                   EOT; parity bit passed back)
         -raw      negate raw mode
         cooked    same as `-raw'
         -nl       allow carriage return for new-line, and output CR-
                   LF for carriage return or new-line
         nl        accept only new-line to end lines
         echo      echo back every character typed
         -echo     do not echo characters
         lcase     map upper case to lower case
         -lcase    do not map case
         -tabs     replace tabs by spaces when printing
         tabs      preserve tabs
         ek        reset erase and kill characters back to  normal  #
                   and @.
         erase c   set erase character to c.
         kill c    set kill character to c.
         cr0 cr1 cr2 cr3
                   select style of delay for carriage return (see be-
                   low)
         nl0 nl1 nl2 nl3
                   select style of delay for linefeed (see below)
         tab0 tab1 tab2 tab3
                   select style of delay for tab (see below)
         ff0 ff1
                   select style of delay for form feed (see below)
         tty33     set all modes suitable for Teletype model 33
         tty37     set all modes suitable for Teletype model 37
         vt05      set all modes suitable for DEC VT05 terminal
         tn300     set all modes suitable for GE Terminet 300
         ti700     set all modes suitable for Texas  Instruments  700
                   terminal
         tek       set all modes suitable for Tektronix 4014 terminal
         hup       hang up dataphone on last close.
         -hup      do not hang up dataphone on last close.
         0         hang up phone line immediately
         50 75 110 134 150 200 300 600 1200 1800 2400 4800 9600  exta
                   extb
                   Set  typewriter  baud rate to the number given, if

                                  - 1 -

    STTY(I)                      6/12/72                      STTY(I)

                   possible.  (These are the speeds supported by  the
                   DH-11 interface).

         The  various  delay algorithms are tuned to various kinds of
         terminals.  In general the specifications ending in `0' mean
         no delay for the corresponding character.

    SEE ALSO
         stty(II)

    BUGS

                                  - 2 -