## ASH8 Assembler

####

    H8/3XX REGISTER SET

    The following is a list of the H8 registers used by ASH8:

            r0  -  r7,sp            16-bit accumulators
            r0L -  r7L,spL          8-bit accumulators
            r0H -  r7H,spH          8-bit accumulators
            spL,spH,sp              stack pointers
            ccr                     condition code

    H8/3XX INSTRUCTION SET

       The  following tables list all H8/3xx mnemonics recognized by
    the ASH8 assembler.  The designation [] refers to a required ad-
    dressing mode argument.  The following list specifies the format
    for each addressing mode supported by ASH8:

            #xx:3           immediate data (3  bit)
            #xx:8           immediate data (8  bit)
            #xx:16          immediate data (16 bit)

            *dir            direct page addressing
                            (see .setdp directive)
                            0xFF00 <= dir <= 0xFFFF

            label           branch label

            rn              registers (16 bit)
                            r0-r7,sp

            rnB             registers (8 bit)
                            r0H-r7H,r0L-r7L,spH,spL

            ccr             condition code register

            @rn             register indirect

            @-rn            register indirect (auto pre-decrement)

            @rn+            register indirect (auto post-increment)

            @[offset,rn]    register indirect, 16-bit displacement

            @@offset        memory indirect, (8-bit address)

            ext             extended addressing (16-bit)

    The  terms  data, dir, label, offset, and ext may all be expres-
    sions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the H8/3xx technical data for valid modes.

    Inherent Instructions

            eepmov
            nop
            sleep
            rte
            rts

    Branch Instructions

            bcc     label                   bcs     label
            beq     label                   bf      label
            bge     label                   bgt     label
            bhi     label                   bhis    label
            bhs     label                   ble     label
            blo     label                   blos    label
            bls     label                   blt     label
            bmi     label                   bne     label
            bpl     label                   bra     label
            brn     label                   bt      label
            bvc     label                   bvs     label
            bsr     label

    Single Operand Instructions

            Free Form

            daa     rnB                     das     rnB

            dec     rnB                     inc     rnB

            neg     rnB                     not     rnB

            rotxl   rnB                     rotxr   rnB

            rotl    rnB                     rotr    rnB

            shal    rnB                     shar    rnB

            shll    rnB                     shlr    rnB

            push    rn                      pop     rn

            Byte / Word Form

            daa.b   rnB                     das.b   rnB

            dec.b   rnB                     inc.b   rnB

            neg.b   rnB                     not.b   rnB

            rotxl.b rnB                     rotxr.b rnB

            rotl.b  rnB                     rotr.b  rnB

            shal.b  rnB                     shar.b  rnB

            shll.b  rnB                     shlr.b  rnB

            push.w  rn                      pop.w   rn

    Double Operand Instructions

            Free Form

            add     rnB,rnB                 add     #xx:8,rnB
            add     rn,rn
            adds    #1,rn                   adds    #2,rn
            addx    rnB,rnB                 addx    #xx:8,rnB

            cmp     rnB,rnB                 cmp     #xx:8,rnB
            cmp     rn,rn

            sub     rnB,rnB
            sub     rn,rn
            subs    #1,rn                   subs    #2,rn
            subx    rnB,rnB                 subx    #xx:8,rnB

            and     rnB,rnB                 and     #xx:8,rnB
                                            and     #xx:8,ccr

            or      rnB,rnB                 or      #xx:8,rnB
                                            or      #xx:8,ccr

            xor     rnB,rnB                 xor     #xx:8,rnB
                                            xor     #xx:8,ccr

            Byte / Word Form

            add.b   rnB,rnB                 add.b   #xx:8,rnB
            add.w   rn,rn

            cmp.b   rnB,rnB                 cmp.b   #xx:8,rnB
            cmp.w   rn,rn

            sub.b   rnB,rnB
            sub.w   rn,rn

            addx.b  rnB,rnB                 addx.b  #xx:8,rnB

            and.b   rnB,rnB                 and.b   #xx:8,rnB
                                            and.b   #xx:8,ccr

            or.b    rnB,rnB                 or.b    #xx:8,rnB
                                            or.b    #xx:8,ccr

            subx.b  rnB,rnB                 subx.b  #xx:8,rnB

            xor.b   rnB,rnB                 xor.b   #xx:8,rnB
                                            xor.b   #xx:8,ccr

    Mov Instructions

            Free Form

            mov     rnB,rnB                 mov     rn,rn
            mov     #xx:8,rnB               mov     #xx:16,rn
            mov     @rn,rnB                 mov     @rn,rn
            mov     @[offset,rn],rnB        mov     @[offset,rn],rn
            mov     @rn+,rnB                mov     @rn+,rn
            mov     @dir,rnB
            mov     dir,rnB
            mov     *@dir,rnB
            mov     *dir,rnB
            mov     @label,rnB              mov     @label,rn
            mov     label,rnB               mov     label,rn
            mov     rnB,@rn                 mov     rn,@rn
            mov     rnB,@[offset,rn]        mov     rn,@[offset,rn]
            mov     rnB,@-rn                mov     rn,@-rn
            mov     rnB,@dir
            mov     rnB,dir
            mov     rnB,*@dir
            mov     rnB,*dir
            mov     rnB,@label              mov     rn,@label
            mov     rnB,label               mov     rn,label

            Byte / Word Form

            mov.b   rnB,rnB                 mov.w   rn,rn
            mov.b   #xx:8,rnB               mov.w   #xx:16,rn
            mov.b   @rn,rnB                 mov.w   @rn,rn
            mov.b   @[offset,rn],rnB        mov.w   @[offset,rn],rn
            mov.b   @rn+,rnB                mov.w   @rn+,rn
            mov.b   @dir,rnB
            mov.b   dir,rnB
            mov.b   *@dir,rnB
            mov.b   *dir,rnB
            mov.b   @label,rnB              mov.w   @label,rn
            mov.b   label,rnB               mov.w   label,rn
            mov.b   rnB,@rn                 mov.w   rn,@rn
            mov.b   rnB,@[offset,rn]        mov.w   rn,@[offset,rn]
            mov.b   rnB,@-rn                mov.w   rn,@-rn
            mov.b   rnB,@dir
            mov.b   rnB,dir
            mov.b   rnB,*@dir
            mov.b   rnB,*dir
            mov.b   rnB,@label              mov.w   rn,@label
            mov.b   rnB,label               mov.w   rn,label

    Bit Manipulation Instructions

            bld     #xx:3,rnB               bld     #xx:3,@rn
            bld     #xx:3,@dir              bld     #xx:3,dir
            bld     #xx:3,*@dir             bld     #xx:3,*dir

            bild    #xx:3,rnB               bild    #xx:3,@rn
            bild    #xx:3,@dir              bild    #xx:3,dir
            bild    #xx:3,*@dir             bild    #xx:3,*dir

            bst     #xx:3,rnB               bst     #xx:3,@rn
            bst     #xx:3,@dir              bst     #xx:3,dir
            bst     #xx:3,*@dir             bst     #xx:3,*dir

            bist    #xx:3,rnB               bist    #xx:3,@rn
            bist    #xx:3,@dir              bist    #xx:3,dir
            bist    #xx:3,*@dir             bist    #xx:3,*dir

            band    #xx:3,rnB               band    #xx:3,@rn
            band    #xx:3,@dir              band    #xx:3,dir
            band    #xx:3,*@dir             band    #xx:3,*dir

            biand   #xx:3,rnB               biand   #xx:3,@rn
            biand   #xx:3,@dir              biand   #xx:3,dir
            biand   #xx:3,*@dir             biand   #xx:3,*dir

            bor     #xx:3,rnB               bor     #xx:3,@rn
            bor     #xx:3,@dir              bor     #xx:3,dir
            bor     #xx:3,*@dir             bor     #xx:3,*dir

            bior    #xx:3,rnB               bior    #xx:3,@rn
            bior    #xx:3,@dir              bior    #xx:3,dir
            bior    #xx:3,*@dir             bior    #xx:3,*dir

            bxor    #xx:3,rnB               bxor    #xx:3,@rn
            bxor    #xx:3,@dir              bxor    #xx:3,dir
            bxor    #xx:3,*@dir             bxor    #xx:3,*dir

            bixor   #xx:3,rnB               bixor   #xx:3,@rn
            bixor   #xx:3,@dir              bixor   #xx:3,dir
            bixor   #xx:3,*@dir             bixor   #xx:3,*dir

    Extended Bit Manipulation Instructions

            bset    #xx:3,rnB               bset    #xx:3,@rn
            bset    #xx:3,@dir              bset    #xx:3,dir
            bset    #xx:3,*@dir             bset    #xx:3,*dir
            bset    rnB,rnB                 bset    rnB,@rn
            bset    rnB,@dir                bset    rnB,dir
            bset    rnB,*@dir               bset    rnB,*dir

            bclr    #xx:3,rnB               bclr    #xx:3,@rn
            bclr    #xx:3,@dir              bclr    #xx:3,dir
            bclr    #xx:3,*@dir             bclr    #xx:3,*dir
            bclr    rnB,rnB                 bclr    rnB,@rn
            bclr    rnB,@dir                bclr    rnB,dir
            bclr    rnB,*@dir               bclr    rnB,*dir

            bnot    #xx:3,rnB               bnot    #xx:3,@rn
            bnot    #xx:3,@dir              bnot    #xx:3,dir
            bnot    #xx:3,*@dir             bnot    #xx:3,*dir
            bnot    rnB,rnB                 bnot    rnB,@rn
            bnot    rnB,@dir                bnot    rnB,dir
            bnot    rnB,*@dir               bnot    rnB,*dir

            btst    #xx:3,rnB               btst    #xx:3,@rn
            btst    #xx:3,@dir              btst    #xx:3,dir
            btst    #xx:3,*@dir             btst    #xx:3,*dir
            btst    rnB,rnB                 btst    rnB,@rn
            btst    rnB,@dir                btst    rnB,dir
            btst    rnB,*@dir               btst    rnB,*dir

    Condition Code Instructions

            andc    #xx:8,ccr               andc    #xx:8
            and     #xx:8,ccr               and.b   #xx:8,ccr

            ldc     #xx:8,ccr               ldc     #xx:8
            ldc     rnB,ccr                 ldc     rnB

            orc     #xx:8,ccr               orc     #xx:8
            or      #xx:8,ccr               or.b    #xx:8,ccr

            xorc    #xx:8,ccr               xorc    #xx:8
            xor     #xx:8,ccr               xor.b   #xx:8,ccr

            stc     ccr,rnB                 stc     rnB

    Other Instructions

            divxu   rnB,rn                  divxu.b rnB,rn

            mulxu   rnB,rn                  mulxu.b rnB,rn

            movfpe  @label,rnB              movfpe  label,rnB
            movfpe.b  @label,rnB            movfpe.b  label,rnB

            movtpe  @label,rnB              movtpe  label,rnB
            movtpe.b  @label,rnB            movtpe.b  label,rnB

    Jump and Jump to Subroutine Instructions

            jmp     @rn                     jmp     @@dir
            jmp     @label                  jmp     label

            jsr     @rn                     jsr     @@dir
            jsr     @label                  jsr     label

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: January 2006