# 2.11BSD#431 - /usr/src/sys/autoconfig/raauto.c

##### Functions

    raprobe           X

       1: /*
       2:  * Copyright (c) 1986 Regents of the University of California.
       3:  * All rights reserved.  The Berkeley software License Agreement
       4:  * specifies the terms and conditions for redistribution.
       5:  *
       6:  *	@(#)raauto.c	1.2 (2.11BSD GTE) 12/30/92
       7:  */
       8:
       9: #include "param.h"
      10: #include "../machine/autoconfig.h"
      11: #include "../machine/machparam.h"
      12:
      13: /*
      14:  * This is one of the few devices which could use the 'vector' parameter.
      15:  * Forcing an interrupt from a MSCP device is a large enough undertaking
      16:  * that it hasn't been done (yet).
      17: */
      18: raprobe(addr,vector)
      19:     u_int *addr;
      20:     int vector;
      21: {
      22:     extern int  errno;
      23:
      24:     errno = 0;
      25:     grab(addr);
      26:     return(errno ? ACP_NXDEV : ACP_EXISTS);
      27: }

#### Defined functions

raprobe defined in line 18; used 2 times

- in /usr/src/sys/autoconfig/uprobe.c line 26, 32

Last modified: 1992-12-31 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 471 |