# 2.11BSD#431 - /usr/src/sys/autoconfig/xpauto.c

##### Functions

    xpprobe           X

       1: /*
       2:  * Copyright (c) 1986 Regents of the University of California.
       3:  * All rights reserved.  The Berkeley software License Agreement
       4:  * specifies the terms and conditions for redistribution.
       5:  *
       6:  *	@(#)xpauto.c	1.2 (2.11BSD GTE) 12/30/92
       7:  */
       8:
       9: /*
      10:  * Several drives use this probe routine.
      11:  *
      12:  * hp -- rjp04/06, rwp04/06
      13:  * rm -- rjm02/rwm03, rm02/03/05
      14:  * xp -- rm02/03/05, rp04/05/06, Diva, Ampex, SI Eagle, Fuji 160
      15:  */
      16: #include "param.h"
      17: #include "../machine/autoconfig.h"
      18: #include "../machine/machparam.h"
      19:
      20: #include "hpreg.h"
      21:
      22: xpprobe(addr,vector)
      23:     struct hpdevice *addr;
      24: {
      25:     stuff(HP_IE | HP_RDY, &(addr->hpcs1.w));
      26:     DELAY(10L);
      27:     stuff(0, &(addr->hpcs1.w));
      28:     return(ACP_IFINTR);
      29: }

#### Defined functions

xpprobe defined in line 22; used 3 times

- in /usr/src/sys/autoconfig/uprobe.c line 24, 31-36(2)

Last modified: 1992-12-31 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 493 |