 wyse_termcap_entries.txt
 =:=:=:==:=:=:==:=:=:==:=

The first part of this file contains entries for the terminfo and/or termcap
terminal-infomation database of a Unix system.  Some are tested, some not.

Further down is some discussion about quirks and problems encountered with
various terminfo/termcap settings (and other configuration, as with stty).

 =:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=

Path: cs.utk.edu!darwin.sura.net!jabba.ess.harris.com!news.ess.harris.com
      !sol.ctr.columbia.edu!howland.reston.ans.net!vixen.cso.uiuc.edu
      !owens.slip.uiuc.edu!jbn
From: (J.B. Nicholson-Owens)
Newsgroups: comp.terminals
Subject: Re: Wyse-50
Date: 8 Sep 94 22:04:04 GMT
Organization: University of Illinois at Urbana
Lines: 52
Message-ID: <jbn.779061844@owens.slip.uiuc.edu>
References: <34nh87$n19@vixen.cso.uiuc.edu>
Reply-To: no email - don't reply (J.B. Nicholson-Owens)
NNTP-Posting-Host: owens.slip.uiuc.edu

gdewan@prairienet.org (Geoffrey DeWan) writes:
>
> I have a Wyse-50 terminal but no manuals.  Would there be any on-line
> documentation for this thing anywhere.  Any titles for off-line documentation
> I could look up?

Purchase "termcap & terminfo" from O'Reilly & Associates, Inc.  It's
available from any technical bookstore and contains a beginner termcap
and terminfo listing for the Wyse-50 (as well as the guidance to help
you fill out the rest of it).  You will also need to call Wyse and
purchase a Wyse-50 manual (I've heard they're cheap).

Any fully-defined terminfo entry will (most likely) be better than any
fully-defined termcap entry (since termcap is so limited and imprecise
wrt delays), but here's a maximized termcap entry for the Wyse-50 to
get you started:

# Wyse 50 termcap by J.B. Nicholson-Owens
w9|wy50|wyse50|wyse 50|Wyse Technology WY-50:\
        :am:bw:bc=^H:co#80:li#24:up=^K:do=0.5*^J:le=^H:ho=^^:nd=^L:cr=^M:\
        :sf=^J:sr=\Ej:dl=\ER:dc=\EW:nw=^M^J:al=\EE:ce=\ET:cd=\EY:cl=5.5*\E*:\
        :cm=\Ea%i%dR%dC:im=\Eq:ei=\Er:mi:ct=\E0:st=\E1:it#8:ta=^I:pt:bt=\EI:\
        :so=\EG4:se=\EG0:sg#1:us=\EG8:ue=\EG0:ug#1:mr=\EG8:mb=\EG2:mh=\EGp:\
        :mk=\EG1:mp=\E):is=100*\E`\072:rs=100*\E';:lq=F27:lr=F28:ls=F29:\
        :vb=\E`8\EA04\EA00\E'9:bl=^G:vs=\E'1\E'5:vi=\E'0:ve=\E'1\E'5:lt=F30:\
        :lu=F31:lv=F32:LO=\EA14:LF=\EA11:Nl#8:lw#9:ul:lh#1:ku=^K:kl=^H:kr=^L:\
        :kd=^J:kh=^^:kb=^H:kC=\EY:kD=\EW:kL=\ER:kM=\Er:kI=\EQ:kA=\EE:kN=\EK:\
        :kP=\EJ:ma=^Kj^Jk^Hh^Ll^^H:kE=\ET:kS=\EY:@8=\E7:%9=\EP:&3=\Er:nl=^J:\
        :#2=\E{:#4=^H:%f=\EP:%i=^L:me=\E(\EG0:kn#32:k1=^A@^M:k2=^AA^M:*8=\EY:\
        :k3=^AB^M:k4=^AC^M:k5=^AD^M:k6=^AE^M:k7=^AF^M:k8=^AG^M:k9=^AH^M:\
        :k0=^AI^M:k;=^AJ^M:F1=^AK^M:F2=^AL^M:F3=^AM^M:F4=^AN^M:F5=^AO^M:\
        :if=/usr/local/lib/tabset/wyse50.init:ic=\EQ:mi:ip=17*:\
        :rf=/usr/local/lib/tabset/wyse50.reset:

These two uuencoded files are also necessary:

begin 660 wyse50.init
F/&-L96%R('1A8G,^"CQS970@=&%B<R!E=F5R>2`X(&-H87)S/@HA
`
end

begin 660 wyse50.reset
M/'-E="!S8W)E96X@=&\@.#`@8V]L=6UN<SX*/'1U<FX@;V9F(&%L;"!S<&5C
M:6%L(&5F9F5C=',L('!R;W1E8W1E9"!C:&%R<RP@<W1A='5S(&QI;F5S("8@
M9G5N8W1I;VX@:V5Y"B!L86)E;',^"CQD;R!E=F5R>71H:6YG(&EN('1H92!I
M;FET9FEL92`O=7-R+VQO8V%L+VQI8B]T86)S970O=WES934P+FEN:70^"CQC
M;&5A<B!S8W)E96X@=&\@<W!A8V5S/@H\8VQE87(@<V-R965N('1O(&YU;&QS
'('1O;S\^"G)E
`
end
--
Do not try to respond to this message in e-mail, it will never get
here.

 =:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=


Article 3139 of comp.terminals:
Newsgroups: comp.terminals
Path: utkcs2!darwin.sura.net!europa.asd.contel.com!uunet!munnari.oz.au!bruce.cs.monash.edu.au!merlin!robin
From: robin@resmel.bhp.com.au (Robin Brown)
Subject: SUMMARY: wyse60 termcap entries
Message-ID: <BoIx65.2Fo@resmel.bhp.com.au>
Organization: BHP Research - Melbourne Laboratories, AUSTRALIA
Date: Wed, 20 May 1992 00:25:14 GMT
Lines: 2092

Here are all the replies I received from my posting to comp.sys.admin.
enjoy....

Robin
robin@resmel.bhp.com.au
----------------------------------
From bob@pta.pyramid.com.au Tue Mar 31 21:19:22 1992
Received: from pta.pyramid.com.au by merlin.resmel.bhp.com.au with SMTP id AA13309
  (5.65b/IDA-1.4.3 for robin); Tue, 31 Mar 92 21:18:45 +1100
Received: by pta.pyramid.com.au id AA15388
  (5.65c/IDA-1.4.4 for robin@resmel.bhp.com.au); Tue, 31 Mar 1992 20:18:22 +1000
Date: Tue, 31 Mar 1992 20:18:22 +1000
From: Bob Vernon <bob@pta.pyramid.com.au>
Message-Id: <199203311018.AA15388@pta.pyramid.com.au>
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
In-Reply-To: <1992Mar31.005748.3186@resmel.bhp.com.au>
Organization: Pyramid Technology Corporation, Sydney
Status: OR

In article <1992Mar31.005748.3186@resmel.bhp.com.au> you write:
>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin

I think this one has a few non-standard extensions in it.

Bob V!

-------------
# Wyse60 modified by Bob Vernon 10/8/88, to support status line and pages.
# & John 21/03/90 for 132 columns
60-w|wyse60-w|wy60-w:\
        :sf=^J:cr=^M:\
        :ks=\E`c\EA1t\Ez\177\Ez(^M:ke=\E`b\EA11:\
        :ms:co#132:li#24:bs:am:mi:ws#78:\
        :cm=\E=%+ %+ :nd=^l:up=^k:do=^v:ho=\E{:\
        :al=\EE:dl=\ER:ei=\Er:im=\Eq:\
        :cd=\Ey:ce=\Et:cl=\E*:dc=\EW:\
        :sg#0:so=\E):se=\E(:ue=\EG0:ug#1:us=\EG8:\
        :kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:\
        :k1=^A@^M:k2=^AA^M:k3=^AB^M:k4=^AC^M:k5=^AD^M:\
        :k6=^AE^M:k7=^AF^M:k8=^AG^M:l9=^AO^M:\
	:Wn#2:Wf=\EwB:Wb=\EwC:\
	:GS=\EH^B:GE=\EH^C:G1=3:G2=2:G3=1:G4=5:GH=\072:GV=6:\
	:sW=\E`\073:sN=\E`\072:\
	:hs:ts=^[A14^[z(:fs=^M:ds=^[z(^M^[A10:cg#2:


      -m-------   Robert Vernon			  bob@pta.pyramid.com.au
    ---mmm-----   Pyramid Technology (Australia)
  -----mmmmm---   402 Pacific Highway		  PHONE: +61 2 901 5333
-------mmmmmmm-   Artarmon 2064 Australia	  FAX: +61 2 906 4353

From rdp1!kriz@seq.uncwil.edu Wed Apr  1 00:48:30 1992
Received: from seq.uncwil.edu by merlin.resmel.bhp.com.au with SMTP id AA16890
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 00:48:18 +1100
Received: by seq.uncwil.edu (5.61/1.35.cgs)
	id AA14249; Tue, 31 Mar 92 08:48:12 -0500
Received: by rdp1 (5.51/6.2); Tue, 31 Mar 92 08:46:07 EST
From: kriz <rdp1!kriz@seq.uncwil.edu>
Message-Id: <9203311346.AA18565@rdp1>
Subject: termcap entry for wy60
To: robin@resmel.bhp.com.au
Date: Tue, 31 Mar 92 8:46:03 EST
Status: OR


here it is, in all its glory:

wy60|wyse-60,
	am, bw, hs, ul,
	cols#80, lines#24,
	bel=^G, blink=\EG2, bold=\EG0, cbt=\EI, civis=\E`0,
	clear=^^\E+$<10>, cub1=\b, cud1=\n, cuf1=\f,
	cup=\E=%p1%'\s'%+%c%p2%'\s'%+%c, cuu1=^K, cvvis=\E`1,
	dl=\ER$<10>, dl1=\ER$<10>, ed=\EY, el=\ET, home=^^,
	ht=\t, hts=\E1, il=\EE$<10>, il1=\EE$<10>, ind=\n,
	invis=\EG1, kcub1=\b, kcud1=\n, kcuf1=\f, kcuu1=^K,
	kf0=^AI\r, kf1=^A@\r, kf2=^AA\r, kf3=^AB\r, kf4=^AC\r,
	kf5=^AD\r, kf6=^AE\r, kf7=^AF\r, kf8=^AG\r, kf9=^AH\r,
	khome=^^, nel=\r\n, rev=\EG4, ri=\Ej, rmso=\EGp,
	rmul=\EGp, sgr0=\EGp, smso=\EG4, smul=\EG8, tbc=\E3,

and for a wyse 60 with 2 pages of memory:

wy60-2p|wyse 60 with 2 pages of memory,
	am, bw, hs, km, mir, msgr, xon,
	cols#80, lines#24,
	bel=^G, cbt=\EI, civis=\E`0, clear=\E*$<100>,
	cnorm=\E`1, cr=\r, cub1=\b, cud1=\n, cuf1=\f,
	cup=\E=%p1%'\s'%+%c%p2%'\s'%+%c, cuu1=^K,
	dch1=\EW$<11>, dl1=\ER$<5>, dsl=\EF\r, ed=\Ey$<100>,
	el=\Et, fsl=\r, home=^^, ht=\t, hts=\E1, il1=\EE$<4>,
	ind=\n, ip=$<3>, is1=\EcB0\EcC1,
	is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1\EwJ\Ew1^N^T$<150>,
	kbs=\b, kcbt=\EI, kcub1=\b, kcud1=\n, kcuf1=\f,
	kcuu1=^K, kdch1=\EW, kdl1=\ER, kf1=^A@\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r, kf7=^AF\r,
	kf8=^AG\r, kf9=^AH\r, khome=^^, kil1=\EE, ri=\Ej$<7>,
	rmacs=\EH^C, rmcup=\Ew1, rmir=\Er, rmso=\EG0,
	rmul=\EG0, rs1=\E~!\E~4$<150>, rs2=\EeG$<150>,
	rs3=\EwG\Ee($<200>, smacs=\EH^B, smcup=\Ew0, smir=\Eq,
	smso=\EGt, smul=\EG8, tbc=\E0, tsl=\EF,
	uc=\EG8%p1%c\EG0,


enjoy!

-- 
patti krizowsky                    e-mail:  kriz@seq.uncwil.edu

"Remember the last words of my grandfather, who said 'A truck!'" - Emo Phillips
                vote Ren and Stimpy in '92!

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -


From cooper@next210.NoDak.edu Wed Apr  1 02:36:24 1992
Received: from plains.NoDak.edu by merlin.resmel.bhp.com.au with SMTP id AA17149
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 02:35:53 +1100
Received: from next210.ndsu.NoDak.edu  (next210.NoDak.edu) by plains.NoDak.edu; Tue, 31 Mar 1992 09:35:32 -0600
Received: by  next210.ndsu.NoDak.edu  (NeXT-1.0 (From Sendmail 5.52)/NeXT-1.0)
	id AA03859; Tue, 31 Mar 92 09:34:50 CST
Date: Tue, 31 Mar 92 09:34:50 CST
From: cooper@next210.NoDak.edu (Jeff Cooper)
Message-Id: <9203311534.AA03859@ next210.ndsu.NoDak.edu >
Received: by NeXT Mailer (1.62)
To: Robin Brown <robin@resmel.bhp.com.au>
Subject: Wyse 60 termcap
Status: OR

Here's the wyse60 entries from /etc/termcap on my NeXTstation...hope this  
helps.

Jeff Cooper
cooper@plains.nodak.edu

--- cut here ---

#
# Basic wyse-60 entry, only used as tc entry
#       Does not specify co, is, rs, vb, ve, or vs
#       or any status line parameters
#
wM|w60base|wyse60base|base wyse 60 entry:\
        :ae=\EcD:al=2\EE:am:as=\EcE:bl=^G:bs:bt=\EI:bw:cd=2*\EY:ce=2\ET:\
        :cl=100\E+:cm=\E=%+ %+ :ct=\E0:da:db:dc=\EW:dl=2\ER:do=^J:ei=\Er:\
        :ho=^^:im=\Eq:kd=\EB:kh=\E{:kl=\ED:kr=\EC:\
        :ks=200\E~2\EZ1+\EA\177\EZ1,\EB\177\EZ1.\EC\177\EZ1-\ED\177\EZ1*\E{\17 
7:\
        :ku=\EA:le=^H:ll=^^^K:lm#0:mb=\EG2:me=\EG0:mh=\EGp:mi:mk=\EG1:\
        :mr=\EG4:ms:nd=^L:nw=\177:se=\EG0:sf=^J:so=\EG4:sr=\Ej:st=\E1:tw#8:\
        :ue=\EG0:up=^K:us=\EG8:vi=95\E`0:
#       :TN=\E`\072:TW=\E`;:ue=\EG0:up=^K:us=\EG8:vi=100\E`0:
#
# wyse-60 in 24 line mode
#
wN|w60|wyse60|wyse60-24:\
        :co#80:\
        :is=200\Ee6\Ec20\E`@\Ed/\E`\072\Ee1\EH^C\Er\EcD\E`4\E`a\EA00\EA10\EA2x 
\EA3x:\
        :li#24:\
        :rs=\E~4\Eu\Ee6\Ec20\Ec40\EC\EDF\EeO\E~.\E`@\Ed/\EO\Ed*\Ee4\E`1\Ee(\Ee 
F\E`\072\E`9\El\Ee"\Ee1\E(\E'\EH^C\E`I\Er\EcD\E`4\E`a\EA00\EA10\EA2x\EA3x:\
        :vb=\EA34\EFB E E E E E E E E P ! ! ! !  
!^M\200\200\200\200\200\200\200\200\200\200\200\200\EF^M\EA3x:\
        :ve=100\E`4:vs=100\E`5:tc=w60base:
#
# wyse-60 in 42 line mode
#
wO|w60-42|wyse60-42:\
        :co#80:\
        :is=200\Ee6\Ec20\E`@\Ed/\E`\072\Ee1\EH^C\Er\EcD\E`4\E`a\EA00\EA10\EA2x 
\EA3x:\
        :li#42:\
        :rs=\E~4\Eu\Ee6\Ec20\Ec40\EC\EDF\EeO\E~.\E`@\Ed/\EO\Ed*\Ee4\E`1\Ee*\Ee 
F\E`\072\E`9\El\Ee"\Ee1\E(\E'\EH^C\E`I\Er\EcD\E`4\E`a\EA00\EA10\EA2x\EA3x:\
        :vb=\EA34\EFB E E E E E E E E P ! ! ! !  
!^M\200\200\200\200\200\200\200\200\200\200\200\200\EF^M\EA3x:\
        :ve=100\E`4:vs=100\E`5:tc=w60base:
#
# wyse 60 in 42 line mode with status line
#
wP|w60-42-s|wyse60-42-s:\
        :co#80:ds=\EA11:fs=\r:hs:\
        :is=200\Ee6\Ec20\E`@\Ed/\E`\072\Ee1\EH^C\Er\EcD\E`4\E`a\EA00\EA10\EA2x 
\EA3x:\
        :li#42:\
        :rs=\E~4\Eu\Ee6\Ec20\Ec40\EC\EDF\EeO\E~.\E`@\Ed/\EO\Ed*\Ee4\E`1\Ee*\Ee 
F\E`\072\E`9\El\Ee"\Ee1\E(\E'\EH^C\E`I\Er\EcD\E`4\E`a\EA00\EA10\EA2x\EA3x:\
        :ts=\EA1t\Ez(:\
        :vb=\EA34\EFB E E E E E E E E P ! ! ! !  
!^M\200\200\200\200\200\200\200\200\200\200\200\200\EF^M\EA3x:\
        :ve=100\E`4:vs=100\E`5:ls#78:ws#78:tc=w60base:
#

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From ryptyde!scott@nosc.mil Wed Apr  1 02:58:06 1992
Received: from trout.nosc.mil by merlin.resmel.bhp.com.au with SMTP id AA17203
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 02:57:55 +1100
Received: by trout.nosc.mil (5.59/1.27)
	id AA04582; Tue, 31 Mar 92 07:57:42 PST
Received: by ryptyde.cts.com (Smail3.1.21.1 #21)
	id <m0lVlAk-000DT3C@ryptyde.cts.com>; Tue, 31 Mar 92 07:54 PST
Message-Id: <m0lVlAk-000DT3C@ryptyde.cts.com>
Date: Tue, 31 Mar 92 07:54 PST
From: scott@ryptyde.cts.com (Scott McClure)
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Status: OR

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin

Okay, here's what I have:


#	@(#) termcap.src 
#
#  Special manufacturer codes:
#	M: Misc. (with only a few terminals)
#  	q: Homemade
#  	s: special (dialup, etc.)
#  
#@##############################################################################
#    Wyse 60
#    Clearing of arrow keys useful in 'is' in case this entry is
#    used after wy60ak entry was used.
#
w7|wy60|wyse60|Wyse WY-60 with 80 column/24 line screen in wy60 mode:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\177\EZ1,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
# Wy60ak:
# Arrow keys are programmed to emit ANSI standard sequences.  Allows 
# applications to distinguish between destructive Back Space and
# non-destructive Left Arrow Key.  END and INS keys also emit
# ANSI standard sequences.
# Held out `te' string so that `is' will remain in effect
# throughout login session.
# On the Enhanced PC Keyboard, only the Cursor Keypad between the Main
# Keypad and the Numeric Keypad is programmable.  These arrow keys
# and special cursor motion keys will function as labeled when using
# wy60ak with applications supporting the wy60ak entry. The Numeric
# Keypad cursor motion keys will continue to emit their default values.
#
WA|wy60ak|wyse60ak|Wyse 60 in wy60 mode with ANSI arrow keys +:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:ti=\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:EN=\E[F:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
w8|wy60w|wyse60w|Wyse WY-60 with 132 column/24 line screen in wy60 mode:\
	:is=\E`\073\Ee(\EO\Ee6\Ec41\E~4\Ec21:\
	:if=/usr/lib/tabset/std:pt:\
	:G1=\EH3:G2=\EH2:G3=\EH1:G4=\EH5:GD=\EH0:GG#0:GH=\EH\072:\
	:GU=\EH=:GV=\EH6:GR=\EH4:GL=\EH9:GC=\EH8:GF=\EH7:\
	:PU=\EJ:PD=\EK:\
	:al=\EE:am:bs:bt=\EI:cd=\EY:ce=\ET:cl=\E+:\
	:cm=\Ea%i%dR%dC:co#132:dc=\EW:dl=\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:sg#0:ug#0:ue=\EG0:ul:up=^K:us=\EG8:
#
#	Wyse Technology
#	3571 North First Street
#	San Jose, CA 95134
#
#	The Wyse 60 is like the Wyse 50 but with more padding.
#	The reset strings are slow and the pad times very depending
#	on other parameters such as font loading.  I have tried
#	to follow the following outline:
#		rs1 -> set personality
#		rs2 -> set number of columns
#		rs3 -> set number of lines
#		is1 -> select the proper font
#		is2 -> do the initialization
#		is3 -> set up display memory (2 pages)
#
#	The Wyse 60's that have vt100 emulation are slower than the
#	older Wyse 60's.  This change happened mid-1987.
#	The capabilities affected are (dch1) (dl1) (il1) (ind) (ri)
#
#	It may be useful to assign two function keys with the
#	values  \E=(\s  look at old data in page 1
#	        \E=W,   look at bottem of page 1
#	Note:							###
#	   The Wyse 60 runs faster when the XON/XOFF		###
#	   handshake is turned off.				###
#
wr|wy60-25|wyse60-25|wyse 60 80-column 25-lines:\
	:is=\E`\072\Ee)\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:li#25:r3=200\EwG\Ee):\
	:tc=wy60:
w9|wy60w-25|wyse60w-25|wy60-25-w|wyse60-25-w|wyse 60 132-column 25-lines:\
	:is=\E`\073\Ee)\EO\Ee6\Ec41\E~4\Ec21:\
	:li#25:r3=200\EwG\Ee):\
	:tc=wy60w:
wv|wy60-42|wyse60-42|wyse 60 80-column 42-lines:\
	:is=\E`\072\Ee*\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:al=11\EE:cd=260\Ey:cl=260\E*:cm=2\E=%+ %+ :dc=16\EW:\
	:dl=11\ER:i1=\EcB2\EcC3:ip=5:li#42:r3=150\Ee*:sr=10\Ej:\
	:tc=wy60:
wx|wy60w-42|wyse60w-42|wy60-42-w|wyse60-42-w|wyse 60 132-column 42-lines:\
	:is=\E`\073\Ee*\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:cm=2\Ea%i%dR%dC:co#132:dc=19\EW:ho=2^^:ip=6:r2=300\EeF\E`;:\
	:tc=wy60-42:
wz|wy60-43|wyse60-43|wyse 60 80-column 43-lines:\
	:is=\E`\072\Ee+\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:li#43:r3=150\Ee+:\
	:tc=wy60-42:
W1|wy60w-43|wyse60w-43|wy60-43-w|wyse60-43-w|wyse 60 132-column 43-lines:\
	:is=\E`\073\Ee+\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:li#43:r3=150\Ee+:\
	:tc=wy60-42-w:
W2|wy60-vb|wyse60-vb|Wyse 60 Visible bell:\
	:vb=\E`8\E`9:\
	:tc=wy60:
wf|wy60w-vb|wyse60w-vb|wy60-w-vb|wy60-wvb|wyse60-wvb|Wyse 60 132-column Visible bell:\
	:vb=\E`8\E`9:\
	:tc=wy60w:


Hope this helps,

Scott

-- 
INTERNET:  scott@ryptyde.cts.com
ARPANET:   ryptyde!scott@nosc.mil
UUCP:      {crash nosc}!ryptyde!scott

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From wvus!pete@elroy.Jpl.Nasa.Gov Wed Apr  1 03:50:23 1992
Received: from elroy.jpl.nasa.gov by merlin.resmel.bhp.com.au with SMTP id AA17373
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 03:50:10 +1100
Received: from wvus.UUCP by elroy.Jpl.Nasa.Gov (4.1/SMI-4.1+DXR)
	id AA09994; Tue, 31 Mar 92 08:50:01 PST
From: Pete Gregory - UNIX SA <pete@wvus.org>
X-Mailer: SCO System V Mail (version 3.2)
To: robin@resmel.bhp.com.au
Date: Tue, 31 Mar 92 8:43:32 PST
Message-Id:  <9203310843.aa13232@wvus.wvus.org>
Status: OR

To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
In-Reply-To: <1992Mar31.005748.3186@resmel.bhp.com.au>
Organization: World Vision U.S.

In article <1992Mar31.005748.3186@resmel.bhp.com.au> you write:
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.

here's mine.  i don't guarantee its accuracy as i don't even have a
wyse60...

#    Wyse 60
#    Clearing of arrow keys useful in 'is' in case this entry is
#    used after wy60ak entry was used.
w7|wy60|wyse60|Wyse WY-60 with 80 column/24 line screen in wy60 mode:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\177\EZ1,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:sg#0:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
# Wy60ak:
# Arrow keys are programmed to emit ANSI standard sequences.  Allows 
# applications to distinguish between destructive Back Space and
# non-destructive Left Arrow Key.  END and INS keys also emit
# ANSI standard sequences.
# Held out `te' string so that `is' will remain in effect
# throughout login session.
# On the Enhanced PC Keyboard, only the Cursor Keypad between the Main
# Keypad and the Numeric Keypad is programmable.  These arrow keys
# and special cursor motion keys will function as labeled when using
# wy60ak with applications supporting the wy60ak entry. The Numeric
# Keypad cursor motion keys will continue to emit their default values.
#
WA|wy60ak|wyse60ak|Wyse 60 in wy60 mode with ANSI arrow keys +:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:ti=\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:EN=\E[F:\
	:tc=wy60:
w8|wy60w|wyse60w|Wyse WY-60 with 132 column/24 line screen in wy60 mode:\
	:is=\E`\073\Ee(\EO\Ee6\Ec41\E~4\Ec21:\
	:if=/usr/lib/tabset/std:pt:\
	:G1=\EH3:G2=\EH2:G3=\EH1:G4=\EH5:GD=\EH0:GG#0:GH=\EH\072:\
	:GU=\EH=:GV=\EH6:GR=\EH4:GL=\EH9:GC=\EH8:GF=\EH7:\
	:PU=\EJ:PD=\EK:\
	:al=\EE:am:bs:bt=\EI:cd=\EY:ce=\ET:cl=\E+:\
	:cm=\Ea%i%dR%dC:co#132:dc=\EW:dl=\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:sg#0:ug#0:ue=\EG0:ul:up=^K:us=\EG8:
#
#	The Wyse 60 is like the Wyse 50 but with more padding.
#	The reset strings are slow and the pad times very depending
#	on other parameters such as font loading.  I have tried
#	to follow the following outline:
#		rs1 -> set personality
#		rs2 -> set number of columns
#		rs3 -> set number of lines
#		is1 -> select the proper font
#		is2 -> do the initialization
#		is3 -> set up display memory (2 pages)
#
#	The Wyse 60's that have vt100 emulation are slower than the
#	older Wyse 60's.  This change happened mid-1987.
#	The capabilities affected are (dch1) (dl1) (il1) (ind) (ri)
#
#	It may be useful to assign two function keys with the
#	values  \E=(\s  look at old data in page 1
#	        \E=W,   look at bottem of page 1
#	Note:							###
#	   The Wyse 60 runs faster when the XON/XOFF		###
#	   handshake is turned off.				###
#
wr|wy60-25|wyse60-25|wyse 60 80-column 25-lines:\
	:is=\E`\072\Ee)\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:li#25:r3=200\EwG\Ee):\
	:tc=wy60:
w9|wy60w-25|wyse60w-25|wy60-25-w|wyse60-25-w|wyse 60 132-column 25-lines:\
	:is=\E`\073\Ee)\EO\Ee6\Ec41\E~4\Ec21:\
	:li#25:r3=200\EwG\Ee):\
	:tc=wy60w:
wv|wy60-42|wyse60-42|wyse 60 80-column 42-lines:\
	:is=\E`\072\Ee*\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:al=11\EE:cd=260\Ey:cl=260\E*:cm=2\E=%+ %+ :dc=16\EW:\
	:dl=11\ER:i1=\EcB2\EcC3:ip=5:li#42:r3=150\Ee*:sr=10\Ej:\
	:tc=wy60:
wx|wy60w-42|wyse60w-42|wy60-42-w|wyse60-42-w|wyse 60 132-column 42-lines:\
	:is=\E`\073\Ee*\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:cm=2\Ea%i%dR%dC:co#132:dc=19\EW:ho=2^^:ip=6:r2=300\EeF\E`;:\
	:tc=wy60-42:
wz|wy60-43|wyse60-43|wyse 60 80-column 43-lines:\
	:is=\E`\072\Ee+\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:li#43:r3=150\Ee+:\
	:tc=wy60-42:
W1|wy60w-43|wyse60w-43|wy60-43-w|wyse60-43-w|wyse 60 132-column 43-lines:\
	:is=\E`\073\Ee+\EO\Ee6\Ec41\E~4\Ec21\Ed/:\
	:li#43:r3=150\Ee+:\
	:tc=wy60-42-w:
W2|wy60-vb|wyse60-vb|Wyse 60 Visible bell:\
	:vb=\E`8\E`9:\
	:tc=wy60:
wf|wy60w-vb|wyse60w-vb|wy60-w-vb|wy60-wvb|wyse60-wvb|Wyse 60 132-column Visible bell:\
	:vb=\E`8\E`9:\
	:tc=wy60w:
-- 

Pete Gregory       |  Internet: pete@wvus.org
UNIX SA            |  Bangpath: ames!elroy!wvus!pete
World Vision U.S.  |  Slowpath: 919 W. Huntington Dr., Monrovia, CA 91016

Hide! Hide!  The cow's outside!!

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From gpstwr!merv Wed Apr  1 05:59:16 1992
Received: from relay.tek.com by merlin.resmel.bhp.com.au with SMTP id AA19183
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 05:58:40 +1100
Received: by relay.tek.com id <AA13120@relay.tek.com>; Tue, 31 Mar 92 10:55:28 -0800
Received: from gvgpsa.gvg.tek.com by tektronix.TEK.COM (4.1/8.0)
	id AA10391; Tue, 31 Mar 92 10:57:35 PST
Received: by gvgpsa.gvg.tek.com (5.57/smail2.5)
	id AA08367; Tue, 31 Mar 92 10:55:42 PST
Received: by gpstwr.UUCP (smail2.5)
	id AA08032; 31 Mar 92 10:56:39 PST (Tue)
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Date: 31 Mar 92 10:56:35 PST (Tue)
From: gpstwr!merv (Merv Graham)
Message-Id: <9203311056.AA08028@gpstwr.UUCP>
Status: OR

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin


Robin,

Here's one that works for us:

Modify to your heart's content.
-------------------------- 8< ---------------------------------
#
wy|wy60|wyse wy-60:\
 	:is=\EC\EDF\E\^1\EG0\E3\E`\072\Er\Ee"\
 	\Ed/\EH^C\Ed*\EX\Ee(\`\072\EwG:\
 	:if=/usr/lib/tabset/std:\
 	:al=\EE:bs:am:bt=\EI:cd=\Ey:ce=\Et:cl=\E*:\
 	:cm=\E=%+ %+ :co#80:dc=\EW:dl=\ER:do=^J:ct=\E0:st=\E1:\
 	:ei=\Er:ho=^^:im=\Eq:\
 	:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:\
 	:li#24:mi:nd=^L:nl=^J:pt:so=\EG4:se=\EG0:\
 	:sr=\Ej:st=\E1:ue=\EG0:ug#1:up=^K:us=\EG8:\
 	:ve=:vs=:te=:ti=:\
 	:vb=\E\^1\177\177\177\177\177\177\177\177\177\177\E\^0:\
 	:k0=^A@^M:k1=^AA^M:k2=^AB^M:k3=^AC^M:k4=^AD^M:\
 	:k5=^AE^M:k6=^AF^M:k7=^AG^M:k8=^AH^M:k9=^AI^M:
 
-------------------------- 8< ---------------------------------

>-- 
>Robin Brown, System administrator, BHP Research - Melbourne Laboratories
>245 Wellington Road Mulgrave VIC 3184 Australia
>E-mail: robin@resmel.bhp.com.au  ph: +61-3-560-7066  fax: +61-3-561-6709
---
Merv Graham                 |     gpstwr!merv@gvgpsa.gvg.tek.com
Graham-Patten Systems, Inc. | or: tektronix!gvgpsa.gvg.tek.com!gpstwr!merv
P.O. Box 1960               | 
Grass Valley, CA 95945      | Ph: 916-273-8412   FAX: 916-273-7458

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From sam@bsu-cs.bsu.edu Wed Apr  1 07:56:14 1992
Received: from BSU-CS.BSU.EDU by merlin.resmel.bhp.com.au with SMTP id AA22657
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 07:55:39 +1100
Received: by bsu-cs.bsu.edu (5.57/Ultrix3.0-C)
	id AA11598; Tue, 31 Mar 92 15:55:01 -0500
Date: Tue, 31 Mar 92 15:55:01 -0500
From: sam@bsu-cs.bsu.edu (B. Samuel Blanchard)
Message-Id: <9203312055.AA11598@bsu-cs.bsu.edu>
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
In-Reply-To: <1992Mar31.005748.3186@resmel.bhp.com.au>
Organization: Ontario Systems Corp. Muncie IN
Cc: 
Status: OR

Following is provided as is etc.  hope I didn't steal anything private.
I also have entries for Wyse60 in Televideo 925 mode and VT100 mode.
The VT100 mode may just be the same as vt100.

wy60|wyse60|wyse 60,
	am, hs, xon,
	cols#80, lines#24, wsl#78,
	bel=^G, blink=\EG2, cbt=\EI, clear=\E+, cr=\r,
	cub1=\b, cud1=\n, cuf1=\f, cup=\Ea%i%p1%dR%p2%dC,
	cuu1=^K, dch1=\EW, dim=\EGp, dl1=\ER, ed=\EY, el=\ET,
	fsl=\r, home=^^, ht=\Ei, ich1=\Eq,
	if=/usr/lib/tabset/std, il1=\EE, ind=\n,
	is2=\Ee.\E`:\Ee(\Ec21, kbs=\b, kcud1=\n, kcuf1=\f,
	kcuu1=^K, kf0=\EQ, kf1=^A@\r, kf10=^AI\r, kf11=^AJ\r,
	kf12=^AK\r, kf13=^AL\r, kf14=^AM\r, kf15=^AN\r,
	kf16=^AO\r, kf17=\EQ, kf18=\EW, kf19=\ET, kf2=^AA\r,
	kf20=\Er, kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	ll=\Ea24R1C, rev=\EG4, rmacs=\EH^C, rmir=\Er,
	rmso=\EG0, rmul=\EG0, sgr0=\EG0, smacs=\EH^B,
	smir=\Eq, smso=\EG4, smul=\EG8, tsl=\Ez(,
-- 
B. Sam Blanchard        sam@bsu-cs.bsu.edu
418 Winfield Dr         (317) 741-4500   work
Greenfield, IN 46140

From alanbe@qdpii.comp.qdpi.oz.au Wed Apr  1 09:52:31 1992
Received: from bunyip.cc.uq.oz.au by merlin.resmel.bhp.com.au with SMTP id AA26769
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 09:52:08 +1100
Received: from cc.uq.oz.au by bunyip.cc.uq.oz.au 
          id <15476-0@bunyip.cc.uq.oz.au>; Wed, 1 Apr 1992 08:50:45 +0000
Received: by qdpii.comp.qdpi.oz.au (5.61) id AA09471;
          Wed, 1 Apr 92 08:40:53 +1000
Date: Wed, 1 Apr 92 08:40:53 +1000
From: alanbe@qdpii.comp.qdpi.oz.au (Alan BESWICK)
Message-Id: <9203312240.AA09471@qdpii.comp.qdpi.oz.au>
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Sender: alanbe@qdpii.comp.qdpi.oz.au
Status: OR

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin

>-- 
>Robin Brown, System administrator, BHP Research - Melbourne Laboratories
>245 Wellington Road Mulgrave VIC 3184 Australia
>E-mail: robin@resmel.bhp.com.au  ph: +61-3-560-7066  fax: +61-3-561-6709

here are wyse50 and 50a if that is a help
cheers
Alan




Alan Beswick,				Snail Mail: Locked Mail Bag No. 4,
Argicultural Production IT Group,	Moorooka,   4105. Qld.
Department of Primary Industries.	ACSNet:	    alanbe@qdpii.comp.qdpi.oz.au
					phone:	    (07) 362 9570



wy|wyse:\
	:am:\
	:bl=^G:\
	:bt=\EI:\
	:co#80:\
	:li#24:\
	:cr=^M:\
	:nl=^J:\
	:bs:\
	:up=^K:\
	:nd=^L:\
	:kl=^H:\
	:kd=^J:\
	:ku=^K:\
	:kr=^L:\
	:cm=\E=%+ %+ :\
	:cl=\E+:\
	:ho=^^:\
	:ce=\ET:\
	:cd=\EY:\
	:al=\EE:\
	:dl=\ER:\
	:dl:\
	:da:\
	:db:\
	:so=\EG4:\
	:se=\EG0:\
	:sg#1:\
	:us=\EG8:\
	:ue=\EG0:\
	:ug#1:\
	:hs:\
	:ts=^[A14^[z(:\
	:fs=^M:\
	:ds=^[z(^M^[A10:
wy50|wyse50:\
        :al=\EE:\
	:am:\
	:bl=^G:\
	:bs:\
	:bt=\EI:\
	:ce=\ET:\
	:cd\EY:\
	:cl=\E+:\
	:cm=\E=%+ %+ :\
        :co#80:\
	:cr=^M:\
	:da:\
	:db:\
	:dc=\EW:\
	:dl=\ER:\
	:ei=\Er:\
	:ho=^^:\
	:im=\Eq:\
	:li#24:\
        :nd=^L:\
	:nl=^J:\
	:so=\EG4:\
	:se=\EG0:\
	:ue=\EG0:\
	:up=^K:\
	:us=\EG8:
#	entry assumes that the terminal has automatic margins.  This
#	translates to the AUTO NL "stub" being on.
wy50a|wyse50a:\
        :al=\EE:\
	:bl=^G:\
	:bs:\
	:bt=\EI:\
	:ce=\ET:\
	:cd\EY:\
	:cl=\E+:\
	:cm=\E=%+ %+ :\
        :co#80:\
	:cr=^M:\
	:da:\
	:db:\
	:dc=\EW:\
	:dl=\ER:\
	:ei=\Er:\
	:ho=^^:\
	:im=\Eq:\
	:li#24:\
        :nd=^L:\
	:nl=^J:\
	:so=\EG4:\
	:se=\EG0:\
	:ue=\EG0:\
	:up=^K:\
	:us=\EG8:

From baur@mdcbbs.com Wed Apr  1 10:42:44 1992
Received: from munnari.OZ.AU by merlin.resmel.bhp.com.au with SMTP id AA28556
  (5.65b/IDA-1.4.3 for robin); Wed, 1 Apr 92 10:41:56 +1100
Received: from uunet by munnari.oz.au with UUCP (5.64+1.3.1+0.50)
	id AA02169; Wed, 1 Apr 1992 09:41:20 +1000 (from baur@MDCBBS.COM)
Received: from uunet.uu.net (via LOCALHOST.UU.NET) by relay2.UU.NET with SMTP 
	(5.61/UUNET-internet-primary) id AA25383; Tue, 31 Mar 92 17:27:17 -0500
Received: from mdcbbs.UUCP by uunet.uu.net with UUCP/RMAIL
	(queueing-rmail) id 172654.6965; Tue, 31 Mar 1992 17:26:54 EST
Received: by MDCBBS.COM with UUCP/PMDF (DECUS UUCP);
          Tue, 31 Mar 1992 14:10 PDT
Received: from gfxhpp4 by MDCBBS.COM (PMDF #12239) id
 <01GIAPAH8TVK003GOU@MDCBBS.COM>; Tue, 31 Mar 1992 14:10 PDT
Received: by gfxhpp4 (16.8/16.2) id AA15830; Tue, 31 Mar 92 14:14:45 -0800
Date: Tue, 31 Mar 92 14:14:45 -0800
From: Steve Baur <baur@mdcbbs.com>
Subject: Looking for wyse60 termcap entry
In-Reply-To: robin@resmel.bhp.com.au's message of 31 Mar 92 00:57:48 GMT
To: robin@resmel.bhp.com.au (Robin Brown)
Message-Id: <01GIAPAH8TVK003GOU@MDCBBS.COM>
X-Envelope-To: uunet!munnari!resmel.bhp.com.au!robin
Status: OR

I am sending you both termcap and terminfo entries.

Terminfo:
------------------ Cut Here --------------------------
60|wy60|wyse60|wy99gt|wyse99gt|Wyse 60 and Wyse 99GT,
	bw, am, km, hs, mir, msgr,
	cols#80, lines#24, wsl#45, nlab#8, lh#1, lw#8,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<100>, el=\Et, ed=\Ey$<100>, cup=\E=%p1%' '%+%c%p2%' '%+%c,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<10>, dl1=\ER$<5>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB0\EcC1, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<4>, ip=$<3>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<3>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>, rs3=\EwG\Ee($<150>,
	ind=\n$<5>, ri=\Ej$<7>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, pln=\Ez%p1%'/'%+%c%p2%s\r,
	smln=\EA10, rmln=\EA11, kf11=^AJ\r, kf12=^AK\r,
	kf13=^AL\r, kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
	
wy60-25|wyse60-25|wyse 60 80-column 25-lines,
	bw, am, km, hs, mir, msgr,
	cols#80, lines#25, wsl#45,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<100>, el=\Et, ed=\Ey$<100>, cup=\E=%p1%' '%+%c%p2%' '%+%c,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<10>, dl1=\ER$<5>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB0\EcC1, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<4>, ip=$<3>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<3>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>, rs3=\EwG\Ee)$<150>,
	ind=\n$<5>, ri=\Ej$<7>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, smln=\EA10,
	rmln=\EA11, kf11=^AJ\r, kf12=^AK\r, kf13=^AL\r,
	kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
wy60-25-w|wyse60-25-w|wyse 60 132-column 25-lines,
	bw, am, km, hs, mir, msgr,
	cols#132, lines#25, wsl#97,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<100>, el=\Et, ed=\Ey$<100>, cup=\Ea%i%p1%dR%p2%dC,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<16>, dl1=\ER$<5>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB0\EcC1, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<4>, ip=$<5>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<3>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>\E`;$<150>, rs3=\EwG\Ee)$<150>,
	ind=\n$<5>, ri=\Ej$<7>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, smln=\EA10,
	rmln=\EA11, kf11=^AJ\r, kf12=^AK\r, kf13=^AL\r,
	kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
wy60-42|wyse60-42|wyse 60 80-column 42-lines,
	bw, am, km, hs, mir, msgr,
	cols#80, lines#42, wsl#45, nlab#8, lh#1, lw#8,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<260>, el=\Et, ed=\Ey$<260>, cup=\E=%p1%' '%+%c%p2%' '%+%c$<2>,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<16>, dl1=\ER$<11>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB2\EcC3, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<11>, ip=$<5>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<6>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>, rs3=\Ee*$<150>,
	ind=\n$<9>, ri=\Ej$<10>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, pln=\Ez%p1%'/'%+%c%p2%s\r,
	smln=\EA10, rmln=\EA11, kf11=^AJ\r, kf12=^AK\r,
	kf13=^AL\r, kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
	
wy60-42-w|wyse60-42-w|wyse 60 132-column 42-lines,
	bw, am, km, hs, mir, msgr,
	cols#132, lines#42, wsl#97, nlab#16, lh#1, lw#7,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<260>, el=\Et, ed=\Ey$<260>, cup=\Ea%i%p1%dR%p2%dC$<2>,
	cud1=\n, home=^^$<2>, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<19>, dl1=\ER$<11>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB2\EcC3, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<11>, ip=$<6>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<11>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>\E`;$<150>, rs3=\Ee*$<150>,
	ind=\n$<9>, ri=\Ej$<10>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, pln=\Ez%p1%'/'%+%c%p2%s\r,
	smln=\EA10, rmln=\EA11, kf11=^AJ\r, kf12=^AK\r,
	kf13=^AL\r, kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
	
wy60-43|wyse60-43|wyse 60 80-column 43-lines,
	bw, am, km, hs, mir, msgr,
	cols#80, lines#43, wsl#45,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<260>, el=\Et, ed=\Ey$<260>, cup=\E=%p1%' '%+%c%p2%' '%+%c$<2>,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<16>, dl1=\ER$<11>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB2\EcC3, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<11>, ip=$<5>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<6>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>, rs3=\Ee+$<150>,
	ind=\n$<9>, ri=\Ej$<10>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, smln=\EA10,
	rmln=\EA11, kf11=^AJ\r, kf12=^AK\r, kf13=^AL\r,
	kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
wy60-43-w|wyse60-43-w|wyse 60 132-column 43-lines,
	bw, am, km, hs, mir, msgr,
	cols#132, lines#43, wsl#97,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<260>, el=\Et, ed=\Ey$<260>, cup=\Ea%i%p1%dR%p2%dC$<2>,
	cud1=\n, home=^^$<2>, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<19>, dl1=\ER$<11>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB2\EcC3, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<11>, ip=$<6>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<11>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>\E`;$<150>, rs3=\Ee+$<150>,
	ind=\n$<9>, ri=\Ej$<10>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, smln=\EA10,
	rmln=\EA11, kf11=^AJ\r, kf12=^AK\r, kf13=^AL\r,
	kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
wy60-vb|wyse60-vb|wy99gt-vb|wyse99gt-vb|Wyse 60 and 99GT Visable bell,
	bw, am, km, hs, mir, msgr,
	cols#80, lines#24, wsl#45, nlab#8, lh#1, lw#8,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<100>, el=\Et, ed=\Ey$<100>, cup=\E=%p1%' '%+%c%p2%' '%+%c,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<10>, dl1=\ER$<5>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, flash=\E`8$<100/>\E`9, fsl=\r, is1=\EcB0\EcC1,
	is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T, is3=^N^T, il1=\EE$<4>, ip=$<3>,
	kbs=\b, kdch1=\EW, kdl1=\ER, kcud1=\n,
	kel=\ET, ked=\EY, kf1=^A@\r, kf10=^AI\r,
	kf2=^AA\r, kf3=^AB\r, kf4=^AC\r, kf5=^AD\r,
	kf6=^AE\r, kf7=^AF\r, kf8=^AG\r, kf9=^AH\r,
	khome=^^, kich1=\EQ, kil1=\EE, kcub1=\b,
	knp=\EK, kpp=\EJ, kcuf1=\f, kcuu1=^K,
	nel=\r\n$<3>, pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP,
	mc4=^T, mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>,
	rs3=\EwG\Ee($<150>, ind=\n$<5>, ri=\Ej$<7>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c,
	hts=\E1, ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0,
	pln=\Ez%p1%'/'%+%c%p2%s\r, smln=\EA10, rmln=\EA11, kf11=^AJ\r,
	kf12=^AK\r, kf13=^AL\r, kf14=^AM\r, kf15=^AN\r,
	kf16=^AO\r,
wy60-w|wyse60-w|wy99gt-w|wyse99gt-w|wyse 60/99gt 132-column,
	bw, am, km, hs, mir, msgr,
	cols#132, lines#24, wsl#97, nlab#16, lh#1, lw#7,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<100>, el=\Et, ed=\Ey$<100>, cup=\Ea%i%p1%dR%p2%dC,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<16>, dl1=\ER$<5>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, fsl=\r, is1=\EcB0\EcC1, is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T,
	is3=^N^T, il1=\EE$<4>, ip=$<5>, kbs=\b,
	kdch1=\EW, kdl1=\ER, kcud1=\n, kel=\ET,
	ked=\EY, kf1=^A@\r, kf10=^AI\r, kf2=^AA\r,
	kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^,
	kich1=\EQ, kil1=\EE, kcub1=\b, knp=\EK,
	kpp=\EJ, kcuf1=\f, kcuu1=^K, nel=\r\n$<3>,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP, mc4=^T,
	mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>\E`;$<150>, rs3=\EwG\Ee($<150>,
	ind=\n$<5>, ri=\Ej$<7>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c, hts=\E1,
	ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0, pln=\Ez%p1%'/'%+%c%p2%s\r,
	smln=\EA10, rmln=\EA11, kf11=^AJ\r, kf12=^AK\r,
	kf13=^AL\r, kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
	
wy60-w-vb|wy60-wvb|wyse60-wvb|wy99gt-wvb|wyse99gt-wvb|Wyse 60 and 99GT 132-column Visable bell,
	bw, am, km, hs, mir, msgr,
	cols#132, lines#24, wsl#97, nlab#16, lh#1, lw#7,
	cbt=\EI, bel=^G, cr=\r, tbc=\E0,
	clear=\E*$<100>, el=\Et, ed=\Ey$<100>, cup=\Ea%i%p1%dR%p2%dC,
	cud1=\n, home=^^, civis=\E`0, cub1=\b,
	cnorm=\E`1, cuf1=\f, ll=^^^K, cuu1=^K,
	dch1=\EW$<16>, dl1=\ER$<5>, dsl=\EF\r, smacs=\EH^B,
	blink=\EG2, dim=\EGp, smir=\Eq, invis=\EG1,
	prot=\E), rev=\EG4, smso=\EGt, smul=\EG8,
	rmacs=\EH^C, sgr0=\E(\EH^C\EG0, rmir=\Er, rmso=\EG0,
	rmul=\EG0, flash=\E`8$<100/>\E`9, fsl=\r, is1=\EcB0\EcC1,
	is2=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T, is3=^N^T, il1=\EE$<4>, ip=$<5>,
	kbs=\b, kdch1=\EW, kdl1=\ER, kcud1=\n,
	kel=\ET, ked=\EY, kf1=^A@\r, kf10=^AI\r,
	kf2=^AA\r, kf3=^AB\r, kf4=^AC\r, kf5=^AD\r,
	kf6=^AE\r, kf7=^AF\r, kf8=^AG\r, kf9=^AH\r,
	khome=^^, kich1=\EQ, kil1=\EE, kcub1=\b,
	knp=\EK, kpp=\EJ, kcuf1=\f, kcuu1=^K,
	nel=\r\n$<3>, pfloc=\EZ2%p1%'?'%+%c%p2%s\177, pfx=\EZ1%p1%'?'%+%c%p2%s\177, mc0=\EP,
	mc4=^T, mc5=^R, rs1=\E~!\E~4$<150>, rs2=\EeF$<150>\E`;$<150>,
	rs3=\EwG\Ee($<150>, ind=\n$<5>, ri=\Ej$<7>, sgr=%?%p8%t\E)%e\E(%;%?%p9%t\EH^B%e\EH^C%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c,
	hts=\E1, ht=\t$<1>, tsl=\EF, uc=\EG8%p1%c\EG0,
	pln=\Ez%p1%'/'%+%c%p2%s\r, smln=\EA10, rmln=\EA11, kf11=^AJ\r,
	kf12=^AK\r, kf13=^AL\r, kf14=^AM\r, kf15=^AN\r,
	kf16=^AO\r,
------------------ Cut Here --------------------------

Termcap:
------------------ Cut Here --------------------------
60|wy60|wyse60|wy99gt|wyse99gt|Wyse 60 and Wyse 99GT:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#80:li#24:kn#8:\
	:ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
	:cl=100\E*:cm=\E=%+ %+ :ct=\E0:dc=10\EW:dl=5\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
	:ip=3:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=150\EeF:r3=150\EwG\Ee(:se=\EG0:so=\EGt:sr=7\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-25-w|wyse60-25-w|wyse 60 132-column 25-lines:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#132:li#25:kn#8:\
	:ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
	:cl=100\E*:cm=\Ea%i%dR%dC:ct=\E0:dc=16\EW:dl=5\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
	:ip=5:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=300\EeF\E`;:r3=150\EwG\Ee):se=\EG0:so=\EGt:\
	:sr=7\Ej:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:\
	:us=\EG8:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-42-w|wyse60-42-w|wyse 60 132-column 42-lines:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#132:li#42:kn#8:\
	:ae=\EH^C:al=11\EE:as=\EH^B:bt=\EI:cd=260\Ey:ce=\Et:\
	:cl=260\E*:cm=2\Ea%i%dR%dC:ct=\E0:dc=19\EW:dl=11\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=2^^:i1=\EcB2\EcC3:im=\Eq:\
	:ip=6:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=300\EeF\E`;:r3=150\Ee*:se=\EG0:so=\EGt:sr=10\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-43-w|wyse60-43-w|wyse 60 132-column 43-lines:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#132:li#43:kn#8:\
	:ae=\EH^C:al=11\EE:as=\EH^B:bt=\EI:cd=260\Ey:ce=\Et:\
	:cl=260\E*:cm=2\Ea%i%dR%dC:ct=\E0:dc=19\EW:dl=11\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=2^^:i1=\EcB2\EcC3:im=\Eq:\
	:ip=6:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=300\EeF\E`;:r3=150\Ee+:se=\EG0:so=\EGt:sr=10\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-w|wyse60-w|wy99gt-w|wyse99gt-w|wyse 60/99gt 132-column:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#132:li#24:kn#8:\
	:ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
	:cl=100\E*:cm=\Ea%i%dR%dC:ct=\E0:dc=16\EW:dl=5\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
	:ip=5:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=300\EeF\E`;:r3=150\EwG\Ee(:se=\EG0:so=\EGt:\
	:sr=7\Ej:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:\
	:us=\EG8:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-25|wyse60-25|wyse 60 80-column 25-lines:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#80:li#25:kn#8:\
	:ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
	:cl=100\E*:cm=\E=%+ %+ :ct=\E0:dc=10\EW:dl=5\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
	:ip=3:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=150\EeF:r3=150\EwG\Ee):se=\EG0:so=\EGt:sr=7\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-42|wyse60-42|wyse 60 80-column 42-lines:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#80:li#42:kn#8:\
	:ae=\EH^C:al=11\EE:as=\EH^B:bt=\EI:cd=260\Ey:ce=\Et:\
	:cl=260\E*:cm=2\E=%+ %+ :ct=\E0:dc=16\EW:dl=11\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB2\EcC3:im=\Eq:\
	:ip=5:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=150\EeF:r3=150\Ee*:se=\EG0:so=\EGt:sr=10\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-43|wyse60-43|wyse 60 80-column 43-lines:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#80:li#43:kn#8:\
	:ae=\EH^C:al=11\EE:as=\EH^B:bt=\EI:cd=260\Ey:ce=\Et:\
	:cl=260\E*:cm=2\E=%+ %+ :ct=\E0:dc=16\EW:dl=11\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB2\EcC3:im=\Eq:\
	:ip=5:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=150\EeF:r3=150\Ee+:se=\EG0:so=\EGt:sr=10\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:ko=le,do,nd,up,dc,dl,ho,al:
wy60-vb|wyse60-vb|wy99gt-vb|wyse99gt-vb|Wyse 60 and 99GT Visable bell:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#80:li#24:kn#8:\
	:ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
	:cl=100\E*:cm=\E=%+ %+ :ct=\E0:dc=10\EW:dl=5\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
	:ip=3:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=150\EeF:r3=150\EwG\Ee(:se=\EG0:so=\EGt:sr=7\Ej:\
	:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:us=\EG8:\
	:vb=100\E`8\E`9:ve=\E`1:vi=\E`0:\
	:ko=le,do,nd,up,dc,dl,ho,al:
wy60-w-vb|wy60-wvb|wyse60-wvb|wy99gt-wvb|wyse99gt-wvb|Wyse 60 and 99GT 132-column Visable bell:\
	:am:bw:hs:km:mi:ms:bs:pt:\
	:co#132:li#24:kn#8:\
	:ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
	:cl=100\E*:cm=\Ea%i%dR%dC:ct=\E0:dc=16\EW:dl=5\ER:\
	:ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
	:ip=5:\
	:is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
	:kh=^^:kl=\b:kr=\f:ku=^K:nd=\f:r1=150\E~!\E~4:\
	:r2=300\EeF\E`;:r3=150\EwG\Ee(:se=\EG0:so=\EGt:\
	:sr=7\Ej:st=\E1:ts=\EF:uc=\EG8%.\EG0:ue=\EG0:up=^K:\
	:us=\EG8:vb=100\E`8\E`9:ve=\E`1:vi=\E`0:\
	:ko=le,do,nd,up,dc,dl,ho,al:
------------------ Cut Here --------------------------

--
- Steve Baur@mdcbbs.com  (221/611 3/17/92)

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From uucp@quick.com Sun Apr  5 09:54:23 1992
Received: from sumax.seattleu.edu by merlin.resmel.bhp.com.au with SMTP id AA14371
  (5.65b/IDA-1.4.3 for robin); Sun, 5 Apr 92 09:53:57 +1100
Received: by sumax.seattleu.edu id AA16280
  (5.65a/IDA-1.4.2 for robin@resmel.bhp.com.au); Sat, 4 Apr 92 14:55:46 -0800
Received: from host.UUCP by quick (4.1/1.15) with UUCP 
	id AA14588; Sat, 4 Apr 92 14:41:06 PST
Received: by Eskimo North Public Access Unix (206) For-Ever  (206) 367-3837
	id AA14799; 4 Apr 92 11:24:14 PST (Sat)
Received: by sea375.uucp (/\==/\ Smail3.1.22.1 #22.3)
	id <m0lXFq8-00003nC@sea375.uucp>; Sat, 4 Apr 92 10:51 PST
Message-Id: <m0lXFq8-00003nC@sea375.uucp>
Date: Sat, 4 Apr 92 10:51 PST
From: sea375!dave@quick.com (David A. Wilson)
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Status: O

robin@resmel.bhp.com.au (Robin Brown):
> Hi,
> The subject says it all, I'm looking for one - can anyone help, it would
> make my life so much easier.
> Thanks in advance,
> Robin
> 
> -- 
# ===== WYSE 60 ======
# all wyse 60 entries DO NOT change the personality mode in init string
# 'status line' means the terminal local status line
#
# the function key setups seem to have problems .....
# :vs=100\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1*\E[H\177:\
# :ve=100\EZ0+^K\177\EZ0,^J\177\EZ0-^H\177\EZ0.^L\177\EZ0*^^\177:\
# :ku=\E[A:kd=\E[B:kr=\E[C:kl=\E[D:kh=\E[H:k0=\EQ:k1=\EW:k2=\ET:\
# :k3=\Er:k4=\EE:k5=\ER:k6=\EY:k7=\Eq:k8=\EK:k9=\EJ:\
#
w6|wy60|wy60-43|Wyse 60 w/ 80 cols x 43 lines:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee+:\
	:if=/usr/lib/tabset/wy60.80:\
	:al=\EE:am:bs:bt=\EI:pt:ct=\E0:st=\E1:ce=\ET:cm=\Ea%i%dR%dC:\
	:cl=150\E*:cd=150\EY:co#80:dc=\EW:dl=\ER:ei=\Er:ho=\E{:\
	:LC:im=\Eq:li#43:mi:mb=\EG2:md=\EG4:mh=\EGp:mr=\EG4:me=\EG0:\
	:so=\EG4:se=\EG0:us=\EG8:ue=\EG0:nd=^L:up=^K:\
	:hs:ts=\EF:fs=\r:ds=\EF\r:
wa|wy60-w|wy60-43-w|Wyse 60 w/ 132 cols x 43 lines:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee+:\
	:co#132:li#43:tc=wy60-43:
ws|wy60-42|Wyse 60 w/ 80 cols x 42 lines + status line:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee*:\
	:li#42:i2=\Ez\177\EA1t\Ez(\r:\
	:hs:ts=\Ez(:fs=\r:ds=\EA10\Ez(\r:tc=wy60:
wd|wy60-42-w|Wyse 60 w/ 132 cols x 42 lines + status line:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee*:\
	:co#132:tc=wy60-42:
wa|wy60-25|Wyse 60 w/ 80 cols x 25 lines:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee):\
	:li#25:tc=wy60:
wa|wy60-25-w|Wyse 60 w/ 132 cols x 25 lines:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee):\
	:co#132:li#25:tc=wy60:
wb|wy60-24|wyse60|Wyse 60 w/ 80 cols x 24 lines + status line:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee(:\
	:li#24:tc=wy60-42:
wc|wy60-24-w|wyse60w|Wyse 60 w/132 cols x 24 lines + status line:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee(:\
	:co#132:tc=wy60-24:
#
# Reverse video versions of Wyse 60
#
wr|wy60-rv|wy60-43-rv|Wyse 60 w/ 80 cols x 43 lines:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee+\EA04\EA14\EA2|\EA3|:\
	:li#43:tc=wy60:
wa|wy60-w-rv|wy60-43-w-rv|Wyse 60 w/ 132 cols x 43 lines:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee+\EA04\EA14\EA2|\EA3|:\
	:co#132:tc=wy60-43-rv:
ws|wy60-42-rv|Wyse 60 w/ 80 cols x 42 lines + status line:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee*\EA04\EA14\EA2|\EA3|:\
	:i2=\Ez\177\EA1t\Ez(\r:hs:ts=\Ez(:fs=\r:ds=\EA14\Ez(\r:tc=wy60-42:
wd|wy60-42-w-rv|Wyse 60 w/ 132 cols x 42 lines + status line:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee*\EA04\EA14\EA2|\EA3|:\
	:co#132:tc=wy60-42-rv:
wa|wy60-25-rv|Wyse 60 w/ 80 cols x 25 lines:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee)\EA04\EA14\EA2|\EA3|:\
	:li#25:tc=wy60-43-rv:
wa|wy60-25-w-rv|Wyse 60 w/ 132 cols x 25 lines:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee)\EA04\EA14\EA2|\EA3|:\
	:co#132:li#25:tc=wy60-43-rv:
wb|wy60-24-rv|wyse60rv|Wyse 60 w/ 80 cols x 24 lines + status line:\
	:is=\Ee6\Ee1\Ec21\E`\072\Ee(\EA04\EA14\EA2|\EA3|:\
	:li#24:tc=wy60-42-rv:
wc|wy60-24-w-rv|wyse60w-rv|Wyse 60 w/132 cols x 24 lines + status line:\
	:if=/usr/lib/tabset/wy60.132:\
	:is=\Ee6\Ee1\Ec21\E`;\Ee(\EA04\EA14\EA2|\EA3|:\
	:co#132:li#24:tc=wy60-42-rv:
#

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From chinacat!chip@cs.utexas.edu Fri Apr  3 19:19:16 1992
Received: from cs.utexas.edu by merlin.resmel.bhp.com.au with SMTP id AA20483
  (5.65b/IDA-1.4.3 for robin); Fri, 3 Apr 92 19:18:36 +1100
Received: from chinacat by cs.utexas.edu (5.64/1.122) with UUCP
	id AA28477; Fri, 3 Apr 92 01:42:45 -0600
Received: by chinacat.unicom.com (3.1.25.1) 
	id <m0lWiam-0000tbC@chinacat.unicom.com>; Fri, 3 Apr 92 01:21 CST
Message-Id: <m0lWiam-0000tbC@chinacat.unicom.com>
Date: Fri, 3 Apr 92 01:21 CST
From: chip@chinacat.unicom.com (Chip Rosenthal)
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
In-Reply-To: <1992Mar31.005748.3186@resmel.bhp.com.au>
Organization: Unicom Systems Development, Austin, TX
Status: O

In article <1992Mar31.005748.3186@resmel.bhp.com.au> you write:
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.

I use the following.

w7|wy60|wyse60|Wyse WY-60:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\177\EZ1,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177\Ec72:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:

#
w7|wy60-25|wyse60-25|Wyse WY-60 25 line:\
	:is=\E`\072\Ee)\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\177\EZ1,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177\Ec72:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#25:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
WA|wy60ak|wyse60ak|Wyse 60 with ANSI arrow keys:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177\Ec72:\
	:ti=\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:EN=\E[F:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kh=^~:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
WA|wy60ak-25|wyse60ak-25|Wyse 60 25 line with ANSI arrow keys:\
	:is=\E`\072\Ee)\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177\Ec72:\
	:ti=\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:EN=\E[F:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kh=^~:\
	:li#25:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#

-- 
Chip Rosenthal   <chip@chinacat.Unicom.COM> | My mind's got a mind of its own.
Unicom Systems Development     512-482-8260 |   -Butch Hancock

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From oli@odbffm.in.sub.org Fri Apr  3 18:03:57 1992
Received: from iraun1.ira.uka.de by merlin.resmel.bhp.com.au with SMTP id AA18018
  (5.65b/IDA-1.4.3 for robin); Fri, 3 Apr 92 18:02:38 +1100
Received: from ira.uka.de by iraun1.ira.uka.de with SMTP (PP) 
          id <15690-58@iraun1.ira.uka.de>; Fri, 3 Apr 1992 08:58:12 +0000
Received: from smurf.sub.org by iraun1.ira.uka.de id aa02708;
          2 Apr 92 20:43 MET DST
Received: from public.sub.org by smurf.sub.org with SMTP id <48141>;
          Thu, 2 Apr 1992 09:32:32 +0200
Received: by public.sub.org (/\@@/\ Smail3.1.20.1 #20.54) 
          id <m0lWLLS-0003VpC@public.sub.org>; Thu, 2 Apr 92 08:32 CEST
Received: by incom.incom.de (/\==/\ Smail3.1.25.1 #25.2) 
          id <m0lWKSz-0001zIC@incom.incom.de>; Thu, 2 Apr 92 07:36 EET
Received: by odbffm.in.sub.org (/\==/\ Smail3.1.22.1 #22.2) 
          id <m0lWL7j-0006OnC@odbffm.in.sub.org>; Thu, 2 Apr 92 07:18 MET
Message-Id: <m0lWL7j-0006OnC@odbffm.in.sub.org>
Date: Thu, 2 Apr 1992 08:18:00 +0200
From: Oliver Boehmer <oli@odbffm.in.sub.org>
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Status: O

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin

Well, here you go. This entry is used on an ALTOS 2000 running System V r3.2.
I think it still needs a little tuning (highlighting-inverse-stuff), but I
don't have time to do it.
I'm using the wy60 all the time..

oli

termcap:

w6|wyse6|wyse60|wy60|Wyse wy-60 with 80 column/25 line screen in wy-60 mode:\
	:am:hs:mi:xo:bs:pt:\
	:co#80:li#25:kn#8:\
	:F1=^AK\r:F2=^AL\r:F3=^AM\r:F4=^AN\r:F5=^AO\r:\
	:F6=^A`\r:F7=^Aa\r:F8=^Ab\r:F9=^Ac\r:FA=^Ad\r:\
	:FB=^Ae\r:FC=^Af\r:FD=^Ag\r:FE=^Ah\r:FF=^Ai\r:\
	:FG=^Aj\r:FH=^Ak\r:FI=^Al\r:FJ=^Am\r:FK=^An\r:\
	:FL=^Ao\r:ac=w0m1l2k3t4j5x607n8u9q\072a;v=:ae=\EcD:\
	:al=\EE:as=\EcE:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=\E+^^:\
	:cm=\E=%+ %+ :cr=\r:dc=\EW:dl=\ER:do=\n:ei=\Er:ho=^^:\
	:if=/usr/lib/tabset/alt7:im=\Eq:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Eu\E~2:k0=^A@\r:\
	:k1=^AA\r:k2=^AB\r:k3=^AC\r:k4=^AD\r:k5=^AE\r:\
	:k6=^AF\r:k7=^AG\r:k8=^AH\r:k9=^AI\r:k;=^AJ\r:kA=\EE:\
	:kD=\EW:kL=\ER:kN=\EK:kP=\EJ:kb=\b:kd=\n:kh=^^:kl=\b:\
	:kr=\f:ku=^K:le=\b:mb=\EG2:me=\EG0\EH^C:mh=\EGp:\
	:mk=\EG1:mr=\EG4:nd=\f:pf=^T\E~ :po=\E~!\Ed#:ps=\E[0i:\
	:.sa=!!! MUST CHANGE BY HAND !!!\EG%?%p2%p3%p6%O%A%p4%A%p5%A%t~%e%p2%p3%A%p4%A%t>%e%p2%p4%A%p6%A%t~%e%p3%p6%O%p4%A%p5%A%tv%e%p3%p4%A%t6%e%p4%p6%A%tv%e%p2%p4%A%p5%A%tz%e%p2%p3%p6%O%Ainfocmp: WARNING: termcap entry is too long!
%p5%A%t|%e%p2%p5%A%tx%e%p3%p6%O%p5%A%tt%e%p4%p5%A%tr%e%p1%t4%e%p2%p4%A%t\072%e%p2%p3%A%t<%e%p2%p6%A%t|%e%p2%t8%e%p3%t4%e%p4%t2%e%p5%tp%e%p6%tt%e%p7%t1%e0%;%?%p9%t\EH^B%e\EH^C%;:\
	:se=\EG0:sf=\n:so=\EG4:sr=\Ej:ta=\t:ue=\EG0:up=^K:\
	:us=\EG8:ko=le,do,nd,up,dc,dl,ho,al:


And terminfo:

w6|wyse6|wyse60|wy60|Wyse wy-60 with 80 column/25 line screen in wy-60 mode,
	am, hs, mir, xon,
	cols#80, lines#25,
	acsc=w0m1l2k3t4j5x607n8u9q:a;v=, bel=^G, blink=\EG2,
	cbt=\EI, clear=\E+^^, cr=\r, cub1=\b, cud1=\n,
	cuf1=\f, cup=\E=%p1%'\s'%+%c%p2%'\s'%+%c, cuu1=^K,
	dch1=\EW, dim=\EGp, dl1=\ER, ed=\EY, el=\ET, home=^^,
	ht=\t, if=/usr/lib/tabset/alt7, il1=\EE, ind=\n,
	invis=\EG1, is2=\E`:\Ee(\EO\Ee6\Ec41\E~4\Ec21\Eu\E~2,
	kbs=\b, kcub1=\b, kcud1=\n, kcuf1=\f, kcuu1=^K,
	kdch1=\EW, kdl1=\ER, kf0=^A@\r, kf1=^AA\r, kf10=^AJ\r,
	kf11=^AK\r, kf12=^AL\r, kf13=^AM\r, kf14=^AN\r,
	kf15=^AO\r, kf16=^A`\r, kf17=^Aa\r, kf18=^Ab\r,
	kf19=^Ac\r, kf2=^AB\r, kf20=^Ad\r, kf21=^Ae\r,
	kf22=^Af\r, kf23=^Ag\r, kf24=^Ah\r, kf25=^Ai\r,
	kf26=^Aj\r, kf27=^Ak\r, kf28=^Al\r, kf29=^Am\r,
	kf3=^AC\r, kf30=^An\r, kf31=^Ao\r, kf4=^AD\r,
	kf5=^AE\r, kf6=^AF\r, kf7=^AG\r, kf8=^AH\r, kf9=^AI\r,
	khome=^^, kil1=\EE, knp=\EK, kpp=\EJ, mc0=\E[0i,
	mc4=^T\E~\s, mc5=\E~!\Ed#, rev=\EG4, ri=\Ej,
	rmacs=\EcD, rmir=\Er, rmso=\EG0, rmul=\EG0,
	sgr=\EG%?%p2%p3%p6%O%A%p4%A%p5%A%t~%e%p2%p3%A%p4%A%t>%e%p2%p4%A%p6%A%t~%e%p3%p6%O%p4%A%p5%A%tv%e%p3%p4%A%t6%e%p4%p6%A%tv%e%p2%p4%A%p5%A%tz%e%p2%p3%p6%O%A%p5%A%t|%e%p2%p5%A%tx%e%p3%p6%O%p5%A%tt%e%p4%p5%A%tr%e%p1%t4%e%p2%p4%A%t:%e%p2%p3%A%t<%e%p2%p6%A%t|%e
%p2%t8%e%p3%t4%e%p4%t2%e%p5%tp%e%p6%tt%e%p7%t1%e0%;%?%p9%t\EH^B%e\EH^C%;,
	sgr0=\EG0\EH^C, smacs=\EcE, smir=\Eq, smso=\EG4,
	smul=\EG8,
-- 
Oliver Boehmer,  W-6000 Frankfurt 80 - Germany         oli@odbffm.in.sub.org

If God is perfect, why did He create discontinous functions?

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -


From fuat@ans.net Thu Apr  2 13:12:39 1992
Received: from interlock.ans.net by merlin.resmel.bhp.com.au with SMTP id AA16971
  (5.65b/IDA-1.4.3 for robin); Thu, 2 Apr 92 13:12:19 +1100
Received: by interlock.ans.net id AA16513
  (InterLock SMTP Gateway 1.02 for robin@resmel.bhp.com.au);
  Wed, 1 Apr 1992 21:11:38 -0500
Received: by interlock.ans.net (Internal Mail Agent-2);
  Wed, 1 Apr 1992 21:11:38 -0500
Received: by interlock.ans.net (Internal Mail Agent-1);
  Wed, 1 Apr 1992 21:11:38 -0500
Date: Thu, 2 Apr 1992 02:11:36 GMT
From: "Fuat C. Baran" <fuat@ans.net>
Message-Id: <199204020211.AA36261@foo.ans.net>
To: robin@resmel.bhp.com.au
Cc: fuat@ans.net
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
In-Reply-To: <1992Mar31.005748.3186@resmel.bhp.com.au>
Organization: Advanced Network & Services, Inc.
Status: O

In article <1992Mar31.005748.3186@resmel.bhp.com.au> you write:
>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.

Try this:

w6|wy60|wyse60|wyse 60 doing it like a wyse 60:\
        :al=\EE:am:bs:bt=\EI:bw:cd=\EY:ce=\ET:cf=^Z:cl=\E*:\
        :cm=\Ea%i%dR%dC:co#80:da:db:dc=\EW:dl=\ER:do=^J:ei=\Er:eo:et=\r:\
        :ge=\EH1:gf=\EH2:gg=\EH3:gh=\EH5:gi=\EH8:gj=\EH6:gk=\EH\072:gl=\EH9:\
        :gm=\EH4:gn=\EH0:go=\EH=:gs=^B:gx=^C:ho=^^:\
        :if=/usr/lib/tabset/stdcrt:im=\Eq:\
        :is=\Ee(\EG0\EC\EX\E0\Er\E\E072\E(\E":\
        :kb=^H:kd=^J:kf=\EK:kg=\EJ:kh=^^:ki=\EE:kj=\ER:kl=^H:kn#10:\
        :kr=^L:ku=^K:ko=cd,ce,dc,al,dl,ei,im,ta:\
        :k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
        :k8=^AG\r:k9=^AH\r:k0=^AI\r:li#24:ll=\Ea24R1C:\
        :l0=F10:l1=F1:l2=F2:l3=F3:l4=F4:l5=F5:l6=F6:l7=F7:l8=F8:l9=F9:\
        :mi:nd=^L:nm=\EG0:pe=\E':ps=\E&:pt:re=\EG0:\
        :rl=\EGt:ru=\EGx:rv=\EG<:rw=\EG|:se=\EG0:so=\EG4:sr=\Ej:ue=\EG0:\
        :up=^K:us=\EG8:ws=\E):we=\E(:\
        :vb=\EA04\200\200\200\200\200\200\200\200\200\200\200\200\EA00:

Hope this helps.  I don't use a Wyse60 so I don't know how good this
is.

						--Fuat

-- 
Advanced Network & Services, Inc.		fuat@ans.net
100 Clearbrook Road				914-789-5328
Elmsford, NY 10523				914-789-5310 (Fax)

From rolf@saans.north.de Fri Apr  3 11:03:36 1992
Received: from unido.Germany.EU.net by merlin.resmel.bhp.com.au with SMTP id AA08858
  (5.65b/IDA-1.4.3 for robin); Fri, 3 Apr 92 11:02:32 +1100
Received: from arbi.Informatik.Uni-Oldenburg.DE 
	by mail.Germany.EU.net with SMTP (5.65+/UNIDO-2.1.0.b)
	via EUnet for resmel.bhp.com.au
	id AA05853; Fri, 3 Apr 92 02:03:21 +0100
Received: by arbi.informatik.uni-oldenburg.de (smail3.1.18 + xalias);
	Fri, 3 Apr 92 01:58 MST
Received: by olis.isc.north.de (/\==/\ Smail3.1.22.1 #22.10)
	id <m0lWYnR-0000HRC@olis.isc.north.de>; Thu, 2 Apr 92 22:54 MES
Received: by skuld.north.de (/\=-/\ Smail3.1.16.1 #16.14)
	id <m0lWW8S-0001JVC@skuld.north.de>; Thu, 2 Apr 92 18:03 GMT
Received: by saans (/\=-/\ Smail3.1.16.1 #16.21)
	id <m0lW9Yf-00016TC@saans>; Wed, 1 Apr 92 19:57 mesz
Message-Id: <m0lW9Yf-00016TC@saans>
Date: Wed, 1 Apr 92 19:57 mesz
From: rolf@saans.north.de (Rolf Nerstheimer)
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Status: O

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.

Hello Robin,
I can help.

#    Wyse 60
#    Clearing of arrow keys useful in 'is' in case this entry is
#    used after wy60ak entry was used.
#
w7|wy60|wyse60|Wyse WY-60 with 80 column/24 line screen in wy60 mode:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\177\EZ1,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177\Ec72:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
# Wy60ak:
# Arrow keys are programmed to emit ANSI standard sequences.  Allows 
# applications to distinguish between destructive Back Space and
# non-destructive Left Arrow Key.  END and INS keys also emit
# ANSI standard sequences.
# Held out `te' string so that `is' will remain in effect
# throughout login session.
# On the Enhanced PC Keyboard, only the Cursor Keypad between the Main
# Keypad and the Numeric Keypad is programmable.  These arrow keys
# and special cursor motion keys will function as labeled when using
# wy60ak with applications supporting the wy60ak entry. The Numeric
# Keypad cursor motion keys will continue to emit their default values.
#
WA|wy60ak|wyse60ak|Wyse 60 in wy60 mode with ANSI arrow keys +:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177\Ec72:\
	:ti=\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:EN=\E[F:\
	:tc=wy60:


Hope it helps.
Regards, 
Rolf
-- 
Rolf Nerstheimer, Surwisch 20, 2856 Sandstedt, Germany   | a private 
E-Mail: rolf@saans.north.de    Voice: +49 4702 1285      |   node           
"Contrariwise," continued Tweedledee, "if it was so, it might be; and if it
were so, it would be; but as it isn't, it ain't. That's logic." Lewis Carroll

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From ksmith!root@uunet.uu.net Fri Apr  3 22:13:56 1992
Received: from munnari.OZ.AU by merlin.resmel.bhp.com.au with SMTP id AA25326
  (5.65b/IDA-1.4.3 for robin); Fri, 3 Apr 92 22:12:59 +1100
Received: from uunet by munnari.oz.au with UUCP (5.64+1.3.1+0.50)
	id AA09581; Fri, 3 Apr 1992 21:12:40 +1000 (from ksmith!root@uunet.uu.net)
From: ksmith!root@uunet.uu.net
Received: from uunet.uu.net (via LOCALHOST.UU.NET) by relay2.UU.NET with SMTP 
	(5.61/UUNET-internet-primary) id AA20824; Wed, 1 Apr 92 18:59:07 -0500
Received: from ksmith.UUCP by uunet.uu.net with UUCP/RMAIL
	(queueing-rmail) id 185842.23893; Wed, 1 Apr 1992 18:58:42 EST
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
In-Reply-To: <1992Mar31.005748.3186@resmel.bhp.com.au>
Organization: Keith's Computer, Hope Mills, NC
Cc: 
Date: Tue, 31 Mar 92 10:55:11 EST
Sender: ksmith!root@uunet.uu.net
Message-Id:  <9203311055.aa27661@ksmith.UUCP>
Status: O

w1|wy60|wyse60|Wyse WY-60 PC Terminal:\
	:CF=\E`0:\
	:CO=\E`1:\
	:Cm=1248:\
	:Co=\EG:\
	:Cp=p0t4x8|<r2v6z\072~>:\
	:Cr#16:\
	:EN=\ET:\
	:G1=\277:\
	:G2=\332:\
	:G3=\300:\
	:G4=\331:\
	:GC=\305:\
	:GD=\302:\
	:GH=\304:\
	:GL=\265:\
	:GR=\303:\
	:GU=\301:\
	:GV=\263:\
	:HM=\036:\
	:IN=\EQ:\
	:PD=\EK:\
	:PU=\EJ:\
	:al=\EE:\
	:am:\
	:bs:\
	:ce=\ET:\
	:cm=\Ea%i%dR%dC:\
	:co#80:\
	:cl=\E{\E*:\
	:k0=\001@\r:\
	:k1=\001A\r:\
	:k2=\001B\r:\
	:k3=\001C\r:\
	:k4=\001D\r:\
	:k5=\001E\r:\
	:k6=^AF\r:\
	:k7=^AG\r:\
	:k8=^AH\r:\
	:k9=^AI\r:\
	:kA=^AJ\r:\
	:kB=^AK\r:\
	:kC=^A`\r:\
	:kD=^Aa\r:\
	:kE=^Ab\r:\
	:kF=^Ac\r:\
	:kG=^Ad\r:\
	:kH=^Ae\r:\
	:kI=^Af\r:\
	:kJ=^Ag\r:\
	:kK=^Ah\r:\
	:kL=^Ai\r:\
	:kM=^Aj\r:\
	:kN=^Ak\r:\
	:kd=^J:\
	:kl=^H:\
	:kr=^L:\
	:ku=^K:\
	:kh=\036:\
	:l0=f1:\
	:l1=f2:\
	:l2=f3:\
	:l3=f4:\
	:l4=f5:\
	:l5=f6:\
	:l6=f7:\
	:l7=f8:\
	:l8=f9:\
	:l9=f10\
	:lA=f11:\
	:lB=f12:\
	:nd=\014:\
	:li#25:\
	:se=\EG0:\
	:so=\EG4:\
	:up=\013:
# 132 Column Wyse
w2|wy60-132|132 Column Wyse 60:\
	:is=\E`;:\
	:co#132:\
	:tc=wy60:
#
# wy60a - with Function Keys programmed like the SCO Console
#	but native other functions
w3|wy60a|Wyse 60 with ansi keys:\
	:CF=\E`0:\
	:CO=\E`1:\
	:Cm=1248:\
	:Co=\EG:\
	:Cp=p0t4x8|<r2v6z\072~>:\
	:Cr#16:\
	:EN=\E[F:\
	:G1=\277:\
	:G2=\332:\
	:G3=\300:\
	:G4=\331:\
	:GC=\305:\
	:GD=\302:\
	:GE=\EcD:\
	:GH=\304:\
	:GL=\265:\
	:GR=\303:\
	:GS=\EcE:\
	:GU=\301:\
	:GV=\263:\
	:HM=\E[H:\
	:IN=\E[L:\
	:PD=\E[G:\
	:PU=\E[I:\
	:al=\EE:\
	:bs:\
	:ce=\ET:\
	:cm=\Ea%i%dR%dC:\
	:cl=\E{\E*:\
	:is=\Ed.:\
	:co#80:\
	:k1=\E[M:\
	:k2=\E[N:\
	:k3=\E[O:\
	:k4=\E[P:\
	:k5=\E[Q:\
	:k6=\E[R:\
	:k7=\E[S:\
	:k8=\E[T:\
	:k9=\E[U:\
	:kd=\E[B:\
	:kl=\E[D:\
	:kr=\E[C:\
	:ku=\E[A:\
	:kA=\E[V:\
	:kB=\E[W:\
	:kC=\E[X:\
	:kD=\E[Y:\
	:kE=\E[Z:\
	:kF=\E[a:\
	:kG=\E[b:\
	:kH=\E[c:\
	:kI=\E[d:\
	:kJ=\E[e:\
	:kK=\E[f:\
	:kL=\E[g:\
	:kM=\E[h:\
	:kN=\E[i:\
	:kO=\E[j:\
	:nd=\014:\
	:li#25:\
	:se=\EG0:\
	:so=\EG4:\
	:up=\013:
# 132 Column Wyse
w4|wy60a-42w|43 X 132 Column Wyse 60:\
	:is=\E`;:\
	:co#132:\
	:li#42:\
	:tc=wy60a:
-- 
Keith Smith          uunet!ksmith!keith            5719 Archer Rd.
Digital Designs      BBS 1-919-423-4216            Hope Mills, NC 28348-2201
Somewhere in the Styx of North Carolina ...

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From mah@dialix.oz.au Thu Apr  2 16:08:04 1992
Received: from uniwa.uwa.oz.au by merlin.resmel.bhp.com.au with SMTP id AA19075
  (5.65b/IDA-1.4.3 for robin); Thu, 2 Apr 92 16:07:33 +1100
Received: by uniwa.uwa.oz.au (5.61+IDA+MU)
	id AA10410; Thu, 2 Apr 1992 13:07:21 +0800
From: Marcus Hayes <mah@dialix.oz.au>
X-Mailer: SCO System V Mail (version 3.2)
To: robin@resmel.bhp.com.au
Date: Thu, 2 Apr 92 12:41:21 WST
Message-Id:  <9204021241.aa02185@DIALix.oz.au>
Status: OR

To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin

wA|wy60|wyse60|wyse 60:\
	:co#80:li#24:am:\
	:al=\EE:\
	:as=\EH^B:ae=\EH^C:\
	:bl=^G:\
	:bs:bt=\EI:\
	:cd=\EY:ce=\ET:cl=\E+:cm=\Ea%i%dR%dC:\
	:ll=\Ea24R1C:\
	:cr=^M:\
	:dc=\EW:dl=\ER:\
	:ho=^^:\
	:im=\Eq:ei=\Er:ic=\Eq:\
	:if=/usr/lib/tabset/stdcrt:\
	:is=\Ee.\E`\072\Ee(\Ec21:\
	:kb=^H:kd=^J:kh=^^:kr=^L:ku=^K:\
	:k0=\EQ:\
	:k1=^A@:k2=^AA:k3=^AB:k4=^AC:\
	:k5=^AD:k6=^AE:k7=^AF:k8=^AG:\
	:k9=^AH:k;=^AI:F1=^AJ:F2=^AK:\
	:F3=^AL:F4=^AM:F5=^AN:F6=^AO:\
	:F7=\EQ:F8=\EW:F9=\ET:FA=\Er:\
	:nd=^L:nl=^J:\
	:so=\EG4:se=\EG0:\
	:us=\EG8:ue=\EG0:\
	:me=\EG0:mb=\EG2:md=\EG4:mh=\EGp:mr=\EG4:\
	:ta=\Ei:\
	:up=^K:\
	:hs:ws#78:ts=\Ez(:fs=^M:
wB|wy60-w|Wyse 60 with 24 rows 132 cols:\
	:if=/usr/lib/tabset/stdcrt-132:\
	:li#24:co#132:is=\E`;\Ee(\Ec21:tc=wy60:
wC|wy60-l|Wyse 60 with 42 rows and 80 cols:\
	:li#42:co#80:is=\Ee*\E`\072\Ec21:tc=wy60:
wD|wy60-wl|wy60-lw|Wyse 60 with 42 rows and 132 cols:\
	:if=/usr/lib/tabset/stdcrt-132:\
	:li#42:co#132:is=\E`;\Ee*\Ec21:tc=wy60:
wE|wy60c|Wyse 60 with seperate scrolling and editing regions (context switch):\
	:ti=\EwB:te=\EwC:\
	:is=\E`\072\Ee(\Ec21\EwJ:\
	:tc=wy60:
wF|wy60c-w|Wyse 60 Context Switch with 24 rows 132 cols:\
	:ti=\EwB:te=\EwC:\
	:is=\E`;\Ee(\Ec21\EwJ:\
	:tc=wy60-w:
wG|wy60emacs|Wyse 60 doesn't set XON/XOFF handshaking (emacs) :\
	:is=\Ee*\E`\072\Ec20:tc=wy60:
wH|wy60emacs-w|Wyse 60 emacs with 24 rows and 132 cols:\
	:if=/usr/lib/tabset/stdcrt-132:\
	:li#24:co#132:is=\E`;\Ee(\Ec20:tc=wy60:
wI|wy60emacs-l|Wyse 60 emacs with 42 rows and 80 cols:\
	:li#42:co#80:is=\Ee*\E`\072\Ec20:tc=wy60:
wJ|wy60emacs-wl|wy60emacs-lw|Wyse 60 emacs with 42 rows and 132 cols:\
	:if=/usr/lib/tabset/stdcrt-132:\
	:li#42:co#132:is=\E`;\Ee*\Ec20:tc=wy60:

hope this helps


+=======================================================================+
|          Mark Hayes                                                   |
|  ,-_|\   Corporate Systems               Internet: mah@DIALix.oz.au   |
| /     \  83 Mill Point Road              Phone: +61 9 264 1616        |
| *_,-._/  South Perth  WA 6151            Fax:   +61 9 474 2553        |
|      v                                                                |
+=======================================================================+
          Only 19,999 lines of C++ to my next ski trip ....
 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -


From andrew@teslab.lab.oz.au Wed Apr  8 12:08:08 1992
Received: from munnari.OZ.AU by merlin.resmel.bhp.com.au with SMTP id AA12230
  (5.65b/IDA-1.4.3 for robin); Wed, 8 Apr 92 12:07:55 +1100
Received: from teslab.lab.oz (via metro) by munnari.oz.au with SunIII (5.64+1.3.1+0.50)
	id AA06446; Wed, 8 Apr 1992 11:07:52 +1000 (from andrew@teslab.lab.oz.au)
Message-Id: <9204080107.6446@munnari.oz.au>
Date:  6 Apr 92 11:37:27 +1000 (Mon)
From: andrew@teslab.lab.oz.au (Andrew Phillips)
To: robin@resmel.bhp.com.au (Robin Brown)
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
Organization: Technology Evaluation Section, L.A.B., Sydney
Status: OR

Find below our Wyse 60 termcap entries.  Note that the uppercase
names such as PU are probably Xenix specific.

The first entry comes with the system.  The other four I made up to
put the terminal into different screen resolutions.  They also
reprogram the arrow keys since by default the arrow keys return
values used by other keys (e.g. left arrow returns the same as Back-space).

--------------
w7|wy60|wyse60|Wyse WY-60 with 80 column/24 line screen in wy60 mode:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ed/:\
	:if=/usr/lib/tabset/std:pt:\
	:G1=\EH3:G2=\EH2:G3=\EH1:G4=\EH5:GD=\EH0:GG#0:GH=\EH\072:\
	:GU=\EH=:GV=\EH6:GR=\EH4:GL=\EH9:GC=\EH8:GF=\EH7:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=\EE:am:bs:bt=\EI:cd=\EY:ce=\ET:cl=\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=\EW:dl=\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:sg#0:ug#0:ue=\EG0:ul:up=^K:us=\EG8:
WA|wy60ak|Wyse 60 with ANSI arrows,PgUp,PgDn,End,Ins & 25 lines:\
	:is=\E~4\EZ0,\E[B\177\EZ0-\E[D\177\EZ0.\E[C\177\EZ0+\E[A\177\
\EZ02\EB\177\EZ03\EF\177\EZ0\134\E[F\177\EZ0\072\E[I\177\EZ0r\E[G\177\
\EZ0q\E[L\177\E`\072\EO\Ee6\Ed/\EeQ\Ee):li#25:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:EN=\E[F:PU=\E[I:PD=\E[G:\
	:tc=wy60:
WL|wy60ak-43|Wyse 60 with 43 lines (and ANSI arrows,PgUp,etc):\
	:is=\EZ0,\E[B\177\EZ0-\E[D\177\EZ0.\E[C\177\EZ0+\E[A\177\
\EZ02\EB\177\EZ03\EF\177\EZ0\134\E[F\177\EZ0\072\E[I\177\EZ0r\E[G\177\
\EZ0q\E[L\177\E`\072\EO\Ee6\E~4\Ed/\EeQ\Ee+:li#43:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:EN=\E[F:PU=\E[I:PD=\E[G:\
	:tc=wy60:
WW|wy60ak-w|Wyse 60 with 132 columns (and ANSI arrows,PgUp,etc):\
	:is=\EZ0,\E[B\177\EZ0-\E[D\177\EZ0.\E[C\177\EZ0+\E[A\177\
\EZ02\EB\177\EZ03\EF\177\EZ0\134\E[F\177\EZ0\072\E[I\177\EZ0r\E[G\177\
\EZ0q\E[L\177\E`;\EO\Ee6\E~4\Ed/\EeQ\Ee):li#25:co#132:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:EN=\E[F:PU=\E[I:PD=\E[G:\
	:tc=wy60:
WX|wy60ak-43-w|Wyse 60 with 43 lines and 132 columns:\
	:is=\EZ0,\E[B\177\EZ0-\E[D\177\EZ0.\E[C\177\EZ0+\E[A\177\
\EZ02\EB\177\EZ03\EF\177\EZ0\134\E[F\177\EZ0\072\E[I\177\EZ0r\E[G\177\
\EZ0q\E[L\177\E`;\EO\Ee6\E~4\Ed/\EeQ\Ee+:li#43:co#132:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:EN=\E[F:PU=\E[I:PD=\E[G:\
	:tc=wy60:

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From wang!fredj@uunet.uu.net Fri Apr 10 06:07:46 1992
Received: from munnari.OZ.AU by merlin.resmel.bhp.com.au with SMTP id AA03198
  (5.65b/IDA-1.4.3 for robin); Fri, 10 Apr 92 06:07:06 +1100
Received: from uunet by munnari.oz.au with UUCP (5.64+1.3.1+0.50)
	id AA13677; Fri, 10 Apr 1992 05:06:44 +1000 (from wang!fredj@uunet.uu.net)
Received: from uunet.uu.net (via LOCALHOST.UU.NET) by relay2.UU.NET with SMTP 
	(5.61/UUNET-internet-primary) id AA15448; Thu, 9 Apr 92 14:59:22 -0400
Received: from wang.UUCP by uunet.uu.net with UUCP/RMAIL
	(queueing-rmail) id 145838.10833; Thu, 9 Apr 1992 14:58:38 EDT
Received: from wonk.wang.com by elf.wang.com
	id aa23260; Thu, 9 Apr 92 13:10:44 EDT
Received:  by wonk.wang.com (5.59/TF-1)
    id AA08269; Thu, 9 Apr 92 13:10:51 EDT
Return-Path: <fredj@wang.com>
Date: Thu, 9 Apr 92 13:10:51 EDT
From: Fred Jewell	<fredj@wang.com>
Message-Id: <9204091710.AA08269@wonk.wang.com>
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Status: OR

In comp.unix.admin you write:

>Hi,
>The subject says it all, I'm looking for one - can anyone help, it would
>make my life so much easier.
>Thanks in advance,
>Robin

>-- 
>Robin Brown, System administrator, BHP Research - Melbourne Laboratories
>245 Wellington Road Mulgrave VIC 3184 Australia
>E-mail: robin@resmel.bhp.com.au  ph: +61-3-560-7066  fax: +61-3-561-6709
 
Robin,
    Here is a bunch....you don't know where they came from, they just
magically appeared, i did'nt give them to you, and you owe me big time :-)
           fredj.wang.com

____________________________________________________________________________

#    Wyse 60
#    Clearing of arrow keys useful in 'is' in case this entry is
#    used after wy60ak entry was used.
#
w7|wy60|wyse60|Wyse WY-60 with 80 column/24 line screen in wy60 mode:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\177\EZ1,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177\Ec72:\
	:if=/usr/lib/tabset/std:pt:\
	:CF=\E`0:CO=\E`1:\
	:G1=3:G2=2:G3=1:G4=5:\
	:GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
	:GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
	:PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
	:al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
	:cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
	:PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
#
# Wy60ak:
# Arrow keys are programmed to emit ANSI standard sequences.  Allows 
# applications to distinguish between destructive Back Space and
# non-destructive Left Arrow Key.  END and INS keys also emit
# ANSI standard sequences.
# Held out `te' string so that `is' will remain in effect
# throughout login session.
# On the Enhanced PC Keyboard, only the Cursor Keypad between the Main
# Keypad and the Numeric Keypad is programmable.  These arrow keys
# and special cursor motion keys will function as labeled when using
# wy60ak with applications supporting the wy60ak entry. The Numeric
# Keypad cursor motion keys will continue to emit their default values.
#
WA|wy60ak|wyse60ak|Wyse 60 in wy60 mode with ANSI arrow keys +:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177\Ec72:\
	:ti=\EZ1+\E[A\177\EZ1,\E[B\177\EZ1-\E[D\177\EZ1.\E[C\177\EZ1\\\E[F\177\EZ1q\E[L\177:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:EN=\E[F:\
	:tc=wy60:
#	Entry based on wy60 with wy60ak functionality.  Refer to 
#	wy60ak for more information.
WA|opus3n1+|Esprit  Opus3n1+ in wy60 mode with ANSI arrow keys +:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\Ezz&\E[A\177\Ezz'\E[B\177\Ezz(\E[D\177\Ezz)\E[C\177\Ezz<\E[Q\177\Ezz`\E[F\177\EA1\052\EZH12:\
	:ti=\Ezz&\E[A\177\Ezz'\E[B\177\Ezz(\E[D\177\Ezz)\E[C\177\Ezz<\E[Q\177:\
	:as=\EH\002:ae=\EH\003:\
	:kb=^H:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:ts=\EF:fs=\r:\
	:EN=\E[F:\
	:tc=wy60:
w8|wy60w|wyse60w|Wyse WY-60 with 132 column/24 line screen in wy60 mode:\
	:is=\E`\073\Ee(\EO\Ee6\Ec41\E~4\Ec21:\
	:if=/usr/lib/tabset/std:pt:\
	:G1=\EH3:G2=\EH2:G3=\EH1:G4=\EH5:GD=\EH0:GG#0:GH=\EH\072:\
	:GU=\EH=:GV=\EH6:GR=\EH4:GL=\EH9:GC=\EH8:GF=\EH7:\
	:PU=\EJ:PD=\EK:\
	:al=\EE:am:bs:bt=\EI:cd=\EY:ce=\ET:cl=\E+:\
	:cm=\Ea%i%dR%dC:co#132:dc=\EW:dl=\ER:ei=\Er:im=\Eq:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
	:li#24:mi:nd=^L:se=\EG0:so=\EG4:sg#0:ug#0:ue=\EG0:ul:up=^K:us=\EG8:



 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

From twg!bill@vanbc.wimsey.bc.ca Sun Apr 12 18:55:23 1992
Received: from van-bc.wimsey.bc.ca by merlin.resmel.bhp.com.au with SMTP id AA01768
  (5.65b/IDA-1.4.3 for robin); Sun, 12 Apr 92 18:55:03 +1100
Received: by vanbc.wimsey.bc.ca (/\==/\ Smail3.1.22.1 #22.7 rmail)
	id <m0lZzOg-0001v1C@vanbc.wimsey.bc.ca>; Sun, 12 Apr 92 00:54 PDT
Received: by twg.bc.ca (smail2.5)
	id AA00686; 12 Apr 92 00:49:39 PDT (Sun)
To: robin@resmel.bhp.com.au
Subject: Re: Looking for wyse60 termcap entry
Newsgroups: comp.unix.admin
References: <1992Mar31.005748.3186@resmel.bhp.com.au>
Reply-To: bill@twg.bc.ca (Bill Irwin)
Message-Id: <9204120049.AA00684@twg.bc.ca>
Date: 12 Apr 92 00:49:38 PDT (Sun)
From: bill@twg.bc.ca (Bill Irwin)
Status: OR

In comp.unix.admin you write:

: Hi,
: The subject says it all, I'm looking for one - can anyone help, it would
: make my life so much easier.
: Thanks in advance,
: Robin

: --
: Robin Brown, System administrator, BHP Research - Melbourne Laboratories
: 245 Wellington Road Mulgrave VIC 3184 Australia
: E-mail: robin@resmel.bhp.com.au  ph: +61-3-560-7066  fax: +61-3-561-6709

Here's the one we use.

w7|wy60|wyse60|Wyse WY-60 with 80 column/24 line screen in wy60 mode:\
        :if=/usr/lib/tabset/std:pt:\
        :CF=\E`0:CO=\E`1:\
        :G1=3:G2=2:G3=1:G4=5:GB=Z6820395]14:\
        :GC=8:GD=0:GE=\EH^C:GF=7:GG#0:GH=\072:\
        :GU==:GV=6:GR=4:GS=\EH^B:GL=9:\
        :PU=\EJ:PD=\EK:mb=\EG2:me=\EG0:\
        :al=4\EE:am:bs:bt=\EI:cd=100\EY:ce=\ET:cl=100\E+:\
        :cm=\Ea%i%dR%dC:co#80:dc=11\EW:dl=5\ER:ei=\Er:im=\Eq:k0=^AI\r:\
        :k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
        :k8=^AG\r:k9=^AH\r:kd=^J:kh=^~:kl=^H:kr=^L:ku=^K:\
        :li#24:mi:nd=^L:se=\EG0:so=\EG4:ug#0:ue=\EG0:ul:up=^K:us=\EG8:\
        :PN=\Ed#:PS=^T:hs:ts=\Ez(:fs=^M:
---
Bill Irwin    -       The Westrheim Group     -    Vancouver, BC, Canada
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
uunet!twg!bill            (604) 431-9600 (voice) |     Your Computer  
bill@twg.bc.ca            (604) 430-4329 (fax)   |    Systems Partner

-- 
Robin Brown, System administrator, BHP Research - Melbourne Laboratories
245 Wellington Road Mulgrave VIC 3184 Australia
E-mail: robin@resmel.bhp.com.au  ph: +61-3-560-7066  fax: +61-3-561-6709

 - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
Article 3630 of comp.terminals:
Path: cs.utk.edu!stc06.CTD.ORNL.GOV!news.ssc.gov!convex!insosf1.infonet.net!solaris.cc.vt.edu!news.mathworks.com!news.alpha.net!uwm.edu!vixen.cso.uiuc.edu!uxh.cso.uiuc.edu!dawn
From: dawn@uxh.cso.uiuc.edu (Dawn Owens-Nicholson)
Newsgroups: comp.terminals
Subject: Re: Help with Wyse 60
Date: 22 Feb 1995 05:33:16 GMT
Organization: University of Illinois at Urbana
Lines: 60
Message-ID: <3ieias$fov@vixen.cso.uiuc.edu>
References: <1995Feb21.133020@nyssa.swt.edu>
NNTP-Posting-Host: uxh.cso.uiuc.edu

rm15876@nyssa.swt.edu (Rodney Muras) writes:
>I'm trying ,with no luck :-(, to hook a Wyse 60 (model# WY-60-02-01)
>terminal up to a PC running Linux.  All I get on the terminal is garbage
>and I have a very incomplete term cap.  I would appreciate
>	
>	1.  Info on the Wyse 60 (I have nothing)
>	2.  Termcap entry for the terminal
>	3.  Any advice you might have ;-) 

Here's some termcap data for the Wyse 60.  Since I didn't write it I
can't guarantee it's value.  On the other hand, if you had a Wyse 60
manual and were willing to ship it to me, I could get a good and
complete Wyse 60 termcap and terminfo entry put together.

-Dawn

w6|wy60|wyse60|Wyse 60:\
        :am:bw:hs:km:mi:ms:bs:pt:\
        :co#80:li#24:kn#9:\
        :ae=\EH^C:al=4\EE:as=\EH^B:bt=\EI:cd=100\Ey:ce=\Et:\
        :cl=100\E*:cm=\E=%+ %+ :ct=\E0:dc=11\EW:dl=5\ER:\
        :ds=\EF\r:ei=\Er:fs=\r:ho=^^:i1=\EcB0\EcC1:im=\Eq:\
        :ip=3:\
        :pf=^T:po=^R:\
        :is=\Ed$\EcD\E'\Er\EH^C\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1^N^T\EwJ\Ew1^^^K:\
        :k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
        :k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=\b:kd=\n:\
        :kh=^^:kl=\b:kr=\f:ku=^K:ll=^^^K:nd=\f:r1=150\E~!\E~4:\
        :r2=150\EeG:r3=200\EwG\Ee(:se=\EG0:so=\EGt:sr=7\Ej:\
        :st=\E1:ts=\EF:ue=\EG0:up=^K:us=\EG8:te=\Ew1:ti=\Ew0:\
        :ve=\E`1:vi=\E`0:ko=bt,le,do,nd,up,dc,dl,ho,al:
#       Must delete uc= if using infocomp to translate
w7|wy60-w|wyse60-w|wyse 60 132-column:\
        :cm=\Ea%i%dR%dC:co#132:dc=16\EW:ip=5:r2=300\EeF\E`;:\
        :tc=wy60:
w8|wy60-25|wyse60-25|wyse 60 80-column 25-lines:\
        :li#25:r3=200\EwG\Ee):\
        :tc=wy60:
w9|wy60-25-w|wyse60-25-w|wyse 60 132-column 25-lines:\
        :li#25:r3=200\EwG\Ee):\
        :tc=wy60-w:
wa|wy60-42|wyse60-42|wyse 60 80-column 42-lines:\
        :al=11\EE:cd=260\Ey:cl=260\E*:cm=2\E=%+ %+ :dc=16\EW:\
        :dl=11\ER:i1=\EcB2\EcC3:ip=5:li#42:r3=150\Ee*:sr=10\Ej:\
        :tc=wy60:
wb|wy60-42-w|wyse60-42-w|wyse 60 132-column 42-lines:\
        :cm=2\Ea%i%dR%dC:co#132:dc=19\EW:ho=2^^:ip=6:r2=300\EeF\E`;:\
        :tc=wy60-42:
wc|wy60-43|wyse60-43|wyse 60 80-column 43-lines:\
        :li#43:r3=150\Ee+:\
        :tc=wy60-42:
wd|wy60-43-w|wyse60-43-w|wyse 60 132-column 43-lines:\
        :li#43:r3=150\Ee+:\
        :tc=wy60-42-w:
we|wy60-vb|wyse60-vb|Wyse 60 Visable bell:\
        :vb=\E`8\E`9:\
        :tc=wy60:
wf|wy60-w-vb|wy60-wvb|wyse60-wvb|Wyse 60 132-column Visable bell:\
        :vb=\E`8\E`9:\
        :tc=wy60-w:

 =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

Article 4867 of comp.terminals:
Newsgroups: comp.terminals
Path: cs.utk.edu!stc06.ctd.ornl.gov!rsg1.er.usgs.gov!ukma!usenet.eel.ufl.edu!news.mathworks.com!tank.news.pipex.net!pipex!howland.reston.ans.net!cs.utexas.edu!news.sprintlink.net!in2.uu.net!uunet.ca!news.uunet.ca!dmog10.bell.ca!bcocek!news
From: Daniel Proulx <daproulx>
Subject: Re: HELP! Problem with character attributes on Wyse 50
X-Nntp-Posting-Host: cmocaj.qc.bell.ca
Content-Type: multipart/mixed;
	boundary="-------------------------------4518982681096976805931336570"
Message-ID: <DFvo4r.Mv1@on.bell.ca>
Sender: news@on.bell.ca
Organization: Bell Sygma Telecom Solutions Inc.
Mime-Version: 1.0
Date: Tue, 3 Oct 1995 14:55:39 GMT
X-Mailer: Mozilla 1.1N (X11; I; SunOS 4.1.3_U1 sun4m)
X-Url: file:/export/nsms/daproulx/Mail/wyseprob.txt
Lines: 215

This is a multi-part message in MIME format.

---------------------------------4518982681096976805931336570
Content-Transfer-Encoding: 7bit
Content-Type: text/plain; charset=us-ascii

We found a terminfo definition in Wyse's support databse on the Web that works.

Previous posting and terminfo definition attached.

Daniel.

===========================================================================
Daniel Proulx						daproulx@qc.bell.ca
Consultant						(514) 391-1633
Bell Sygma Telecom Solutions Inc.			(514) 870-3004 FAX
25N1-700 de la Gauchetiere ouest
Montreal(Que.) H3B 4L1
Canada
===========================================================================

---------------------------------4518982681096976805931336570
Content-Transfer-Encoding: 7bit
Content-Type: text/plain

From daproulx Sat Sep 30 01:44:13 1995
Date: Sat, 30 Sep 95 01:44:12 -0400
Sender: daproulx
From: Daniel Proulx <daproulx>
Organization: Bell Sygma Telecom Solutions Inc.
X-Mailer: Mozilla 1.1N (X11; I; SunOS 4.1.3_U1 sun4m)
Mime-Version: 1.0
Newsgroups: comp.terminals
To: daproulx, nsmslog, jrokos@wyse.com, marcom@wyse.com
Subject: HELP! Problem with characrter attributes on Wyse 50.
X-Url: news:comp.terminals
Content-Transfer-Encoding: 7bit
Content-Type: text/plain; charset=us-ascii
Content-Length: 1785

Hi,

We are trying to display character attributes (underline, reverse video or
standout, blinking, etc.) and when we enable the attribute the terminal
always adds a blank at the current position and then sets the attribute.
A blank is also added when we turn off the attribute.  Is it a normal
behavior?  When we send the same sequences on a Wyse 60 it works OK.

Example: Let's say we want to display the following box with the 3 inner
	 characters in stand out mode:
		+++++
		|   |
		+++++

	It appears the following way:

		+++++
		| XXX |
		+++++

		where XXX are blanks in stand out mode.

	We activate the stand out mode with \EGt (\E = ESC) and disable it 
	with \EG0.  More precisely, the second line is sent as:

		|\EGt   \EG0|

The application we want to run was build with the character-based version
of Neuron Data and it runs on a Solaris 2.4 Unix workstation.  The terminal
we use is a real Wyse 50 and we set TERM=wyse50.  Neuron Data uses the terminal
definition in the terminfo database (on Solaris 2.4).

Is there any special mode to set to avoid these extra blanks?

Does anybody have an electronic version of the Wyse 50 Reference Manual?

Could somebody fax me the pages related to control sequences or anything
that would explain how to use the attributes properly?

Anything that could help?

It is actually 1:30 am EDT and I need help!

Please e-mail also, so I will get the answer more directly.

Thanks,

Daniel.

===========================================================================
Daniel Proulx						daproulx@qc.bell.ca
Consultant						(514) 391-1633
Bell Sygma Telecom Solutions Inc.			(514) 870-3004 FAX
25N1-700 de la Gauchetiere ouest
Montreal(Que.) H3B 4L1
Canada
===========================================================================



#
#	   The Wyse 50 can support one attribute (e.g. Dim, Inverse,
#	Normal) without magic cookies by using the protect mode.
#	The following description uses this feature, but when more
#	than one attribute is put on the screen at once, all attributes
#	will be changed to be the same as the last attribute given.
#	   The Wyse 50 can support more attributes when used with magic
#	cookies.  The wy50-mc terminal description uses magic cookies
#	to correctly handle multiple attributes on a screen.
#
wy50-syg|wyse50-syg|Wyse 50-syg,
	acsc=0wa_h[jukslrmqnxqzttuyv]wpxv,
	am,
	bel=^G,
	bw,
	cbt=\EI,
	civis=\E`0,
	clear=\E+$<20>,
	cnorm=\E`1,
	cols#80,
	cr=^M,
	cub1=^H,
	cud1=^J,
	cuf1=^L,
	cup=\E=%p1%' '%+%c%p2%' '%+%c,
	cuu1=^K,
	dch1=\EW$<1>,
	dim=\E`7\E),
	dl1=\ER,
	dsl=\EF^M,
	ed=\EY$<20>,
	el=\ET,
	fsl=^M,
	home=^^,
	hs,
	ht=^I,
	hts=\E1,
	.ich1=\EQ,
	il1=\EE,
	ind=^J$<2>,
	ip=$<1>,
	is1=\E`:\E`9$<30>,
	is2=^N^T\E'\E(,
	.it#8,
	kbs=^H,
	kcbt=\EI,
	kcub1=^H,
	kcud1=^J,
	kcuf1=^L,
	kcuu1=^K,
	kdch1=\EW,
	kdl1=\ER,
	ked=\EY,
	kel=\ET,
	kent=\E7,
	kf1=^A@^M,
	kf2=^AA^M,
	kf3=^AB^M,
	kf4=^AC^M,
	kf5=^AD^M,
	kf6=^AE^M,
	kf7=^AF^M,
	kf8=^AG^M,
	kf9=^AH^M,
	kf10=^AI^M,
	kf11=^AJ^M,
	kf12=^AK^M,
	kf13=^AL^M,
	kf14=^AM^M,
	kf15=^AN^M,
	kf16=^AO^M,
	kHOM=\E{,
	khome=^^,
	kich1=\EQ,
	kil1=\EE,
	knp=\EK,
	kpp=\EJ,
	kprt=\EP,
	krpl=\Er,
	lh#1,
	lines#24,
	ll=^^^K,
	lw#8,
	ma#1,
	mc0=\EP,
	mc4=^T,
	mc5=^X,
	mc5i,
	mir,
	msgr,
	nel=^M^J,
	nlab#8,
	pfx=\Ez%p1%'?'%+%c%p2%s\177,
	pln=\Ez%p1%'/'%+%c%p2%s^M,
	prot=\E`7\E),
	rev=\E`6\E),
	ri=\Ej,
	rmacs=\EH^C,
	rmir=\Er,
	rmln=\EA11,
	rmso=\E(,
	sgr=%?%p1%p3%|%t\E`6\E)
		%e%p5%p8%|%t\E`7\E)%e\E(%;
		%?%p9%t\EH^B%e\EH^C%;,
	sgr0=\E(\EH^C,
	smacs=\EH^B,
	smir=\Eq,
	smln=\EA10,
	smso=\E`6\E),
	tbc=\E0,
	tsl=\EF,
	wsl#45,
	xon,

---------------------------------4518982681096976805931336570--


 =:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=:=

Path:  cs.utk.edu!stc06.ctd.ornl.gov!fnnews.fnal.gov!uwm.edu!lll-winken.llnl.gov!news.larc.nasa.gov!night.primate.wisc.edu!tmpnews.crd.ge.com!news.crd.ge.com!rebecca!rpi!wrf
From: wrf@speed.ecse.rpi.edu (Wm Randolph Franklin)
Newsgroups: comp.terminals
Subject: Wyse ASCII terminal info, esp WY520
Date: 9 May 1996 14:23:33 GMT
Organization: ECSE Dept, Rensselaer Polytechnic Institute, Troy, NY, 12180 USA
Lines: 469
Message-ID: <4msv55$s0c@usenet.rpi.edu>
Reply-To: wrf@ecse.rpi.edu

Wyse's current URL is http://www.wyse.com/

Wyse has a BBS containing termcap and terminfo stuff for their
terminals.  According to their tech support, at 800-800-9973, it's
at 408-922-4400 thru 4405.  The 4400 modem is flaky as of 5/96, so
call 4401 etc.  Come in at 9600 hard; Don't use autospeed sense.

Appended are the entries for the Wyse 520.

------------------------
		      Wm. Randolph Franklin
			 wrf@ecse.rpi.edu
	      http://www.ecse.rpi.edu/Homepages/wrf/
		  +1 (518) 276-6077;  Fax: -6261
ECSE Dept., 6026 JEC, Rensselaer Polytechnic Inst, Troy NY, 12180 USA

================================================================

#
#TITLE:  TERMINFO ENTRY WY520
#DATE:   8/5/93
# The WY520 terminfo is based on the WY285 entry published on the WYSE 
# BBS with the addition of more function keys and special keys.
#
#               rs1 -> set personality
#               rs2 -> set number of columns
#               rs3 -> set number of lines
#               is1 -> select the proper font
#               is2 -> do the initialization
#               is3 -> If this string is empty then rs3 gets sent.
#
#       Wyse 520 emulating a vt420 7 bit mode with default ANSI keyboard
#       - The BS key is programmed to generate BS in smcup since
#         is2 doesn't seem to work.
#       - Remove and shift/Remove: delete a character
#       - Insert : enter insert mode
#       - Find   : delete to end of file
#       - Select : clear a line
#       - F11, F12, F13: send default sequences (not ESC, BS, LF)
#       - F14 : Home key
#       - Bottom status line (host writable line) is used.
#       - smkx,rmkx are removed because this would put the numeric
#         keypad in Dec application mode which doesn't seem to work
#         with SCO applications.
#
wy520|wyse520|wyse 520,
        acsc=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~,
        am,
        bel=^G,
        blink=\E[5m,
        bold=\E[1m,
        cbt=\E[Z,
        civis=\E[?25l,
        clear=\E[H\E[J$<40>,
        .cnorm=\E[?25h,
        cnorm=\E[34h\E[?25h,
        cols#80,
        cr=\r,
        csr=\E[%i%p1%d;%p2%dr$<20>,
        cub1=\b,
        cub=\E[%p1%dD,
        cud1=\n,
        cud=\E[%p1%dB,
        cuf1=\E[C,
        cuf=\E[%p1%dC, 
        cup=\E[%i%p1%d;%p2%dH,
        cuu1=\E[A,
        cuu=\E[%p1%dA,
        cvvis=\E[?25h\E[34l,
        dch=\E[%p1%dP$<3>,
        dch1=\E[P$<30>,
        dim=\E[2m,
        dl=\E[%p1%dM$<2*>,
        dl1=\E[M$<2>,
        .dsl=\E7\E[99;0H\E[K\E8,
        dsl=\E[0$~,
        ech=\E[%p1%dX,
        ed=\E[J$<40>,
        el1=\E[1K,
        el=\E[K,
        enacs=\E)0,
        .eslok,
        .fsl=\E[1;24r\E8,
        fsl=\E[0$},
        home=\E[H,
        hpa=\E[%i%p1%d`,
        hs,
        ht=^I,
        hts=\EH,
        ich=\E[%p1%d@$<2>,
        .ich1=\E[@,
        il=\E[%p1%dL$<3*>,
        il1=\E[L$<3>,
        ind=\n$<2>,
        invis=\E[8m,
        ip=$<4>,
        is1=\E[?5W,
        is2=\E[2;4;20;30l\E[?1;4;10;16l\E[12h\E[?7;8;25;67h,
        is3=\E>\E(B\E)0^O\E[m,
        it#8,
        ka1=\EOw,
        ka3=\EOu,
        kb2=\EOy,
        kc1=\EOq,
        kc3=\EOs,
        kbs=^H,
        kcbt=\E[Z,
        kcub1=\E[D,
        kcud1=\E[B,
        kcuf1=\E[C,
        kcuu1=\E[A,
        kdch1=\E[3~,
        ked=\E[1~,
        kel=\E[4~,
        kent=\EOM,
        kf10=\E[21~,
        kf11=\E[23~,
        kf12=\E[24~,
        kf13=\E[25~,
        kf14=\E[26~,
        kf15=\E[28~,
        kf16=\E[29~,
        kf17=\E[31~,
        kf18=\E[32~,
        kf19=\E[33~,
        kf20=\E[34~,
        kf1=\EOP,
        kf2=\EOQ,
        kf3=\EOR,
        kf4=\EOS,
        kf6=\E[17~,
        kf7=\E[18~,
        kf8=\E[19~,
        kf9=\E[20~,
        kfnd=\E[1~,
        khlp=\E[28~,
        khome=\E[26~,
        kich1=\E[2~,
        km,
        knp=\E[6~,
        kpp=\E[5~,
        kslt=\E[4~,
        lf1=PF1,
        lf2=PF2,
        lf3=PF3,
        lf4=PF4,
        lines#24,
        mc0=\E[0i,
        mc4=\E[4i,
        mc5=\E[5i,
        mc5i,
        mir,
        rc=\E8,
        rev=\E[7m,
        ri=\EM$<2>,
        rmacs=^O,
        rmam=\E[?7l,
        rmcup=\E[ R,
        rmir=\E[4l,
        .rmkx=\E>,
        rmso=\E[m,
        rmul=\E[24m,
        rs1=\E[13l\E[3l\E\\\E[63;1"p\E[!p,
        rs2=\E[35h\E[?3l,
        rs3=\E[?5l\E[47h\E[40l\E[r,
        sc=\E7,
        sgr0=\E[m^O,
        sgr=\E[0%?%p2%t;4%;%?%p3%p1%|%t;7%;%?%p4%t;5%;%?%p5%t;2%;%?%p6%t;1%;%?%p7%t;8%;m%?%p9%t^N%e^O%;,
        smacs=^N,
        smam=\E[?7h,
        smcup=\E[ Q\E[?67;8h,
        smir=\E[4h,
        .smkx=\E[?1l\E=,
        smso=\E[7m,
        smul=\E[4m,
        tbc=\E[3g,
        .tsl=\E7\E[99;%i%p1%dH,
        tsl=\E[2$~\E[1$}\E[%i%p1%d`,
        vpa=\E[%i%p1%dd,
        wsl#80,
        xenl,
        xon,
#
#       Wyse 520 with 24 data lines and status (terminal status)
wy520-24|wyse520-24|wyse 520 with 24 data lines,
        tsl@, fsl@, dsl@, hs@,
        rs3=\E[?5l\E[47h\E[40l\E[1;24r,
        use=wy520,
#
#       Wyse 520 with visual bell.
wy520-vb|wyse520-vb|wyse 520 with visible bell,
        flash=\E[30h\E\,\E[30l$<100>,
        use=wy520,
#
#       Wyse 520 in 132-column mode.
wy520-w|wyse520-w|wyse 520 in 132-column mode,
        cols#132,
        wsl#132,
        dch=\E[%p1%dP$<7>,
        dch1=\E[P$<7>,
        ich=\E[%p1%d@$<7>,
        ip=$<7>,
        rs2=\E[35h\E[?3h,
        use=wy520,
#
#       Wyse 520 in 132-column mode with visual bell.
wy520-wvb|wyse520-wvb|wyse 520 with visible bell 132-columns,
        flash=\E[30h\E\,\E[30l$<100>,
        use=wy520-w,
#
#
#       Wyse 520 emulating a vt420 7 bit mode.
#       The DEL key is programmed to generate BS in is2.
#       With EPC keyboard.
#       - 'End' key will clear till end of line on EPC keyboard
#       - Shift/End : ignored.
#       - Insert : enter insert mode.
#       - Delete : delete a character (have to change interrupt character
#                  to CTRL-C: stty intr '^c') for it to work since the
#                  Delete key sends 7FH.
wy520-epc|wyse520-epc|wyse 520 with EPC kb,
        kdch1=\177,
        kel=\E[4~,
        kend=\E[4~,
        kf0=\E[21~,
        kf1=\E[11~,
        kf2=\E[12~,
        kf3=\E[13~,
        kf4=\E[14~,
        kf5=\E[15~,
        khome=\E[H,
        use=wy520,
#
#       Wyse 520 with 24 data lines and status (terminal status)
#       with EPC keyboard.
wy520-epc-24|wyse520-pc-24|wyse 520 with 24 data lines,
        tsl@, fsl@, dsl@, hs@,
        rs3=\E[?5l\E[47h\E[40l\E[1;24r,
        use=wy520-epc,
#
#       Wyse 520 with visual bell.
wy520-epc-vb|wyse520-pc-vb|wyse 520 with visible bell,
        flash=\E[30h\E\,\E[30l$<100>,
        use=wy520-epc,
#
#       Wyse 520 in 132-column mode.
wy520-epc-w|wyse520-epc-w|wyse 520 in 132-column mode,
        cols#132,
        wsl#132,
        dch=\E[%p1%dP$<7>,
        dch1=\E[P$<7>,
        ich=\E[%p1%d@$<7>,
        ip=$<7>,
        rs2=\E[35h\E[?3h,
        use=wy520-epc,
#
#       Wyse 520 in 132-column mode with visual bell.
wy520-epc-wvb|wyse520-p-wvb|wyse 520 with visible bell 132-columns,
        flash=\E[30h\E\,\E[30l$<100>,
        use=wy520-epc-w,
#
#       Wyse 520 in 80-column, 36 lines
wy520-36|wyse520-36|wyse 520 with 36 data lines,
        lines#36,
        tsl@, fsl@, dsl@, hs@,
        rs3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r,
        use=wy520,
#
#       Wyse 520 in 80-column, 48 lines
wy520-48|wyse520-48|wyse 520 with 48 data lines,
        lines#48,
        tsl@, fsl@, dsl@, hs@,
        rs3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r,
        use=wy520,
#
#       Wyse 520 in 132-column, 36 lines
wy520-36w|wyse520-36w|wyse 520 with 36 data lines,
        cols#132,
        wsl#132,
        rs2=\E[?3h,
        rs3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r\E[132$|,
        use=wy520-36,
#
#       Wyse 520 in 132-column, 48 lines
wy520-48w|wyse520-48w|wyse 520 with 48 data lines,
        cols#132,
        wsl#132,
        rs2=\E[?3h,
        rs3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r\E[132$|,
        use=wy520-48,
#
#
#       Wyse 520 in 80-column, 36 lines with EPC keyboard
wy520-36pc|wyse520-36pc|wyse 520 with 36 data lines,
        lines#36,
        tsl@, fsl@, dsl@, hs@,
        rs3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r,
        use=wy520-epc,
#
#       Wyse 520 in 80-column, 48 lines with EPC keyboard
wy520-48pc|wyse520-48pc|wyse 520 with 48 data lines,
        lines#48,
        tsl@, fsl@, dsl@, hs@,
        rs3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r,
        use=wy520-epc,
#
#       Wyse 520 in 132-column, 36 lines with EPC keyboard
wy520-36wpc|wyse520-36wpc|wyse 520 with 36 data lines,
        cols#132,
        wsl#132,
        rs2=\E[?3h,
        rs3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r\E[132$|,
        use=wy520-36pc,
#
#       Wyse 520 in 132-column, 48 lines with EPC keyboard
wy520-48wpc|wyse520-48wpc|wyse 520 with 48 data lines,
        cols#132,
        wsl#132,
        rs2=\E[?3h,
        rs3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r\E[132$|,
        use=wy520-48pc,

================================================================

#
# TITLE: TERMCAP ENTRY WY520
# DATE : 8/5/93
#
# wy520 termcap is based on wy285 termcap
#
Wt|wy520|wyse520|wyse 520:\
        :5i:am:hs:km:mi:xn:xo:bs:pt:\
        :co#80:li#24:\
        :AL=3*\E[%dL:DC=3\E[%dP:DL=2*\E[%dM:DO=\E[%dB:\
        :IC=2\E[%d@:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:ae=^O:\
        :al=3\E[L:as=^N:bt=\E[Z:cd=40\E[J:ce=\E[K:ch=\E[%i%d`:\
        :cl=40\E[H\E[J:cm=\E[%i%d;%dH:cs=20\E[%i%d;%dr:\
        :ct=\E[3g:cv=\E[%i%dd:dc=3\E[P:dl=2\E[M:ds=\E[0$~:\
        :ei=\E[4l:fs=\E[0$}:ho=\E[H:i1=\E[?5W:im=\E[4h:ip=4:\
        :is=\E[2;4;20;30l\E[?1;4;10;16l\E[12h\E[?7;8;25;67h:\
        :k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:k6=\E[17~:k7=\E[18~:\
        :k8=\E[19~:k9=\E[20~:k0=\E[21~:F1=\E[23~:F2=\E[24~:\
        :kD=\E[3~:kI=\E[2~:kN=\E[6~:kP=\E[5~:\
        :kb=\b:kd=\E[B:ke=\E>:kh=\E[26~:kl=\E[D:\
        :kr=\E[C:ku=\E[A:l1=PF1:l2=PF2:l3=PF3:l4=PF4:nd=\E[C:\
        :r1=\E[13l\E[3l\E\\\E[63;1"p\E[!p:r2=\E[35h\E[?3l:\
        :r3=\E[?5l\E[47h\E[40l\E[r:rc=\E8:sc=\E7:se=\E[m:\
        :so=\E[7m:sr=2\EM:le=\E[D:do=\E[B:\
        :ts=\E[2$~\E[1$}\E[%i%d`:ue=\E[24m:up=\E[A:us=\E[4m:\
        :ve=\E[34h\E[?25h:vi=\E[?25l:vs=\E[?25h\E[34l:
#
#       Wyse 520 with 24 data lines and status (terminal status)
Wu|wy520-24|wyse520-24|wyse 520 with 24 data lines:\
        :r3=\E[?5l\E[47h\E[40l\E[1;24r:\
        :tc=wy520:
#
#       Wyse 520 with visual bell.
Wv|wy520-vb|wyse520-vb|wyse 520 with visible bell:\
        :vb=100\E[30h\E\,\E[30l:\
        :tc=wy520:
#
#       Wyse 520 in 132-column mode.
Wx|wy520-w|wyse520-w|wyse 520 in 132-column mode:\
        :co#132:\
        :ws#132:\
        :r2=\E[35h\E[?3h:\
        :tc=wy520:
#
#       Wyse 520 in 132-column mode with visual bell.
Wy|wy520-wvb|wyse520-wvb|wyse 520 with visible bell 132-columns:\
        :vb=100\E[30h\E\,\E[30l:\
        :tc=wy520-w:
#
#
#       Wyse 520 emulating a vt420 7 bit mode.
#       The DEL key is programmed to generate BS in is2.
#       With EPC keyboard.
Wz|wy520-epc|wyse520-epc|wyse 520 with EPC kb:\
        :@7=\E[4~:\
        :k0=\E[21~:\
        :k1=\E[11~:\
        :k2=\E[12~:\
        :k3=\E[13~:\
        :k4=\E[14~:\
        :k5=\E[15~:\
        :kh=\E[H:\
        :tc=wy520:
#
#       Wyse 520 with 24 data lines and status (terminal status)
#       with EPC keyboard.
za|wy520-epc-24|wyse520-pc-24|wyse 520 with 24 data lines:\
        :r3=\E[?5l\E[47h\E[40l\E[1;24r:\
        :tc=wy520-epc:
#
#       Wyse 520 with visual bell.
zb|wy520-epc-vb|wyse520-pc-vb|wyse 520 with visible bell:\
        :vb=100\E[30h\E\,\E[30l:\
        :tc=wy520-epc:
#
zc|wy520-epc-w|wyse520-epc-w|wyse 520 in 132-column mode:\
        :co#132:\
        :ws#132:\
        :r2=\E[35h\E[?3h:\
        :tc=wy520-epc:
#
#       Wyse 520 in 132-column mode with visual bell.
zd|wy520-epc-wvb|wyse520-p-wvb|wyse 520 with visible bell 132-columns:\
        :vb=\E[30h\E\,\E[30l:\
        :tc=wy520-epc-w:
#
#       Wyse 520 in 80-column, 36 lines
ze|wy520-36|wyse520-36|wyse 520 with 36 data lines:\
        :li#36:\
        :r3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r:\
        :tc=wy520:
#
#       Wyse 520 in 80-column, 48 lines
zf|wy520-48|wyse520-48|wyse 520 with 48 data lines:\
        :li#48:\
        :r3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r:\
        :tc=wy520:
#
#       Wyse 520 in 132-column, 36 lines
zg|wy520-36w|wyse520-36w|wyse 520 with 36 data lines:\
        :co#132:\
        :ws#132:\
        :r2=\E[?3h:\
        :r3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r\E[132$|:\
        :tc=wy520-36:
#
#       Wyse 520 in 132-column, 48 lines
zh|wy520-48w|wyse520-48w|wyse 520 with 48 data lines:\
        :co#132:\
        :ws#132:\
        :r2=\E[?3h:\
        :r3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r\E[132$|:\
        :tc=wy520-48:\
#
#
#       Wyse 520 in 80-column, 36 lines with EPC keyboard
zi|wy520-36pc|wyse520-36pc|wyse 520 with 36 data lines:\
        :li#36:\
        :r3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r:\
        :tc=wy520-epc:
#
#       Wyse 520 in 80-column, 48 lines with EPC keyboard
zj|wy520-48pc|wyse520-48pc|wyse 520 with 48 data lines:\
        :li#48:\
        :r3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r:\
        :tc=wy520-epc:
#
#       Wyse 520 in 132-column, 36 lines with EPC keyboard
zk|wy520-36wpc|wyse520-36wpc|wyse 520 with 36 data lines:\
        :co#132:\
        :ws#132:\
        :r2=\E[?3h:\
        :r3=\E[?5l\E[36*|\E[36t\E[40l\E[1;36r\E[132$|:\
        :tc=wy520-36pc:
#
#       Wyse 520 in 132-column, 48 lines with EPC keyboard
zl|wy520-48wpc|wyse520-48wpc|wyse 520 with 48 data lines:\
        :co#132:\
        :ws#132:\
        :r2=\E[?3h:\
        :r3=\E[?5l\E[48*|\E[48t\E[40l\E[1;48r\E[132$|:\
        :tc=wy520-48pc:
###

================================================================
 //////////////////////////////////////////////////////////////////////////////


Date: Mon, 3 Jul 2000 11:10:59 +0100
From: mike <mike@islesofscilly-travel.co.uk>
Subject: Wyse Terminal emulations in terminfo database

Hi,

I've recently had occasion to connect a number of Wyse120 and Wyse60
terminals to a SuSe (6.4) distribution and found that the terminfo entries
are somewhat lacking compared with the SCO versions found on our other
server. The most siginificant failing is in the box drawing characters which
seem to be completely wrong!

I have attached the infocmp output from our currently configured wyse60
entry, which also works as is for the wyse120 (the wyse120 being a superset
of the wyse60 AFAICT). By a bit of careful reconfiguration I have made the
dim attribute become the 'normal' one so that 'bold' text stands out.

This set-up might be a useful alternative to the one currently in the
database.

regards,

Mike Winiberg

--------------
Note:
line-break after '>>' in acsc is introduced by mail client and should be
removed

#	Reconstructed via infocmp from file: /usr/share/terminfo/w/wyse60
# suitable for wyse60 and wyse120 terminals in native mode with PC/AT
keyboards
wy60|wyse60|Wyse 60,
	am, bw, hs, mc5i, mir, ul, xon,
	cols#80, lh#1, lines#24, lw#8, nlab#8, pb#9601, wsl#45,

acsc=+/\,u0z5566778899\:\:;;<<==>>FFGGHHIIJJKKLLMMNNOOPPQQRRSSTTUUVVWWXX`ja2
fxgqh2jYk?lZm@nEqDtCu4vAwBx3~y,
	bel=^G, blink=\EG2, bold=\EG0, cbt=\EI, clear=\E+$<50>,
	cr=^M, cub1=^H, cud1=^J, cuf1=^L, cup=\Ea%i%p1%dR%p2%dC,
	cuu1=^K, dch1=\EW$<7>, dim=\EGp, dl1=\ER$<3>,
	dsl=\EA3x\EF\r, ed=\EY$<50>, el=\ET, fsl=^M, home=^^, ht=^I,
	hts=\E1, il1=\EE$<3>, ind=\n$<3>, invis=\EG1, ip=$<2>,
	is1=\EGp,
	is2=\EZ1+\177\EZ1\,\177\EZ1-\177\EZ1.\177\EZ1\\\177\EZ1q\177,
	is3=\Ew0$<16>, kHOM=\E{, kbs=^H, kcbt=\EI, kcub1=^H,
	kcud1=^J, kcuf1=^L, kcuu1=^K, kdch1=\EW, kdl1=\ER, ked=\EY,
	kel=\ET, kent=\E7, kf1=^A@\r, kf10=^AI\r, kf11=^AJ\r,
	kf12=^AK\r, kf13=^AL\r, kf14=^AM\r, kf15=^AN\r, kf16=^AO\r,
	kf2=^AA\r, kf3=^AB\r, kf4=^AC\r, kf5=^AD\r, kf6=^AE\r,
	kf7=^AF\r, kf8=^AG\r, kf9=^AH\r, khome=^^, kich1=\EQ,
	kil1=\EE, knp=\EK, kpp=\EJ, kprt=\EP, krpl=\Er, mc0=\EP,
	mc4=^T, mc5=\Ed#, nel=\177,
	pfloc=\EZ2%p1%'?'%+%c%p2%s\177,
	pfx=\EZ1%p1%'?'%+%c%p2%s\177,
	pln=\Ez%p1%'/'%+%c%p2%s\r, prot=\E), rev=\EG4,
	ri=\Ej$<2>, rmacs=\EcB@\EcD, rmam=\Ed., rmir=\Er,
	rmln=\EA11, rmso=\EGp, rmul=\EGp, rs1=\E~!\E~4$<30>,
	rs2=\EeF\E`\:$<70>, rs3=\EwG\Ee($<100>,
	sgr0=\E(\EH\003\EGp\EcD, smacs=\EcBA\EcD, smam=\Ed/,
	smir=\Eq, smln=\EA10, smso=\EG4, smul=\EG8, tbc=\E0,
	tsl=\EA3x\EF,


 //////////////////////////////////////////////////////////////////////////////

Newsgroups: comp.terminals
Organization: Clark Internet Services, Inc., Ellicott City, MD USA
Message-ID: <0_3H3.33$Qw4.1324@dfw-read.news.verio.net>
Date: Sat, 25 Sep 1999 13:19:56 GMT
From: T.E.Dickey <dickey@shell.clark.net>
Subject: Re: wyse

B'ichela <mdalene@pinkrose.dhis.org> wrote:
> wy50 to dumb. BTW if you don't have a terminfo file for the wyse
> terminal you have. thats the needed step. On the www.wyse.com site
> there is a terminfo file for my wyse50. if you lack a good
> terminfo.ti file   feed that into tic after cutting it out of the
> faq.

some terminfo files for wyse50 have some typographical errors (I think that
the ncurses 4.2 sources are correct though - I updated those from wyse's
and other versions a while ago).

-- even Redhat 6.0 has that ok (but their termcap file is old - lots of
errors).

--
Thomas E. Dickey
dickey@clark.net
http://www.clark.net/pub/dickey

 //////////////////////////////////////////////////////////////////////////////


Date: Sat, 25 Sep 1999 11:19:16 +0200
Organization: http://news.icm.edu.pl/
Newsgroups: comp.terminals
Message-ID: <7si420$5v9$1@sunsite.icm.edu.pl>
From: gunar <gunar@beer.com>
Subject: Re: wyse

B'ichela napisa³(a) w wiadomo¶ci: ...
>On Sun, 19 Sep 1999 16:43:22 +0200, gunar <gunar@beer.com> wrote:
>>i have got a big problem with my wyse terminal
>>i dont know how to configure my RH 6.0 to work whit my term :(
>>is there somebody who know that or maybe any howto or www site ???
>>please help
>>
>>
>>P.S: sory for my english :)
>>
>>
>First of all. which Wyse terminal is it? Look on the back for the
>model number terminal name. on my Wyse 50 it says wy50. then login to
>the Wyse website at http://www.wyse.com there you can find any
>technical info you need.
>for Linux type systems  read the HowTos reguarding
>Serial-Terminal-HOWTO to help you set your inittab and terminfo files.
>heres a short example for my wyse 50 (wy50):
>1.  Plug terminal into a working serial port. say Com1 or ttyS0 for
>this example
>in the /etc/inittab file  you will see several lines one of which is
>like this
>
># Serial lines
>#s1:345:respawn:/sbin/agetty 19200 ttyS0 vt100
>#s2:345:respawn:/sbin/agetty 19200 ttyS1 vt100
>Change the ttyS0 line to the following
>s2:345:respawn:/sbin/agetty -Lh 9600 ttyS0 wy50
>
> Now plug your terminal into your computer with a null-modem
>cable. into  com0 (ttyS0). at the # prompt of linux  (console) type
>init q
>that should reload init level 3 and you should see your login prompt
>on your wyse. be aware of one teeny detail. wyse 50's are natorious of
>using weird control codes and magic cookies that will muff up the
>screen display under some linux programs. If that irks you set the
>wy50 to dumb. BTW if you don't have a terminfo file for the wyse
>terminal you have. thats the needed step. On the www.wyse.com site
>there is a terminfo file for my wyse50. if you lack a good
>terminfo.ti file   feed that into tic after cutting it out of the
>faq.

> B'ichela
> N O T E
> ---------------------
>If mdalene@pinkrose.dhis.org don't work try mdalene@ctol.net


thanx it working !!!!
:)


 //////////////////////////////////////////////////////////////////////////////

Newsgroups: comp.terminals
References: <7s2spl$svs$1@sunsite.icm.edu.pl>
    <slrn7ua90l.7gc.mdalene@pinkrose.dhis.org>
    <0_3H3.33$Qw4.1324@dfw-read.news.verio.net>
    <slrn7uvolm.fga.rottenNOSPAM@oragam.example.com>
Message-ID: <6J4I3.1053$Qw4.30196@dfw-read.news.verio.net>
Date: Tue, 28 Sep 1999 14:59:14 GMT
NNTP-Posting-Host: 168.143.0.8
From: T.E.Dickey <dickey@shell.clark.net>
Subject: Re: wyse

John Burg <rottenNOSPAM@ccil.org> wrote:
> On Sat, 25 Sep 1999 13:19:56 GMT, T.E.Dickey <dickey@shell.clark.net> wrote:
>>
>>-- even Redhat 6.0 has that ok (but their termcap file is old - lots of
errors).

> Oh? Where might I find a better termcap? My wyse 350 give me all sorts of

I'd make one (infocmp -C) from a current terminfo, and test it with tack.
Redhat's termcap dates from before I made a number of corrections for
someone's typographical errors.

> problems... it is pretty much useless with the wyse350 termcap, actually- I
use
> the wyse50 entry. And even that gets screwed up pretty easily, and doesn't
work
> well with many programs. Wyse50-mc is worse.

They both use "magic cookies" (which are not well-supported - some termcaps
simply turn off bold/underlining, etc., to "work").

--
Thomas E. Dickey
dickey@clark.net
http://www.clark.net/pub/dickey

 //////////////////////////////////////////////////////////////////////////////


Newsgroups: comp.terminals
References: <9s0cgp$10dmgq$4@ID-1927.news.dfncis.de>
    <e15f68fcec1e5aa4@mayday.cix.co.uk>
Message-ID: <9sgpeh$319$4@news1.Radix.Net>
Organization: RadixNet Internet Services
Date: 9 Nov 2001 14:32:49 GMT
From: Thomas Dickey <dickey@saltmine.radix.net>
Subject: Re: Wyse WY-60, Linux and the return key

Robert de Bath <rd104097@mayday.cix.co.uk> wrote:
> On Sat, 3 Nov 2001, Gunther Schmidt wrote:

>> I have a Wyse WY-60 attached to a PC running SuSE Linux 6.3, and apart
>> from the fact that I can't connect with speeds over 9600 it's running
>> quite well. But I have some problems with the return key - it's not
>> always recognized as such. For example in mc the return key brings a
>> 'M' onto the screen, so I have to type Ctrl-M instead.
>>
>> How can I solve this problem?


> This is a terminfo/termcap problem.
> The host is putting the keypad into application mode, a very silly idea
> from when terminals didn't have function keys. Application mode is
> just a PITA on a unix system.

> You'll probably want to start by removing the smkx and rmkx strings
>    rmkx=\E[?1l\E>, smkx=\E[?1h\E=,

> and adjusting the arrow key strings to ...
>    kcub1=\E[D, kcud1=\E[B, kcuf1=\E[C, kcuu1=\E[A,


I don't see in his posting any indication that the terminal was set to run
in vt100 mode.  (You seem to be assuming that he's confusing the numeric
keypad's "Enter" key with the return key).  The wy60 terminfo entry doesn't
contain smkx/rmkx.

-- 
Thomas E. Dickey <dickey@radix.net> <dickey@herndon4.his.com>
http://dickey.his.com
ftp://dickey.his.com


 //////////////////////////////////////////////////////////////////////////////

Newsgroups: comp.terminals
References: <9s0cgp$10dmgq$4@ID-1927.news.dfncis.de>
    <e15f68fcec1e5aa4@mayday.cix.co.uk> <9sgpeh$319$4@news1.Radix.Net>
Message-ID: <7ae0debbfea7776e@mayday.cix.co.uk>
Organization: Mayday Technology Ltd
Date: Sat, 10 Nov 2001 19:32:09 +0000
From: Robert de Bath <rd104097@mayday.cix.co.uk>
Subject: Re: Wyse WY-60, Linux and the return key

On 9 Nov 2001, Thomas Dickey wrote:

> I don't see in his posting any indication that the terminal was set to run
> in vt100 mode.

Oh haven't you installed the ESP module yet ?  :-)

Seriously tho, I've used wy60's and wy120's and they are _very_ good
terminals but if they were running in native mode he would have been
having problems with the backspace key and the left and down arrow keys
not return. (BTW: Most Users are used to the PC keyboard under windows,
or the linux console, and think Enter and Return are synonyms)

IME on most unix machines (But never the linux console) the commonest
termcapinfo problems are:


1) Wrong TERM= setting.
   If possible an auto-detect is best but can only be reliable if all
   the terminals are one of a small set of types.

2) VT100 Klone function keys.
   ARRRRRRRRRRRGGGGGG!!! ****! ****! ****! ****! ****! ****! ****!!!!
   I told a lie -- the linux console _is_ a culprit here!

   Nearly every terminal emulator has a vt100 klone emulation most of
   them agree on F1..F4 (Except Linux! and XTerm R5) but _none_ of them
   agree on the rest; and as for Shift Fkeys don't make me laugh!

3) VT100 Application keypad.
   This can be as evil as some termcaps having smkx and rmkx the wrong
   way around but the terminfo on the same machine is different. So one
   application will work until you use 'vi'. But just turning it on
   will effectivly disable the numeric keypad just when your 'User'
   wants to use it.

4) WY60 arrow keys.
   This is rare nowadays as it's much more likely that TERM= will be
   set wrongly.


Enough! I expect you know all this Thomas; for me it's an everyday
occurance, I was at a client's on Tuesday and they haven't even got
the 'stty' setting setup (let alone termcapinfo) on their HP-UX box.


"Is the caplock light turned off?"
"Press the colon key" -- "What's a colon."
"I can't find the 'any' key"
"The backslash is the key with a line from to left to bottom right"
"What's a tilda?" -- "The squiggle key"    (This was _yesterday_!!)

-- 
Rob.                          (Robert de Bath <robert$ @ debath.co.uk>)
                                       <http://www.cix.co.uk/~mayday>

 //////////////////////////////////////////////////////////////////////////////


Newsgroups: comp.terminals
References: <9s0cgp$10dmgq$4@ID-1927.news.dfncis.de>
    <e15f68fcec1e5aa4@mayday.cix.co.uk> <9sgpeh$319$4@news1.Radix.Net>
    <7ae0debbfea7776e@mayday.cix.co.uk>
Message-ID: <9sm50f$3em$2@news1.Radix.Net>
Organization: RadixNet Internet Services
Date: 11 Nov 2001 15:20:47 GMT
From: Thomas Dickey <dickey@saltmine.radix.net>
Subject: Re: Wyse WY-60, Linux and the return key

Robert de Bath <rd104097@mayday.cix.co.uk> wrote:
> 3) VT100 Application keypad.
>    This can be as evil as some termcaps having smkx and rmkx the wrong
>    way around but the terminfo on the same machine is different. So one
>    application will work until you use 'vi'. But just turning it on
>    will effectivly disable the numeric keypad just when your 'User'
>    wants to use it.


I've been spoiled by xterm, which lets me reset the cursor- and keypad-modes
from the popup menu (it's been a long time since I had to tinker with the
setup mode in a serial terminal).  So I guess it is inconvenient when you
run into a program that doesn't treat smkx/rmkx properly (but it's probably
better to just fix the program).

-- 
Thomas E. Dickey <dickey@radix.net> <dickey@herndon4.his.com>
http://dickey.his.com
 ftp://dickey.his.com

 //////////////////////////////////////////////////////////////////////////////

Newsgroups: comp.terminals
References: <b738160dd23d66ba@mayday.cix.co.uk>
    <ac2so0$nfi$2@news1.Radix.Net> <f36cb7367ab9029c@mayday.cix.co.uk>
Message-ID: <acd737$s3c$3@news1.Radix.Net>
Organization: RadixNet Internet Services
Date: 21 May 2002 10:21:27 GMT
From: Thomas Dickey <dickey@saltmine.radix.net>
Subject: Re: WYSE150   v.   ASCII line graphics

Robert de Bath <rd11824@mayday.cix.co.uk> wrote:

> On 17 May 2002, Thomas Dickey wrote:

>> Robert de Bath <rd11824@mayday.cix.co.uk> wrote:
>>
>> > BTW:
>> >   I use ISO-8859-1 on all of wy120, Linux console, xterm and Windows
>> >   terminal emulators (PuTTY, CRT etc). The wyse works fine (including
>> >   boxes) in vt220 mode with a stock vt220 terminfo but the f-keys are
>> >   mis-labeled so I use this instead:
>>
>> > vt220-120|Wyse120 in VT220 emulation mode,
>> >       kf1=\EOP, kf2=\EOQ, kf3=\EOR, kf4=\EOS,
>> >       kf5=\E[M, kf6=\E[17~, kf7=\E[18~, kf8=\E[19~,
               ^^^^ (ok, didn't see that)

>> >       kf9=\E[20~, kf10=\E[21~, kf11=\E[23~, kf12=\E[24~,
>> >       use=vt220,
>>
>> hmm - just looking at it, I don't see which is mislabeled.  (Is your
>> base 'vt220' numbering the keys off-by-one?)

> These are the function keys in my vt220 terminfo.

>    kf1=\EOP, kf2=\EOQ, kf3=\EOR, kf4=\EOS, kf5=\E[17~,
>    kf6=\E[18~, kf7=\E[19~, kf8=\E[20~, kf9=\E[21~, kf10=\E[29~,

> Hmmm, looking at the master it looks like I've got the 'vt220-old' version,
> I still need to do the same with the new one though 'cause of F5.


Actually a vt220 doesn't transmit F1-F5, so the assignment of F5 (to what
appears to be a delete-line control sequence) is arbitrary.

-- 
Thomas E. Dickey <dickey@radix.net> <dickey@herndon4.his.com>
http://dickey.his.com
 ftp://dickey.his.com

 //////////////////////////////////////////////////////////////////////////////


Newsgroups: comp.terminals
References: <b738160dd23d66ba@mayday.cix.co.uk>
    <ac2so0$nfi$2@news1.Radix.Net> <f36cb7367ab9029c@mayday.cix.co.uk>
    <acd737$s3c$3@news1.Radix.Net>
Message-ID: <acdfvl$b56$1@newsmaster.cc.columbia.edu>
Organization: Columbia University
Date: 21 May 2002 12:53:09 GMT
From: Jeffrey Altman <jaltman@watsun.cc.columbia.edu>
Subject: Re: WYSE150   v.   ASCII line graphics

In article <acd737$s3c$3@news1.Radix.Net>,
Thomas Dickey  <dickey@saltmine.radix.net> wrote:
:
: Actually a vt220 doesn't transmit F1-F5, so the assignment of F5 (to what
: appears to be a delete-line control sequence) is arbitrary.


What they appear to be doing here is replacing F1 to F4 with Pf1
through Pf4.  Then, for F5 and above, they are down-shifting the rest of
the function keys.  F6 becomes F5, F7 becomes F6, ...  This is so they
can take advantage of as many of the 20 function keys as possible.

Now if they were using the definition, the key assignments for a VT4xx
and above when used with a PC 101 keyboard you would see:

    kf1=\E[11~
    kf2=\E[12~
    kf3=\E[13~
    kf4=\E[14~
    kf5=\E[15~
    kf6=\E[17~
    kf7=\E[18~
    kf8=\E[19~
    kf9=\E[20~
    kf10=\E[21~
    kf11=\E[23~
    kf12=\E[24~

-- 
 Jeffrey Altman * Sr.Software Designer      Kermit 95 1.1.21  available now!!!
 The Kermit Project @ Columbia University   SSH plus Telnet, FTP and HTTP
 http://www.kermit-project.org/             secured with Kerberos, SRP, and 
 kermit-support@columbia.edu                OpenSSL.


 //////////////////////////////////////////////////////////////////////////////

Newsgroups: comp.terminals
References: <b738160dd23d66ba@mayday.cix.co.uk>
    <ac2so0$nfi$2@news1.Radix.Net> <f36cb7367ab9029c@mayday.cix.co.uk>
    <acd737$s3c$3@news1.Radix.Net> <acdfvl$b56$1@newsmaster.cc.columbia.edu>
Message-ID: <acdpj9$97m$2@news1.Radix.Net>
Organization: RadixNet Internet Services
Date: Tue, 21 May 2002 15:37:13 GMT
From: Thomas Dickey <dickey@saltmine.radix.net>
Subject: Re: WYSE150   v.   ASCII line graphics

Jeffrey Altman <jaltman@watsun.cc.columbia.edu> wrote:
> :
> : Actually a vt220 doesn't transmit F1-F5, so the assignment of F5 (to what
> : appears to be a delete-line control sequence) is arbitrary.
>
> What they appear to be doing here is replacing F1 to F4 with Pf1
> through Pf4.  Then, for F5 and above, they are down-shifting the rest of

I understood that (I do that in xterm since terminfo has kf1 but not a kpf1).


> the function keys.  F6 becomes F5, F7 becomes F6, ...  This is so they
> can take advantage of as many of the 20 function keys as possible.

I've seen in some of the terminfo entries that there's some disagreement
about the numbering (I thought it was more a matter of differing over
whether to assign kf0 the F1 string, or kf1). 

On the other hand, I have seen downshifting applied in this manner,
e.g., ncsa telnet.

-- 
Thomas E. Dickey <dickey@radix.net> <dickey@herndon4.his.com>
http://dickey.his.com
 ftp://dickey.his.com

 //////////////////////////////////////////////////////////////////////////////

http://www.wyse.com/service/support/kbase/wits/80203.txt

TOPIC:  Differences between WY85 and WY185 features and commands.

DATE:   05/03/90

PRODUCT: Wyse WY-85, WY-185

THE ISSUE:
        Differences between WY85 and WY185 features and commands.

OVERVIEW:
        The following lists all of the differences between the WY85
        and the WY185 terminals regarding the WY85 features/commands
        not currently supported by the WY185 terminal or differences
        in how they are implemented. The additional features such as
        multiple pages, DEC VT320 additional commands found on the
        WY185 are not listed.

RESOLUTION:
        MNEMONIC          DESCRIPTION       COMMAND      WY85  WY185
        --------          -----------       -------      ----  -----
        DECLL             LED simulation    CSI n q         Y     N
        CRM               Monitor mode      CSI 3 toggle    Y     N
        TTM               Transmit thru     CSI 16 toggle   Y     N
                          cursor
        DECEDCM (??)      BLOCK mode        CSI ? 10 toggle Y     N
        WYGATM            Send erasable     CSI 37 toggle   Y     N
                          characters only
        WYTEXM            Send screen or    CSI 38 toggle   Y     N
                          scroll region
        MC                Send screen       CSI 2 i         Y     N
        MC                Send line         CSI ? 3 i       Y     N
        DECTTC            Transmit FF after CSI n |         Y     N
                          send screen
        WYSTR             Terminal m,ode    ESC ! p         Y     N
                          reset
        WYEXTM            25th data line    CSI 40 toggle   Y     Y*
                          on/off
        N/A               Alternate         ESC ( l/ESC ) 1 Y     N
                          character set     ESC * l/ESC + 1
        N/A               20ma current loop                 Y     N

        *  The 25th data line command is implemented differently on
           the WY185 in that the current page format (1x or 2x) will
           also be taken into account and screen data is lost when
           command is executed (i.e., from 25th data line OFF to ON,
           and vice versa).

 //////////////////////////////////////////////////////////////////////////////

