	This UIC contains the command files KMSGEN, MCRSLP, and EXECSLP
which should do the job of applying the KMSKIT enhancements to the
user's system.  I must point out, however, that I have never tried
applying KMSGEN from start to finish.  Our mode of operation is that
I have applied each SLP file by hand, assembled it, checked for errors
and inserted it into the appropriate .OLB.  

	In operation, I always apply the SYSGEN command file patches,
and do a SYSGEN after answering the appropriate questions.  If the various
KMS enhancements are desired, the conditionally assembled HELLO, BYE,
SET routines, and INSHD modules will be reassembled each SYSGEN.
Hopefully, MCRSLP.CMD will correctly assemble and insert the other modules.

	However, I am sure bugs will crop up.  As a general rule of thumb.
Each and every SLP file is there for a reason. Use it, assemble the
resultant file, and insert it into its respective object module library.
Remember that the RSXMC.MAC symbols must be correct to support the options
you want.
