	LASer is a program which allows one to take advantage of
	the various printing styles that a DEC LN03 printer has.

	command format is :  LASer filespec,.../switches

		  /CO:nn  Print nn copies
		  /FF     Inserts formfeeds after every 60 lines
		  /HE     Print this help message
                  /HU     Print in "huge" mode 
		  /LA     Print in landscape mode.
		  /LE:nn  Shift the left margin nn spaces to the right
		  /WI     Allow wide output of up to 156 characters
                          (For text with imbedded portrait mode commands)
                  /TW     Print twelve characters/inch mode.
                  /EI     Print eight lines/inch mode.
                  /TI     Print in "tiny" mode (15cpi/8lpi)

	Note that using the /tw/ei/la switches allows one to print listings
	from fortran, macro etc very nicely. the only problem is that the
	compilers must have the number of lines/page changed.

	The MACRO, TKB and F77 command build files to use different lines
	per page are as follows:

	MACRO
	; Specify default output page size
	;
	;	Changed to 72/58. so that landscape mode on lno3 fits
	;	F. Borger, nov 87
	;
	GBLPAT=MACRO:LINPPG:72


	TKB
	;GBLDEF=P$LNTH:74	; SET NUMBER OF LINES PER PAGE FOR TKB
	GBLDEF=P$LNTH:72	; changed so output fits ln03 at 12lpi


	FORTRAN	
	; DEFINE PRINTER WIDTH AND NUMBER OF SOURCE LINES PER LISTING PAGE
	; F77 DEFAULT VALUES ARE:
	;	55  SOURCE LINES PER PAGE (PLUS 3 LINES OF HEADING)
	;	132 COLUMN LINE PRINTER
	; NOTE:
	;	55(10) = 67(8)
	;	80(10) = 120(8)		132(10) = 204(8)
	;
	GBLPAT	=FORTRN:LPLINE:65
