.;
.; This is the BRUTK50 command file which allows users and the system manager
.; to use the BRU utility for backing up and restoring files to/from a TK50
.; magnetic tape drive.  Note that this procedure is based on a paper in the
.; January 1988, page 70, issue of the DEC Professional.
.;
.; Although the original procedure was developed for an RSX system, it is easily
.; modifiable to suit your own purposes (RSX-11M+, other devices, batch backups
.; at night, etc.).  The original routine, BRUWORK.CMD, keyed in from the DEC
.; Professional is included in this directory.
.; 
.; Command files called from BRUTK50 are:
.;
.;	None
.;
.; Programs or utilities this routine is dependent on:
.;
.;	BRU, SRD
.;
.; Data files this routine is dependent on:
.;
.;	[1,54]CLEAR.DAT	(Homes cursor and clears screen.)
.;	[1,54]BELL.DAT  (Rings bell on terminal when operation done.)
.;	[3,54]BACKUP.LOG (Log of incremental backup sets, date, time, etc.)
.;
.; The following files are also included in this directory:
.;
.;	BRUWORK.CMD (The original RSX version keyed in from DEC Professional)
.;	README.1st (This file)
.;	BRUTK50.CMD (Version of BRUWORK.CMD modified for M+)
.;
.; Created by Doug Sasseen on  5-10-88.
.; Revised by Doug Sasseen on  6-24-88 from RSX-11M to RSX-11M-Plus.
.; Edited by Doug Sasseen on 9-29-88.

.; National Food Laboratory (NFL)
.; a.k.a. National Food Processors Association
.; 6363 Clark Avenue
.; Dublin, CA 94568
.; (415)828-1440
.;
