I/O PAGE SYSTEM STACK MULTITERMINAL ROUTINES (ONLY MULTITERMINAL SYSTEMS) MEMORY 28K

476

SYSTEM DEVICE HANDLER

60 56 40 36 0

MAPPED-MONITOR PROGRAMMED REQUESTS

RESIDENT MONITOR

CONTEXT SWITCH ROUTINE

INTERRUPT VECTORS

FORK PROCESSOR

SYSTEM COMMUNICATION AREA

COMMON INTERRUPT ENTRY AND EXIT

TRAP VECTORS

CLOCK INTERRUPT HANDLER I/O QUEUE MANAGER MESSAGE HANDLER TT HANDLER TTY I/O INTERRUPT HANDLERS PROGRAMMED REQUESTS (SCATTERED ABOVE) EMT DISPATCHER ERROR PROCESSOR BACKGROUND IMPURE AREA MONITOR TABLES FIXED OFFSETS