DEVICE HANDLER RESIDENT MONITOR

HEADER SECTION PUTS NEW QUEUE ELEMENT ON THIS HANDLER’S QUEUE AND CALLS THE HANDLER AS A CO-ROUTINE.

RUNS THIS JOB, OR WAITS FOR THIS TRANSFER TO COMPLETE.

RETURNS QUEUE ELEMENT TO THE LIST OF AVAILABLE ELEMENTS, OR PUTS IT ON THE COMPLETION QUEUE.

I/O INITIATION SECTION . . | | DEVICE INTERRUPT

RTS PC

HANDLER TERMINATION SECTION

PREAMBLE SECTION

INTERRUPT SERVICE SECTION . . .

.DRFIN

I/O COMPLETION SECTION . . .