	WHAM IS AN RSX MCR TASK THAT WILL FORCE CHECKPOINTING OF ALL TASKS WITHIN
THE SYSTEM PARTITION THAT IT IS RUN IN.  ALL TASKS IN THE PARTITION AT THE TIME
WHAM IS EXECUTED MUST BE CHECKPOINTABLE OR WHAM WILL BE CHECKPOINTED INSTEAD.
WHAM MUST ALSO BE INSTALLED WITH A HIGHER PRIORITY THAN ALL TASKS IN THE PARTITION.
WHAM IS USED TO FORCE ALIGNMENT OF TASKS WHITHIN A PARTITION TO REDUCE
FRAGMENTATION WHEN EITHER THE SHUFFLER IS NOT INSTALLED OR MANUAL SHUFFLING
IS DESIRED.
 
	TO BUILD WHAM SEE WHAMBLD.CMD
