	FRAG IS A PRIVILEGED RSX-11M MCR TASK THAT WILL LIST FRAGMENTATION
STATISTICS FOR A SPECIFIED FILES-11 DEVICE.  GROUPS OF CONTIGUOUS FREE
BLOCKS (HOLES) ARE LISTED IN SEVERAL RANGES OF FREE SPACE, AS WELL AS THE
ACTUAL NUMBER OF NONCONTIGUOUS FREE BLOCKS WITHIN EACH RANGE AND THE TOTAL
NUMBER OF FREE BLOCKS FOR THE DEVICE. THIS VERSION OF FRAG WILL WORK
WITH LARGE MASS STORAGE DEVICES SUCH AS THE RP.
 
AUTHOR:	RICHARD L. MICHAUD
	(UPDATED SEP 78)
	BRIDGEPORT CONTROLS
	200 PRECISION ROAD
	HORSHAM, PA.  19044
	(215) 674-2700
 
	FRGMAK.CMD MAY BE USED TO ASSEMBLE AND BUILD TASK FRAG.
 
	TO EXECUTE:
 
MCR>FRG DDN:
 
	WHERE:
 
DD	- A LEGAL FILES-11 DEVICE
N	- A LEGAL DEVICE NUMBER <8.
 
NOTE: MCR> RUN FRAG
      MCR> RUN $FRAG
 WILL NOT WORK- FRAG REQUIRES A COMMAND LINE. THEREFORE FRAG MUST BE INSTALLED.
