	This file is to explain how to add lun to hcs and Paul's
plot routines.
The following routines must be editted to reflect changes int he
logical unit numbers of the ploting terminals of to add more
plotting terminals.
	1). PSEUDO
		table with lun must be changed to reflect
		correct terminal types.
 
	2). HCMAG
		table of maginfaction factors must be changed
 
	3). HCS.FTN
		Number of terminals and the terminal number
		table must be modified.
	4). HCSTKB.CMD
		Need be changed only if terminals are added
		then  the number of units and the asg must be corrected
 
	5). HCSGET.FTN
		Need be changed only if units added, then change the
		lun of the read file .
 
	6). GEBUDA.MAC
		Change the assigment table for lun number and
		the number of plotting terminals
 
	7). HCSIZE.MAC
		Change the check at 3$: for dialup lines to correct
		terminal numbers
 
	i think this is all that is necessary.
Then rebuild TVG, HCS.
