	This is the contribution of the Jpl Computer Graphics Lab.
     
               Each directory contains a readme.txt file.
     
            A summary of the contributions is listed below.
     
            (The directorys are before tape copy at decus)


222     1       This file


222     7       A Macro-11 pre-processor used to  assemble  some
                of the other contributions. 

                A  3.2  terminal characteristics display program
                for the full duplex driver. Its non  priveledged
                so  the  task  image should run. If it can get a
                command line, then the terminal  number  can  be
                specified  else ti: is used. Usage: >tty n ;e.g.
                tty 10 for tt10: 


222     53      Combination   of  Conroy's  Grep  and  Directory
                utilities. (i.e. uses Grep's pattern matcher  as
                a directory list argument). 


222     65      Modified version of  the  Original  Conroy  Unix
                editor.  Includes  `Screen'  mode  for vt100 and
                teleray.  Also,  big  editor  fixes   and   many
                additional  enhancements.  This  text  file  was
                formatted  interactively   using   this   editor
                without any external help. 


222     102     A  file  transfer  utility   with   Queue-driven
                monitor.   For  11m  3.2  (needs  typeahead  and
                spawning).  Stripped  down  version   (i.e.   no
                monitor)  allows file transfer if user is logged
                onto 2 systems. 


222     344     lpkill program - allows any user  to  abort  the
                print  spooler.  Definitely  not  for unfriendly
                systems. Also  allows  one  to  delete  separate
                entries  in  the  queue.  (When  the  spooler is
                aborted, the queue  is  hidden  away  and  later
                restored  and  the  next  print job is started).
                This program was partially taken  from  the  spq
                program.  - Note some distributions of spq had a
                lun assignment error i.e. the ti:  lun  and  the
                file lun were both the same. 


222     346     A   modified   version  of  Stamerjohn's  Assign
                Virtual Disk  (AVD).  Allows  one  to  assign  a
                virtual  disk to anywhere on the disk. Useful on
                300 megabyte disks that emulate big rp06's. Also
                can  have  the  system  disk  overlaped  with  a
                virtual disk which is READ-ONLY. (Good for those
                who have been victims of BRU.) 


If you have any questions, you may reach me at:



	Eric Levy
	Jet Propulsion Lab
	4800 Oak Grove Dr.
	Pasadena, Calif. 91103
	Bldg. 264/125
	(213) 354-2969
