





                3M ES&T 1982 Fall DECUS Symposium SIG Tape Submission



               This is the 1982 Fall DECUS Symposium submission to the  RSX
          SIG tape from 3M Engineering Systems and Technology Laboratories.
          Three UFDs will be found in this kit.

               The first UFD contains this README.NOW file.

               The second UFD contains source and command files to build  a
          main  memory  resident pseudodisk driver for 22-bit PDP-11s.  The
          function of this package is to allow the use of a block  of  main
          memory  as  a  high-speed  disk emulator.  This software has been
          tested under RSX-11M-Plus V2.0.  This UFD contains  92/95  blocks
          in 7 files.

               The third UFD contains source and command files to build the
          idle  terminal  monitor  for  RSX-11M or M-Plus.  The function of
          this package is to enforce  security  on  industrial  systems  by
          logging  out  terminals  which have been inactive for a specified
          period of time.  This software has been tested under RSX-11M V3.2
          and  V4.0,  and  under  RSX-11M-Plus  V1.0  and  V2.0.   This UFD
          contains 88/88 blocks in 5 files.

               Caveat:  3M makes no warranty, expressed or implied,  as  to
          the  fitness  of this software for any application, and expressly
          disclaims  responsibility  for  any  damages,  consequential   or
          otherwise, resulting from the use of this software.

