			Notes on current release
			------------------------
	This release of Apple Kermit fixes a number of the problems
which were encountered with the first release.

Changes made in KERMIT.M65:

   4		Reduce max packet length by one so we don't get
		a <Del> character when we quote it.
		Make escape sequence read '^'<esc-char>'C'.
		Make VT52-EMULATION be ON by default.

   5		Make the default time-out interval default to a 
		reasonable amount of time instead of 0. The default 
		is now 15 seconds for both send and receive. 

   6		Make Kermit locate the actual end-of-file instead 
		of sending blindly to the end of the last sector
		of the file. 

   7		Don't send trailing spaces in the file header 
		packets. 

   8		Convert <cr> to <cr><lf> line terminator on the way 
		out and <cr><lf> to <cr> on the way in for text 
		files. 

   9		Account for carry in jump table calculations for 
		those cases where the table starts on a page 
		boundary. 

The bootstrap problems have also been resolved - see the current
documenation files, and the BASIC program.

	CROSS has been fixed so that the '.phase' pseudo-op now works
correctly - it generates code to run at one address and load at another. This
means the BASIC loader program has to be modified so it doesn't change
the load address in the '.hex' file. If you have an older copy
of APPLBT.BAS, simply modify it by removing line  265.
