	This UIC contains a few programs I developed for data acquisition.
	These programs were developed for a PDP-11/t55 system that has 
	TE16 tape transports. The routines will allow you to input or
	output data via a DR11-K digital interface or an AR11 analog
	subsystem.

	Included on this UIC are :

	Fortran Programs :

	ADORDA		Input/output data via an AR11. User selectable
			sample rate (up to at least 4000 Hz continious).
	DR2TAP		Input data from a DR11-K. User selectable sample
			rate (up to at least 8000 Hz continious).
	CLOCKS		Can either turn the Line Frequency Clock off or
			it can turn it on and set it to our systems
			Digital Pathways TCU-150 time keeper.
	TAPDSK		Reads data put onto tape by ADORDA or DR2TAP and
			outputs it to a disk file.

	MACRO Subroutines :

	LABWORK		Miscillaneous AR11, DR11-K, TCU-150, and TE16
			handling routines.
	TAPEIO		Connect to unmounted tapes to allow reading,
			writting, and other various operations.

	Command Files :

	BLDLAB		Compiles the source files on this UIC and builds
			privlidged tasks that map to the I/O page via the
			KCOM partition.
	GO		Runs ADORDA and DR2TAP


	If you have a problem you can let me know. I don't promise to
	fix it, but I may be able to help you out.

	NOTICE A) These routines require that the K-LAB series must be built
		  on your system since the I/O page is mapped to KCOM.

	NOTICE B) USE ALL SOFTWARE CONTAINED HERE AT YOUR OWN RISK !!!
		  The programs run fine on our system but if there are any
		  differences in the address assignments of your system
		  and what the program is set up for then the result could
		  be a SYSTEM CRASH. So please, check the DEFINE module in
		  LABWORK.MAC carefully	before using!

	NOTICE C) Please check the source files for additional comments
		  and documentation.


	Richard A. Crawford
	E-Systems Inc.
	P.O. Box 1056  CBN-27
	Greenville, Texas  75401
	(214)457-6018 or outside Texas (800)527-1000
