                        Changes in KERMIT-65 (V2.1)

	Some new functionality has been added to KERMIT-65, especially
in relation to CONNECT mode support. A cursor is now displayed when
connected to a remote host. Upper case characters appear in inverse
so the user can now distinguish between upper and lower case characters.
Also, characters which can not be directly generated from the Apple ][
keyboard can now be generated by using a right-arrow as a prefix character.
The connect-escape processing now has more options. Break signals
can be sent, etc. Some bugs have been fixed in the GET and SEND
commands. KERMIT-65 no longer runs out of buffers in long sessions. The
GET command uses file names out of the File-header packets sent from
the remote Kermit. There is now an easy way to change the drive
which KERMIT-65 uses for file transfers.

                           CONNECT Enhancements

	The keyboard is always in either default UPPERCASE mode or default
lowercase mode.  When in UPPERCASE, all letters typed are sent out as
uppercase. In lowercase, all letters are sent as lowercase. To reverse the
case for the next character only, hit the right-arrow ("prefix") key. To
switch the default case, hit the prefix-key twice in a row.

	Funny characters: The prefix key is also used to get the unusual
punctuation characters which are not on the Apple keyboard. Here they are:
(To represent the prefix character I am using the letter p).

To get			Type	Appearence

Left Square Bracket	p(	[
Right Square Bracket	p)	]
Left Curly Bracket	p<	{
Right Curly Bracket	p>	}
Underline		p-	_
Backslash		p/	\
Tilde (wiggle)		p^	~
Vertical Line		p.	|

	With left-arrow and right arrow doing special things, its a little
hard to enter their characters (^H and ^U respectivly). There is therefore
an escape from prefix mode sequence. If you type prefix-ESC, the next
character is sent without any interpretation.


                        CONNECT-ESCAPE Enhancements

	The options now available after typing the connect-escape
character are:

	B - Send a BREAK Signal.

	C - Close the connection and return to KERMIT-65.

	S - Show status of the connection.

	0 - Send a null.

	Connect-escape - Send the Connect-escape character itself.

	? - List all the possible single-character arguments.


                         DEFAULT-DISK Enhancement

	There are two new commands which are used to manipulate or check
the setting of the disk which KERMIT-65 will use for its file transfers.
They are described below.

Syntax: SET DEFAULT-DISK parameter value

	This command will tell KERMIT-65 which disk drive should be
used for file transfers. The two parameters which may be set separately
are SLOT and DRIVE. The value for SLOT ranges from 1 to 7. The value
for DRIVE is either 1 or 2.

Syntax: SHOW DEFAULT-DISK

	This command shows what the slot and drive of the default disk
for file transfers.


                                 The EDITS


  31		By: Peter Trei			On: 10-Feb-1984
		Added support for visible cursor. See CURON and
		CUROFF routines.
				oc.trei%cu20b@columbia-20



  32		By: Peter Trei			On: 12-Feb-1984
		Fixed bug in SSC support software; altered RRF
		flag mask from $#04 to $#08.
				oc.trei%cu20b@columbia-20



  33		By: Peter Trei			On:  21-FEB-1984
		Corrected definitions of BASL and BASH.
				oc.trei%cu20b@columbia-20



  34		By: Peter Trei			On:  23-FEB-1984
		Adjustments to make uppercase and weird chars appear
		inverse.



  35		By Peter Trei			On:  17-MAR-84
		Installed CHRCON routine to allow the 2/2+
		keyboard to enter lowercase, rubout, and other
		'missing' characters. This also involved adding the
		'SET KEYBOARD' switch, with positions for 2P and 2E.



  36		By: Antonino N.J. Mione		On: 22-JUN-1984
		Make the FILE-BYTE-SIZE default sensible (i.e.
		Seven-bit since we are defaulting the FILE-TYPE-MODE
		to TEXT).



  37		By: Antonino N.J. Mione		On: 25-JUN-1984
		Fix 'Get' so that the first time it is used,
		it will work. 



  38		By: Antonino N.J. Mione		On: 25-JUN-1984
		Handle error packet processing correctly. 



  39		By:  Tim Heuser			On: 26-JUN-1984
		Start assembly at $801 so we don't break Applesoft. 



  40		By: Antonino N.J. Mione		On: 29-JUN-1984
		Add capability to set drive for file transfers.
		Added the 'SET DEFAULT-DISK' and 'SHOW DEFAULT-DISK'
		commands. 



  41		By: Antonino N.J. Mione		On: 29-JUN-1984
		Add capabilities to code which processes Escaping
		from CONNECT mode. Give user ability to send a
		BREAK signal, a nul character, or the Escape
		character itself. Also, add these to the online
		help message. 



  42		By: Antonino N.J. Mione		On: 02-JUL-1984
		Fix the 'GET' command. When receiving files, have
		KERMIT-65 use the filenames from the File-header
		packets. 



  43		By: Antonino N.J. Mione		On: 11-JUL-1984
		Clear the FCB when fetching a filename from the
		packet buffer. Previously when receiving files,
		if subsequent filenames where shorter than filenames
		in the beginning of the session, the name of the
		file created on disk would be incorrect. 



  44		By: Antonino N.J. Mione		On: 12-JUL-1984
		Fix 'No buffers available' problem when doing
		>3 SENDs in one session. Make the SDAT routine
		reset the eofinp flag and close the file when
		the BUFILL routine returns an end-of-file. 



  45		By: Antonino N.J. Mione		On: 12-JUL-1984
		Make version read '2.1'. 

