[200,*] Files

The [200,*] directories are allocated for P/OS RX50
images. Task images have been "hexified" to ensure they
are movable by any Kermit. The hexify and dehexify programs
must be downloaded to a Pro, and can then be used to
convert to task image form again. Note that where the
tasks start in DDT, use the control-[ key on a Pro to
generate an Escape. esc G will start the programs.
	All these areas assume that the .HEX files are
reconverted into .TSK or .OLB files or whatever using
the DEHEX program before attempts to put them onto RX50. It
is a good idea to make sure .TSK files are contiguous on
RX50.

[374,*] has PRO 350 DECUS C. README files there note where
	the original diskettes are. All files are present.
[356,40] on the 1st backup set has all Kermits including PRO
350 Kermit. The VAX hexifier and the PRO hexifier are compatible.

[200,2]	-	SRD, TECO, MCR from R. Kirkman. MCR emulator is for
		P/OS V1 but instructions for updating it are
		included. TECO V36 and SRD should work OK on
		all versions, though SRD wildcards DON'T include
		directories and his SRD is NOT the same as the working
		group's flavor.
[200,3] -	DEHEX, PRO Kermit. Kermit for DEC PRO in hex format,
		plus utils to change .hex files back into .tsk files.
		(Isolated from Kermit area for convenience.)
[200,4]	-	FIXIT - utility in DECUS library that converts (mostly)
		files in micro dialects of BASIC (e.g. microsoft) into
		DEC Basic.
[200,5]	-	BASIC, PASCAL, PortaCalc. Michael Reese BASIC, Swedish
		PASCAL (and the runtime library), and PortaCalc (AnalytiCalc)
		all built for the Pro. Get your free utilities here, folks!
		NOTE: This area needs more than 1 RX50 for everything
		to fit; 2 will do nicely.
[200,6] -	DDT debugger for the PRO. Since it is useless without
		the tool kit, complete sources are provided. Use the
		DDTBLD.CMD file to generate DDT. It will also give you
		an I/O PAGE COMMON which allows nonprivileged tasks to
		map to the I/O page and get anywhere in the machine. This
		DDT version will provide the common when "2 task" DDT is
		built and memory mapping is not disabled.
