%
$[1m VT220/PRO350 series function keys$[0m

$[7m\
$[1mF10$[m$[7m	Exit (same as GOLD F).  Only from window zero $[m
$[7m\
$[1mF12$[m$[7m	Toggle from the start to end of  current line $[m
$[7m\
$[1mF13$[m$[7m	Toggle the keypad for commands or data entry  $[m
$[7m\
$[1mF14$[m$[7m	CPU, IO and page fault statistics  (VMS only) $[m
$[7m\
$[1mF17$[m$[7m	Switch to file editing window zero            $[m
$[7m\
$[1mF18$[m$[7m	Switch to file editing window one             $[m
$[7m\
$[1mF19$[m$[7m	Switch to file editing window two             $[m
$[7m\
$[1mF20$[m$[7m	Spawn a host command (VMS only)               $[m
$[7m$[1m\
FIND$[m$[7m	FindNext (PF3)                                $[m
$[7m$[1m\
INSERT$[m$[7m	Insert contents of the current paste buffer   $[m
$[7m$[1m\
REMOVE$[m$[7m	Delete current line(s) or active select range $[m
$[7m$[1m\
SELECT$[m$[7m	Start/End a select range (see help for GOLD 3)$[m
$[7m$[1m\
PREV$[m$[7m	Display previous page of text                 $[m
$[7m$[1m\
NEXT$[m$[7m	Display the next page of text                 $[m
$[7m$[1m\
DO $[m$[7m	Execute line editor command (VMS only)        $[m
$[7m$[1m\
HELP$[m$[7m	Enter help menu                               $[m
$[m\
