[273,10]	CPM

This is CPM.C, a DECUS C (and many 8080 Cs) compatible kludge
that reads/writes/modifies CP/M diskettes.
I use it on RX01s to diddle standard CP/M 8" floppys.
I know DECUS is wretching with CP/M diskette readers, but I include this
because: (1) you can #include cpmoscpm.h to do a BDS C version
of this program for your 8080, and (2) I haven't seen one done in
C.
If DECUS C's wild cards worked, this would be much better.
Because I pranged DECUS C's quick-sort routine, a crude bubble sort
is used instead.

A program to drive RX01/02/03 diskette drives to use
CP/M(sic(k)) standard diskettes. Diskettes are electromagnetically
equivalent to IBM 3740 standards. Program does detailed or brief
directories. Binary or text input or output are supported. Help
is in the program. Wildcards are supported. Beware DECUS C wildcards
for RSX: needs a total rewrite! Initialising diskettes or deleting
(wild) files is easy. The program is in production and has been sold.
No known bugs or deficiencies. Design suggestions welcomed. Contact:

	Dean Elsner			Dean Elsner
	M L Silbert P/L			Rent-A-Mind
	26 Queen Street			Box T 1680
	Perth 6000			GPO Perth 6001
	Western Australia		Western Australia

	phone: +61 (9) 322 6048		phone: +61 (9) 271 9014
