
	This directory has the submission from for the
Fall 86 RSX SIG tape.

File		Description
----		-----------

TTDAT.SLP	Patch to M+ v3.0 to provide I/D space on Qbus DH-11
		clones.
TTYH.SLP	Same as above
PROTREE.86A	RSX SIG Other media working group tape tree
PRO.86A		RSX SIG Other media working group users list


	The patches to the YH driver were used at our site to allow
an EMMULEX CS01 to be used on an 11/73 sysgened with I/D space support.
The existing gen procedure provided by Emmulex required the sysgen be done
with no I/D space support.

	To use the patches apply them to the sysgen kit before starting
sysgen, then proceed with the Emmulex instructions except choose I/D space
support in Executive configuration. This patch also allows terminals to be
set to 19200 baud.

	The other media working group has started the spring 86 tapes down the
tree. Our working group is made of volunteers that will convert the SIG tapes
to other media including but not limited to RX50, RL02, TK50, 800BPI TAPE,
and 6250BPI TAPE. For more information contact me on how to volunteer or how
to obtain something off the tapes.

Bob Uleski
Baker Instruments Corp.
100 Cascade Drive
Allentown, PA  18103
(215) 264-2800	(work)
(215) 395-9018	(home)

