.AP
.STANDARD
.ps 54,70
.FIGURE 5
.C;Modifications to RNO from CARTS
.skip 2
The following modifications may be made to the standard RUNOFF.
.ls
.le;Change bar support.
 This allows modified areas of text to be marked by a bar (| ASCII code 174 octal) on the left hand side of the page.
.le;.BLANK and .SKIP may use negative arguments.
 This allows text to be moves some number of lines from the end of the page.
.le;A shift right switch /RI.
 This switch allows text to be shifted right some number of columns.
.els
There is also build command files for RSX that allow mapping to shared FCS.
 The files for these modification are:
.ls
.le;RNO.SLP -- applies the corrections to the RNO modules
.le;Source correction files
.ls
.le;CMTAB.COR -- CMTAB corrections
.le;ERMAG.COR
.LE;FMTCOR.COR
.LE;PINDX.COR
.LE;RNCMD.COR
.LE;RNORSX.COR
.LE;RUNOFF.COR
.els
.LE;RNODOC.COR -- RUNOFF.RNO corrections
.LE;RNOBLDFCS.CMD -- MAPS TO A SHARED FCSRES LIBRARY
.LE;RNOBLDFCS.ODL -- OVERLAYS FOR A SHARED FCSRES LIBRARY (you may need to change this)
.le;README.1ST -- This document
.le;README.2ND -- The standard README.1ST document normally distrubuted.
.ELS
To install runoff:
.ls
.le;read this document and the README.2ND document.
.le;If you want the modifications listed above:
.ls
.le;transfer the files to the UICs specified in README.2ND.
.le;set the UIC to the source UIC
.le;Run SLP with @RNO.SLP as input
.els
.le;Now follow the assembly and task build instructions in README.2ND.
.le;If you want to use the shared FCSRES library, use "TKB#@[1,24]RNOBLDFCS" instead of "TKB#@[1,24]RNOBLD".
.le;Once you have made RNO use RUNOFF.RNO as input to check out the task and to generate a manual.
.els
 At Fermilab, we have used these modifications without problems for some time.
If you have problems, call Daniel#B.#Curtis at (312)#840-3927.
