Barton,

  Here are the files you asked for. Please note that they were rather
quickly put together. I apologize for the delay in getting this to you,
but we were having trouble with our TE-16 tape drive (AGAIN)!

 The code was properly conditionalized for Named directory support as of the 
working group's WG-6.6 version. However, no question in the build file enabled 
the conditional for RSX-11M-PLUS. The conditional symbol is N$$DIR.

 The code for Decimal Version Number support was also included in the V6.6 
release, but it was conditionalized on the P$$OS rather than the F$$DVN. This
has been corrected in V6.61.

Bugs and cavets:

	Sometimes on the heading line Named Directories are truncated
to 6 characters (I haven't been able to track this one down ... I think some
foolish person hardcoded the number of characters to 6 ... the limit on P/OS)!

The following modules have modifications/hacks in them:

Decimal Version Number Support:

Module	SRDINI.MAC
Module	SRDLST.MAC

Named Directory Support:

Module	SRDNUD.MAC
Module	SRDOPR.MAC
Module	SRDSYS.MAC

Other Modified Modules:

Module SRDATA.MAC

That is All.

-Arnold

P.S.

 If you have time to do modifications to this GREAT program, may
I suggest that the Feature Mask be tested to determine Decimal Version
Number and Named Directory Support. Further, if you can fix the Named Directory 
Truncation Problem, I'm sure that the SRD working group would be most
greatful!

