This directory contains a variety of tape routines. It varies from displaying
the ANSI label blocks on a tape, setting up a tape for use, winding to EOV, to
testing for bad blocks.
Try them, maybe they are as useful for you as they were for us. Most of them 
were developed long ago.

ABORT.MAC		See [264,1]

AETST.FTN		ASCII-to-EBCDIC conversion test
AETSTBLD.CMD
ASCEBC.MAC		

ANSDMP.FTN		Formatted dump of ANSI labels
ANSDMP.TSK
ANSDMPBLD.CMD
ANSDMPCBC.CMD

ATDET.MAC		See [264,1]

BADMM.FTN		Check tape for bad blocks
BADMMBLD.CMD
BADMMCBC.CMD

DKGET.CMN		Get logical block from disk
DKGET.FTN

ERRMM.FTN		Ask for action on tape-error found

IBMSWP.FTN		Swap the bytes

INITMM.FTN		Initialize tape unit for read or write

MTGET.CMN		Get logical block from tape
MTGET.FTN

MTPOS.FTN		Position tape to a file

MTPUT.CMN		Write logical block to disk
MTPUT.FTN

MTTMK.FTN		Write tape-mark

README.1ST		This file

RHDR1.FTN		Formatted dump of ANSI HDR1 block
LHDR1.CMN
RHDR2.FTN		Formatted dump of ANSI HDR2 block
LHDR2.CMN
RHDR3.FTN		Formatted dump of ANSI HDR3 block
LHDR3.CMN
RVOL1.FTN		Formatted dump of ANSI VOL1 block		
LVOL1.CMN

SPLTAP.FTN		Find EOV on tape and rewind to BOT.
SPLTAP.TSK
SPLTAPBLD.CMD

TAPEOF.FTN		Write EOF  after specified block.
TAPEOFBLD.CMD


Jan H. Belgraver
Organon International B.V.
CNS Pharmacology Dept.
Room RE1148
P.O. Box 20
5340 BH  Oss
The Netherlands

Tel.:	+31 (4120) 62943
Fax.:	+31 (4120) 62617
