110424     CIT101: Routines to Drive the CIT101 and VT100 Terminals
Version: V2.2, March 1984
 
Submitted by: Ralston W. Barnard, Sandia National Labs, Albuquerque,
NM
 
Operating System: RT-11 V5.0  Source Language: FORTRAN IV, MACRO-11
Memory Required: 1328 (10) wds - max.  Hardware Required: VT100
terminal, CIT-101 terminal  Keywords: Terminal Handler, VT100 Routines
 
Abstract: CIT101 is a MACRO subroutine which is an extension of
the DECUS No. 11-424, "VT". It is a collection of
FORTRAN-callable routines for control of the VT100
terminal functions. Additions to this package include
support for the enhanced screen-control features of the
CIT101 terminal (including both the 10A and 11C ROM
sets), and for the CIT101 and VT100/102 printer ports.
Both of these extra features are individually available
as conditional assemblies in the source code. The
original submission has been recoded to reduce its size.
The code has also been divided into "I and D"
PSECTs.
 
The original demos provided with 11-424 are included.
Also included are three routines which use the CIT101
library for centering text, displaying text in two
columns, and for putting out a string of numbers after a
prompt. The file CICALL.TXT is a handy summary of all
the calls.
 
Media (Service Charge Code): Write-Up (AA), One RX01 Diskette (KA)
Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
