110772     RAID: A Really Awesome Interactive Debugger  Version: V1.0,
December 1984
 
Submitted by: John Wilson, Concord Academy, Concord, MA
 
Operating System: RSTS/E V7.0-07, RT-11 V04.0  Source Language:
MACRO-11  Memory Required: 2215 Words for RSTS/E, 2116 Words for RT-11
Keywords: Debugging, Tools - Software Development
 
Abstract: RAID is a symbolic debugger for the PDP-11 series.  It
includes most of the major facilities for ODT, with some
important additions.  RAID provides commands to:
 
. Set breakpoints (up to 16)
. Deposit values in memory
. Dump (ranges of) memory (with ASCII, if byte)
. Start or continue execution at any point
. Disassemble (range of) memory
. Display and change registers and flags
. Perform single steps
 
RAID, like ODT, is linked to the program to be debugged.
RAID can disassemble all PDP-11 instructions (including FIS
and FP11) except for CIS.  Two versions of RAID are provided:
one for RT-11, and one for RSTS/E.  The RSTS/E version is the
same as the RT-11 version (except it uses RSTS I/O calls),
but adds ^C trapping, and a command to print RSTS system
error messages.  The RT-11 version doesn't use any EIS
instructions, and will run on any PDP-11 series computer
(including LSI-11s).
 
Media (Service Charge Code): User's Manual (EC), One RX01 Diskette
(KA)  Format: RT-11, 600' Magnetic Tape (MA)  Format: DOS-11
 
 
