110612     CDPACK: Interface Routines for DR-11W  Version: December
1984
 
Author: Vicky White, Fermilab, Batavia, IL
 
Submitted by: Peter Heinicke, Fermilab, Batavia, IL
 
Operating System: RT-11 V4 or later  Source Language: MACRO-11  Memory
Required: 1000KW  Software Required: DR-11W Driver for RT-11 (DECUS
No. 11-611)  Keywords: Data Communications, Interface Routines
 
Abstract: This is a collection of routines which interface to the
DR-11W driver (DECUS No. 11-611).  These routines implement
no-wait, wait, and completion routine I/O.  Multiple messages
may be awaited, and error status of each message is saved
until the status routine is called.  The interface is
standardized so that the same FORTRAN routines may be used on
RT-11 or RSX-11.  See also "CD" (DECUS No. 11-611) - an
"RT-11 device driver for the DR-11W" which is required
software.
 
Media (Service Charge Code): Write-Up (AA), Two RX01 Diskettes (KB)
Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
