110687     FORTRAN Callable Subroutines Package for Fast Continuous
A/D on the MINC  Version: V1.0, November 1983
 
Submitted by: Digital Equipment Corporation
 
Operating System: RT-11 V5.0  Source Language: FORTRAN IV, MACRO-11
Memory Required: 280 (decimal) Words  Software Required: MACRO-11
Assembler, RT-11 O/S, FORTRAN IV compiler  Hardware Required:
MNCAD-MINC A/D Module, MNCKW-MINC Clock Module  Keywords: Conversions
- Analog/Digital
 
Abstract: Assembly routines, ADCONT, WAITFD, and STOPIT,
constitute a FORTRAN callable package capable of
providing dedicated, continuous (buffer management with
transfer to peripheral storage) analog-to-digital
acquisition at rates two to eight times faster than the
maximum rates provided by REAL-11 routines in a fraction
of the memory space. The interface is also less complex
and was modeled after MINC BASIC. Experienced users
should be able to modify the sources for use with K and
V series logic running under RT-11. A programmable clock
and A/D modules are required.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
