110823     Task to Task Communications  Version: V1.01, November 1985
 
Submitted by: Eddy Fey, Utah Power & Light, Salt Lake City, UT
 
Operating System: RSX-11M-PLUS V2.1  Source Language: FORTRAN 77,
MACRO-11  Keywords: Utilities - RSX-11
 
Abstract: This package contains a task-to-task communications and
flying
install subsystem.  Some of the individual programs in the
package are:
 
RUNNER & INSREM	  Set of programs used to send
  		  parameters to a task, install the task, activate it and
  		  remove it upon exit.  This is a complete 'flying install'
  		  subsystem and will work for permanently installed tasks as
  		  well (see RUNNER.DOC).
VXDRV & VXUTIL 	  This is yet another re-write of the
  		  VSDRV by Osudar.  It provides multiple units each capable of
  		  having 16kb of pool space.  This will only work on RSX11M+
  		  with I/D.
CMB 		  Compare binary.  Compares two fixed length binary
  		  files for equality.  Can be used for task images, data
  		  files, etc.
WATCHER 	  Nifty patch for finding executive space memory
  		  clobbers.
IODUMP 		  Dumps buffers in hex-ascii byte or word format.
CDUMP 		  Searches a binary CDA file for a given pattern.
 
Media (Service Charge Code): 600' Magnetic Tape (MA)  Format: FILES-11
 
 
