110664     ADCON: A/D Conversions Package for Use with ADV11-C and
KWV11-C  Version: V1.2, August 1984
 
Submitted by: G. C. Scott
 
Operating System: RT-11SJ V4.0  Source Language: FORTRAN IV, MACRO-11
Memory Required: 6.656KW  Hardware Required: ADV11-C analog-to digital
conversion pc board, KWV11-C programmable realtime clock pc board.
Keywords: Conversions - Analog/Digital
 
Abstract: ADCON is a software package which can be used with
Digital Equipment Corporation's ADV11-C analog-to
digital conversion and KWV11-C programmable realtime
clock boards. The characteristics of this software
package include:
 
. Digitizations from 8 differential analog input
  channels
. Up to 1 KHz sampling rate,
. Software programmable gain
. 12 bit data resolution, and
. DC offset corrections and calibrations of the data
 
The package includes the following:
 
. DY1:DOCA.TXT, user instructions and programming
  example
. DY1:ADCONF.FOR, a FORTRAN IV program which sets up
  for the A/D conversions and performs corrections and
  calibrations of the digitized data
. DY1:ADCONM.MAC, a MACRO-11 program which controls
  the A/D conversions
. Listing files for the above FORTRAN IV and MACRO-11
  programs
 
Error checking is performed throughout DY:ADCONF.FOR and
DY:ADCONM.MAC. Suggestions for software and hardware
setup are included for users who require more customized
A/D conversion schemes.
 
Media (Service Charge Code): One RX01 Diskette (KA)  Format: RT-11,
600' Magnetic Tape (MA)  Format: RT-11
 
 
