110335     RASM: Reverse Assembler for RT-11  Version: 2.01, March
1979
 
Submitted by: S. C. Chou, University of Malaya, Malaysia
 
Operating System: RT-11 V3  Source Language: MACRO-11  Keywords:
Conversions, Utilities - RT-11
 
Abstract: This program takes any RT-11 disk file and converts it
instruction by instruction into instruction mnemonic
form together with octal word and optional octal byte,
ASCII and RAD50 equivalents. The user may specify
several switch options in the standard RT-11 command
string format to obtain reverse assembly listing of any
block or consecutive blocks of a particular file. RASM
can also be used as an extended file dump utility, and
runs on all RT-11 configurations, including the
smallest.
 
Restrictions: RASM V2.01 does not run under RT-11 V1 and V2 monitors.
 
Media (Service Charge Code): Write-Up (AA), One RX01 Diskette (KA)
Format: RT-11, 600' Magnetic Tape (MA)  Format: RT-11
 
 
